{"text_format":"1","workbook":"xlsx","n_sheets":7,"sheets":["PLSCargas","PLSLinea","INLI_ObraCivil","Peanas","Atributos CAD","Limites","Perfiles"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":5,"defined_names":318,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"PLSCargas","index":0,"n_rows":1873,"n_cols":11,"rows_kept":1873,"cut":false,"hidden":true,"merged":[]}
["str_no","structure_name","load_case","foundation_description","axial_force","units3","shear_force","units4","bending_moment","units5","foundation_usage"]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Viento,C NA+","91S",-933.97,"kN",155.99,"kN",4.01,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Viento,C NA+","91X",-1591.34,"kN",281.48,"kN",2.39,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Viento,C NA+","91XY",1172.21,"kN",191.56,"kN",3.83,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Viento,C NA+","91Y",1829.52,"kN",317.23,"kN",1.91,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Viento,C NA-","91S",-1601.6,"kN",280.18,"kN",2.04,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Viento,C NA-","91X",-924.38,"kN",152.4,"kN",3.75,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Viento,C NA-","91XY",1839.8,"kN",321.3,"kN",2.15,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Viento,C NA-","91Y",1162.6099999999999,"kN",192.41,"kN",3.98,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Hielo,C NA+","91S",-1290.8,"kN",221.61,"kN",2.3199999999999998,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Hielo,C NA+","91X",-1280.27,"kN",220.11,"kN",2.29,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Hielo,C NA+","91XY",1547.77,"kN",262.86,"kN",2.27,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Hielo,C NA+","91Y",1537.19,"kN",261.38,"kN",2.2599999999999998,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Viento+Hielo,C NA-","91S",-1408.03,"kN",242.4,"kN",2.1,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Viento+Hielo,C NA-","91X",-1231.1300000000001,"kN",210.32,"kN",2.56,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Viento+Hielo,C NA-","91XY",1664.98,"kN",284.18,"kN",2.11,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Viento+Hielo,C NA-","91Y",1488.08,"kN",251.97,"kN",2.58,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Viento+Hielo,C NA+","91S",-1241.81,"kN",212.3,"kN",2.64,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Viento+Hielo,C NA+","91X",-1397.14,"kN",241.36,"kN",2.17,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Viento+Hielo,C NA+","91XY",1498.78,"kN",253.04,"kN",2.57,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Viento+Hielo,C NA+","91Y",1654.07,"kN",282.19,"kN",2.04,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Tiro Vertical,C NA+","91S",-881.8,"kN",151.9,"kN",1.73,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Tiro Vertical,C NA+","91X",-874.87,"kN",150.84,"kN",1.61,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Tiro Vertical,C NA+","91XY",1120.03,"kN",190.17,"kN",1.58,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Tiro Vertical,C NA+","91Y",1112.92,"kN",189.2,"kN",1.68,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Desequilibrio Amar Atras,C NA+","91S",-1270.06,"kN",217.15,"kN",2.68,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Desequilibrio Amar Atras,C NA+","91X",-1426.51,"kN",246.33,"kN",2.2200000000000002,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Desequilibrio Amar Atras,C NA+","91XY",1525.6,"kN",257.68,"kN",2.61,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Desequilibrio Amar Atras,C NA+","91Y",1682.02,"kN",286.94,"kN",2.09,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Desequilibrio Amar Atras,C NA-","91S",-1436.58,"kN",247.31,"kN",2.15,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Desequilibrio Amar Atras,C NA-","91X",-1260.22,"kN",215.25,"kN",2.61,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Desequilibrio Amar Atras,C NA-","91XY",1692.11,"kN",288.86,"kN",2.16,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Desequilibrio Amar Atras,C NA-","91Y",1515.74,"kN",256.67,"kN",2.63,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Desequilibrio Amar Del,C NA+","91S",-849.75,"kN",145.41,"kN",2.02,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Desequilibrio Amar Del,C NA+","91X",-1006.92,"kN",174.76,"kN",1.57,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Desequilibrio Amar Del,C NA+","91XY",1108.79,"kN",186.45,"kN",1.96,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Desequilibrio Amar Del,C NA+","91Y",1265.92,"kN",215.92,"kN",1.42,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Desequilibrio Amar Del,C NA-","91S",-1016.05,"kN",175.5,"kN",1.5,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Desequilibrio Amar Del,C NA-","91X",-840.83,"kN",143.72999999999999,"kN",1.93,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Desequilibrio Amar Del,C NA-","91XY",1275.07,"kN",217.61,"kN",1.49,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Desequilibrio Amar Del,C NA-","91Y",1099.8499999999999,"kN",185.68,"kN",1.97,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CT1 Atras,C NA+","91S",-1246.27,"kN",212.91,"kN",2.54,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CT1 Atras,C NA+","91X",-1403.08,"kN",242.21,"kN",2.2200000000000002,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CT1 Atras,C NA+","91XY",1502.62,"kN",253.64,"kN",2.62,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CT1 Atras,C NA+","91Y",1659.45,"kN",282.89999999999998,"kN",1.95,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CT1 Atras,C NA-","91S",-1411.04,"kN",242.82,"kN",2.0099999999999998,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CT1 Atras,C NA-","91X",-1238.05,"kN",211.32,"kN",2.62,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CT1 Atras,C NA-","91XY",1667.38,"kN",284.56,"kN",2.16,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CT1 Atras,C NA-","91Y",1494.43,"kN",252.8,"kN",2.5,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CT1 Del,C NA+","91S",-1171.94,"kN",203.4,"kN",4.05,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CT1 Del,C NA+","91X",-1324.18,"kN",230.63,"kN",1.71,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CT1 Del,C NA+","91XY",1428.36,"kN",242.65,"kN",1.72,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CT1 Del,C NA+","91Y",1579.87,"kN",272.17,"kN",3.44,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CT1 Del,C NA-","91S",-1332.96,"kN",232.45,"kN",3.48,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CT1 Del,C NA-","91X",-1163.4000000000001,"kN",200.17,"kN",1.79,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CT1 Del,C NA-","91XY",1589.36,"kN",273.19,"kN",1.54,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CT1 Del,C NA-","91Y",1419.11,"kN",242.93,"kN",4.01,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CT2 Atras,C NA+","91S",-1248.73,"kN",213.3,"kN",2.7,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CT2 Atras,C NA+","91X",-1400.15,"kN",241.78,"kN",2.08,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CT2 Atras,C NA+","91XY",1505.13,"kN",253.88,"kN",2.48,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CT2 Atras,C NA+","91Y",1656.47,"kN",282.57,"kN",2.08,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CT2 Atras,C NA-","91S",-1413.97,"kN",243.25,"kN",2.15,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CT2 Atras,C NA-","91X",-1235.5899999999999,"kN",210.93,"kN",2.4500000000000002,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CT2 Atras,C NA-","91XY",1670.36,"kN",284.89,"kN",2.02,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CT2 Atras,C NA-","91Y",1491.93,"kN",252.57,"kN",2.64,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CT2 Del,C NA+","91S",-1173.8900000000001,"kN",202.13,"kN",1.86,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CT2 Del,C NA+","91X",-1322.57,"kN",231.46,"kN",3.53,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CT2 Del,C NA+","91XY",1429.65,"kN",244,"kN",3.98,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CT2 Del,C NA+","91Y",1578.98,"kN",271.26,"kN",1.49,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CT2 Del,C NA-","91S",-1334.97,"kN",231.65,"kN",1.61,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CT2 Del,C NA-","91X",-1161.72,"kN",201.51,"kN",3.96,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CT2 Del,C NA-","91XY",1590.71,"kN",274.13,"kN",3.51,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CT2 Del,C NA-","91Y",1418.14,"kN",241.66,"kN",1.76,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CS 1  Amar Atras,C NA+","91S",-1248.03,"kN",213.17,"kN",2.4700000000000002,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CS 1  Amar Atras,C NA+","91X",-1405.98,"kN",242.73,"kN",2.29,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CS 1  Amar Atras,C NA+","91XY",1504.48,"kN",254.01,"kN",2.7,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CS 1  Amar Atras,C NA+","91Y",1662.48,"kN",283.39,"kN",1.88,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CS 1 Amar Atras,C NA-","91S",-1414.36,"kN",243.33,"kN",1.95,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CS 1 Amar Atras,C NA-","91X",-1239.8800000000001,"kN",211.71,"kN",2.7,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CS 1 Amar Atras,C NA-","91XY",1670.8,"kN",285.14,"kN",2.2400000000000002,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CS 1 Amar Atras,C NA-","91Y",1496.4,"kN",253.13,"kN",2.42,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CS 1  Amar Del,C NA+","91S",-1140.1400000000001,"kN",198.73,"kN",4.96,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CS 1  Amar Del,C NA+","91X",-1296.0999999999999,"kN",225.54,"kN",1.41,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CS 1  Amar Del,C NA+","91XY",1398.12,"kN",236.99,"kN",0.77,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CS 1  Amar Del,C NA+","91Y",1552.88,"kN",267.98,"kN",4.3099999999999996,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CS 1 Amar Del,C NA-","91S",-1306.3800000000001,"kN",228.29,"kN",4.3499999999999996,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CS 1 Amar Del,C NA-","91X",-1130.06,"kN",194.12,"kN",0.96,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CS 1 Amar Del,C NA-","91XY",1564.35,"kN",268.44,"kN",1.1100000000000001,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CS 1 Amar Del,C NA-","91Y",1386.86,"kN",238.17,"kN",4.9000000000000004,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CS 2 Amar Atras,C NA+","91S",-1249.3499999999999,"kN",213.5,"kN",2.78,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CS 2 Amar Atras,C NA+","91X",-1404.75,"kN",242.48,"kN",2.02,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CS 2 Amar Atras,C NA+","91XY",1505.88,"kN",254.01,"kN",2.4,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CS 2 Amar Atras,C NA+","91Y",1661.17,"kN",283.35000000000002,"kN",2.16,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CS 2 Amar Atras,C NA-","91S",-1415.67,"kN",243.59,"kN",2.2200000000000002,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CS 2 Amar Atras,C NA-","91X",-1238.6500000000001,"kN",211.39,"kN",2.38,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CS 2 Amar Atras,C NA-","91XY",1672.19,"kN",285.19,"kN",1.96,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CS 2 Amar Atras,C NA-","91Y",1495.08,"kN",253.13,"kN",2.72,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CS 2 Amar Del,C NA+","91S",-1140.24,"kN",196.04,"kN",1,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CS 2 Amar Del,C NA+","91X",-1295.98,"kN",227.28,"kN",4.3899999999999997,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CS 2 Amar Del,C NA+","91XY",1397.06,"kN",239.21,"kN",4.88,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CS 2 Amar Del,C NA+","91Y",1553.93,"kN",266.51,"kN",1.1299999999999999,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CS 2 Amar Del,C NA-","91S",-1306.48,"kN",226.48,"kN",1.31,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CS 2 Amar Del,C NA-","91X",-1129.95,"kN",196.87,"kN",4.88,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CS 2 Amar Del,C NA-","91XY",1563.29,"kN",269.87,"kN",4.3899999999999997,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CS 2 Amar Del,C NA-","91Y",1387.91,"kN",236.02,"kN",0.84,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CM 1 Amar Atras,C NA+","91S",-1247.32,"kN",213.17,"kN",2.4700000000000002,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CM 1 Amar Atras,C NA+","91X",-1403.37,"kN",242.49,"kN",2.34,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CM 1 Amar Atras,C NA+","91XY",1503.92,"kN",254.06,"kN",2.76,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CM 1 Amar Atras,C NA+","91Y",1660.11,"kN",283.14999999999998,"kN",1.89,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CM 1 Amar Atras,C NA-","91S",-1413.6,"kN",243.32,"kN",1.96,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CM 1 Amar Atras,C NA-","91X",-1237.3,"kN",211.48,"kN",2.75,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CM 1 Amar Atras,C NA-","91XY",1670.19,"kN",285.18,"kN",2.29,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CM 1 Amar Atras,C NA-","91Y",1494.05,"kN",252.9,"kN",2.42,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CM 1 Amar Del,C NA+","91S",-1162.6600000000001,"kN",200.58,"kN",4.9800000000000004,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CM 1 Amar Del,C NA+","91X",-1318.44,"kN",227.22,"kN",1.33,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CM 1 Amar Del,C NA+","91XY",1421.24,"kN",238.68,"kN",0.22,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CM 1 Amar Del,C NA+","91Y",1574.63,"kN",269.70999999999998,"kN",4.29,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CM 1 Amar Del,C NA-","91S",-1328.9,"kN",230.13,"kN",4.32,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CM 1 Amar Del,C NA-","91X",-1152.4100000000001,"kN",195.68,"kN",0.51,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CM 1 Amar Del,C NA-","91XY",1587.46,"kN",270.22000000000003,"kN",1.05,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CM 1 Amar Del,C NA-","91Y",1408.62,"kN",239.91,"kN",4.93,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CM 2 Amar Atras,C NA+","91S",-1247.98,"kN",213.46,"kN",2.83,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CM 2 Amar Atras,C NA+","91X",-1402.71,"kN",242.28,"kN",2.0299999999999998,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CM 2 Amar Atras,C NA+","91XY",1504.75,"kN",253.97,"kN",2.4,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CM 2 Amar Atras,C NA+","91Y",1659.28,"kN",283.19,"kN",2.2200000000000002,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CM 2 Amar Atras,C NA-","91S",-1414.26,"kN",243.53,"kN",2.2799999999999998,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CM 2 Amar Atras,C NA-","91X",-1236.6400000000001,"kN",211.19,"kN",2.39,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CM 2 Amar Atras,C NA-","91XY",1671.02,"kN",285.14,"kN",1.96,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CM 2 Amar Atras,C NA-","91Y",1493.23,"kN",252.99,"kN",2.77,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CM 2 Amar Del,C NA+","91S",-1162.92,"kN",197.66,"kN",0.48,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CM 2 Amar Del,C NA+","91X",-1318.17,"kN",229.07,"kN",4.3600000000000003,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CM 2 Amar Del,C NA+","91XY",1419.15,"kN",240.99,"kN",4.92,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CM 2 Amar Del,C NA+","91Y",1576.71,"kN",268.24,"kN",1.1200000000000001,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CM 2 Amar Del,C NA-","91S",-1329.16,"kN",228.19,"kN",1.27,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CM 2 Amar Del,C NA-","91X",-1152.1400000000001,"kN",198.67,"kN",4.8899999999999997,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CM 2 Amar Del,C NA-","91XY",1585.37,"kN",271.64999999999998,"kN",4.37,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CM 2 Amar Del,C NA-","91Y",1410.7,"kN",237.68,"kN",0.3,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CI 1 Amar Atras,C NA+","91S",-1246.3599999999999,"kN",213.17,"kN",2.52,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CI 1 Amar Atras,C NA+","91X",-1400.87,"kN",242.22,"kN",2.35,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CI 1 Amar Atras,C NA+","91XY",1502.67,"kN",253.99,"kN",2.76,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CI 1 Amar Atras,C NA+","91Y",1658.29,"kN",283.02,"kN",1.94,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CI 1 Amar Atras,C NA-","91S",-1412.61,"kN",243.31,"kN",2.0099999999999998,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CI 1 Amar Atras,C NA-","91X",-1234.82,"kN",211.22,"kN",2.75,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CI 1 Amar Atras,C NA-","91XY",1668.91,"kN",285.10000000000002,"kN",2.2999999999999998,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CI 1 Amar Atras,C NA-","91Y",1492.26,"kN",252.77,"kN",2.4700000000000002,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CI 1 Amar Del,C NA+","91S",-1181.3900000000001,"kN",201.05,"kN",4.28,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CI 1 Amar Del,C NA+","91X",-1344.58,"kN",229.62,"kN",1.04,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CI 1 Amar Del,C NA+","91XY",1446.68,"kN",240.96,"kN",0.18,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CI 1 Amar Del,C NA+","91Y",1594.06,"kN",270.55,"kN",3.56,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CI 1 Amar Del,C NA-","91S",-1347.63,"kN",230.76,"kN",3.59,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CI 1 Amar Del,C NA-","91X",-1178.56,"kN",198.08,"kN",0.18,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CI 1 Amar Del,C NA-","91XY",1612.89,"kN",272.48,"kN",0.78,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CI 1 Amar Del,C NA-","91Y",1428.05,"kN",240.62,"kN",4.24,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CI 2 Amar Atras,C NA+","91S",-1246.18,"kN",213.33,"kN",2.83,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CI 2 Amar Atras,C NA+","91X",-1401,"kN",242.12,"kN",2.08,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CI 2 Amar Atras,C NA+","91XY",1503.64,"kN",253.98,"kN",2.4500000000000002,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CI 2 Amar Atras,C NA+","91Y",1657.28,"kN",282.95999999999998,"kN",2.23,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CI 2 Amar Atras,C NA-","91S",-1412.43,"kN",243.41,"kN",2.2799999999999998,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CI 2 Amar Atras,C NA-","91X",-1234.95,"kN",211.05,"kN",2.4500000000000002,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CI 2 Amar Atras,C NA-","91XY",1669.88,"kN",285.14999999999998,"kN",2.0099999999999998,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CI 2 Amar Atras,C NA-","91Y",1491.25,"kN",252.76,"kN",2.78,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CI 2 Amar Del,C NA+","91S",-1188.82,"kN",200.01,"kN",0.12,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CI 2 Amar Del,C NA+","91X",-1337.14,"kN",229.77,"kN",3.62,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CI 2 Amar Del,C NA+","91XY",1438.34,"kN",241.64,"kN",4.24,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CI 2 Amar Del,C NA+","91Y",1602.39,"kN",270.56,"kN",0.87,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CI 2 Amar Del,C NA-","91S",-1355.05,"kN",230.53,"kN",0.98,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CI 2 Amar Del,C NA-","91X",-1171.1199999999999,"kN",199.18,"kN",4.1900000000000004,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CI 2 Amar Del,C NA-","91XY",1604.56,"kN",272.44,"kN",3.65,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CI 2 Amar Del,C NA-","91Y",1436.39,"kN",240.01,"kN",0.1,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CS Amar Atras (A4),C NA+","91S",-1241.81,"kN",212.3,"kN",2.64,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CS Amar Atras (A4),C NA+","91X",-1397.14,"kN",241.36,"kN",2.17,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CS Amar Atras (A4),C NA+","91XY",1498.78,"kN",253.04,"kN",2.57,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CS Amar Atras (A4),C NA+","91Y",1654.07,"kN",282.19,"kN",2.04,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CS Amar Atras (A4),C NA-","91S",-1408.03,"kN",242.4,"kN",2.1,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CS Amar Atras (A4),C NA-","91X",-1231.1300000000001,"kN",210.32,"kN",2.56,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CS Amar Atras (A4),C NA-","91XY",1664.98,"kN",284.18,"kN",2.11,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CS Amar Atras (A4),C NA-","91Y",1488.08,"kN",251.97,"kN",2.58,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CS Amar Del (A4),C NA+","91S",-1241.81,"kN",212.3,"kN",2.64,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CS Amar Del (A4),C NA+","91X",-1397.14,"kN",241.36,"kN",2.17,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CS Amar Del (A4),C NA+","91XY",1498.78,"kN",253.04,"kN",2.57,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CS Amar Del (A4),C NA+","91Y",1654.07,"kN",282.19,"kN",2.04,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CS Amar Del (A4),C NA-","91S",-1408.03,"kN",242.4,"kN",2.1,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CS Amar Del (A4),C NA-","91X",-1231.1300000000001,"kN",210.32,"kN",2.56,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CS Amar Del (A4),C NA-","91XY",1664.98,"kN",284.18,"kN",2.11,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CS Amar Del (A4),C NA-","91Y",1488.08,"kN",251.97,"kN",2.58,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CM Amar Atras (A4),C NA+","91S",-1241.81,"kN",212.3,"kN",2.64,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CM Amar Atras (A4),C NA+","91X",-1397.14,"kN",241.36,"kN",2.17,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CM Amar Atras (A4),C NA+","91XY",1498.78,"kN",253.04,"kN",2.57,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CM Amar Atras (A4),C NA+","91Y",1654.07,"kN",282.19,"kN",2.04,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CM Amar Atras (A4),C NA-","91S",-1408.03,"kN",242.4,"kN",2.1,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CM Amar Atras (A4),C NA-","91X",-1231.1300000000001,"kN",210.32,"kN",2.56,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CM Amar Atras (A4),C NA-","91XY",1664.98,"kN",284.18,"kN",2.11,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CM Amar Atras (A4),C NA-","91Y",1488.08,"kN",251.97,"kN",2.58,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CM Amar Del (A4),C NA+","91S",-1241.81,"kN",212.3,"kN",2.64,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CM Amar Del (A4),C NA+","91X",-1397.14,"kN",241.36,"kN",2.17,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CM Amar Del (A4),C NA+","91XY",1498.78,"kN",253.04,"kN",2.57,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CM Amar Del (A4),C NA+","91Y",1654.07,"kN",282.19,"kN",2.04,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CM Amar Del (A4),C NA-","91S",-1408.03,"kN",242.4,"kN",2.1,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CM Amar Del (A4),C NA-","91X",-1231.1300000000001,"kN",210.32,"kN",2.56,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CM Amar Del (A4),C NA-","91XY",1664.98,"kN",284.18,"kN",2.11,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CM Amar Del (A4),C NA-","91Y",1488.08,"kN",251.97,"kN",2.58,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CI Amar Atras (A4),C NA+","91S",-1241.81,"kN",212.3,"kN",2.64,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CI Amar Atras (A4),C NA+","91X",-1397.14,"kN",241.36,"kN",2.17,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CI Amar Atras (A4),C NA+","91XY",1498.78,"kN",253.04,"kN",2.57,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CI Amar Atras (A4),C NA+","91Y",1654.07,"kN",282.19,"kN",2.04,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CI Amar Atras (A4),C NA-","91S",-1408.03,"kN",242.4,"kN",2.1,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CI Amar Atras (A4),C NA-","91X",-1231.1300000000001,"kN",210.32,"kN",2.56,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CI Amar Atras (A4),C NA-","91XY",1664.98,"kN",284.18,"kN",2.11,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CI Amar Atras (A4),C NA-","91Y",1488.08,"kN",251.97,"kN",2.58,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CI Amar Del (A4),C NA+","91S",-1241.81,"kN",212.3,"kN",2.64,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CI Amar Del (A4),C NA+","91X",-1397.14,"kN",241.36,"kN",2.17,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CI Amar Del (A4),C NA+","91XY",1498.78,"kN",253.04,"kN",2.57,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","Rotura CI Amar Del (A4),C NA+","91Y",1654.07,"kN",282.19,"kN",2.04,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CI Amar Del (A4),C NA-","91S",-1408.03,"kN",242.4,"kN",2.1,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CI Amar Del (A4),C NA-","91X",-1231.1300000000001,"kN",210.32,"kN",2.56,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CI Amar Del (A4),C NA-","91XY",1664.98,"kN",284.18,"kN",2.11,"kN-m",0]
["T-1","d4a4f-aa-vidrio_ed.l_v3.tow","-Rotura CI Amar Del (A4),C NA-","91Y",1488.08,"kN",251.97,"kN",2.58,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Viento,C NA+","99S",1570.74,"kN",274.68,"kN",4.1500000000000004,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Viento,C NA+","99X",-1253.47,"kN",226.65,"kN",4.0199999999999996,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Viento,C NA+","99XY",-1266.54,"kN",228.93,"kN",3.98,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Viento,C NA+","99Y",1557.65,"kN",272.32,"kN",4.13,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Viento,C NA-","99S",584.49,"kN",90.08,"kN",1.35,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Viento,C NA-","99X",-306.14999999999998,"kN",42.75,"kN",1.1299999999999999,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Viento,C NA-","99XY",-280.23,"kN",38.630000000000003,"kN",1.1399999999999999,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Viento,C NA-","99Y",610.29,"kN",94.28,"kN",1.41,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Hielo,C NA+","99S",1119.22,"kN",189.29,"kN",1.51,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Hielo,C NA+","99X",-773.36,"kN",133.61000000000001,"kN",1.63,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Hielo,C NA+","99XY",-780.1,"kN",134.87,"kN",1.55,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Hielo,C NA+","99Y",1112.3399999999999,"kN",187.91,"kN",1.46,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Viento+Hielo,C NA-","99S",1009.79,"kN",169.18,"kN",1.01,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Viento+Hielo,C NA-","99X",-677.11,"kN",115.1,"kN",1.18,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Viento+Hielo,C NA-","99XY",-670.42,"kN",114.15,"kN",1.0900000000000001,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Viento+Hielo,C NA-","99Y",1016.33,"kN",170.03,"kN",0.94,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Viento+Hielo,C NA+","99S",1271.46,"kN",216.56,"kN",2.0699999999999998,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Viento+Hielo,C NA+","99X",-925.73,"kN",161.47,"kN",2.14,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Viento+Hielo,C NA+","99XY",-932.11,"kN",162.68,"kN",2.06,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Viento+Hielo,C NA+","99Y",1264.97,"kN",215.23,"kN",2.0099999999999998,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Tiro Vertical,C NA+","99S",838.33,"kN",141.77000000000001,"kN",1.1100000000000001,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Tiro Vertical,C NA+","99X",-453.38,"kN",79.319999999999993,"kN",1.27,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Tiro Vertical,C NA+","99XY",-536.72,"kN",93.18,"kN",1.05,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Tiro Vertical,C NA+","99Y",754.37,"kN",127.54,"kN",1,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Desequilibrio Amar Atras,C NA+","99S",768.35,"kN",131.77000000000001,"kN",1.42,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Desequilibrio Amar Atras,C NA+","99X",-1179.97,"kN",203.63,"kN",1.42,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Desequilibrio Amar Atras,C NA+","99XY",-433.76,"kN",81.31,"kN",2.95,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Desequilibrio Amar Atras,C NA+","99Y",1520.03,"kN",258.13,"kN",2.3199999999999998,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Desequilibrio Amar Atras,C NA-","99S",506.6,"kN",84.32,"kN",0.37,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Desequilibrio Amar Atras,C NA-","99X",-931.21,"kN",157.62,"kN",0.8,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Desequilibrio Amar Atras,C NA-","99XY",-172,"kN",34.1,"kN",2.11,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Desequilibrio Amar Atras,C NA-","99Y",1271.25,"kN",212.94,"kN",1.25,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Desequilibrio Amar Del,C NA+","99S",1527.35,"kN",259.58,"kN",2.38,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Desequilibrio Amar Del,C NA+","99X",-426.87,"kN",80.260000000000005,"kN",3.05,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Desequilibrio Amar Del,C NA+","99XY",-1185.69,"kN",204.8,"kN",1.44,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Desequilibrio Amar Del,C NA+","99Y",762.86,"kN",130.63999999999999,"kN",1.38,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Desequilibrio Amar Del,C NA-","99S",1265.42,"kN",212.19,"kN",1.32,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Desequilibrio Amar Del,C NA-","99X",-178.11,"kN",35.159999999999997,"kN",2.2200000000000002,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Desequilibrio Amar Del,C NA-","99XY",-923.75,"kN",156.61000000000001,"kN",0.88,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Desequilibrio Amar Del,C NA-","99Y",514.09,"kN",85.35,"kN",0.32,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CT1 Atras,C NA+","99S",1181.33,"kN",203.09,"kN",1.41,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CT1 Atras,C NA+","99X",-969.12,"kN",167.16,"kN",1.39,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CT1 Atras,C NA+","99XY",-843.77,"kN",150.71,"kN",3.01,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CT1 Atras,C NA+","99Y",1307.33,"kN",221.93,"kN",3.19,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CT1 Atras,C NA-","99S",922.92,"kN",156.31,"kN",0.73,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CT1 Atras,C NA-","99X",-726.95,"kN",121.89,"kN",0.38,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CT1 Atras,C NA-","99XY",-585.36,"kN",102.59,"kN",2.08,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CT1 Atras,C NA-","99Y",1065.1500000000001,"kN",177.58,"kN",2.21,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CT1 Del,C NA+","99S",1313.89,"kN",223.28,"kN",3.27,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CT1 Del,C NA+","99X",-834.65,"kN",149.18,"kN",3.13,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CT1 Del,C NA+","99XY",-975.66,"kN",168.42,"kN",1.34,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CT1 Del,C NA+","99Y",1171.98,"kN",201.35,"kN",1.35,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CT1 Del,C NA-","99S",1060.3900000000001,"kN",177.02,"kN",2.31,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CT1 Del,C NA-","99X",-590.14,"kN",103.33,"kN",2.2000000000000002,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CT1 Del,C NA-","99XY",-722.13,"kN",121.23,"kN",0.38,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CT1 Del,C NA-","99Y",927.44,"kN",156.88999999999999,"kN",0.76,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CT2 Atras,C NA+","99S",1179.97,"kN",203.92,"kN",2.92,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CT2 Atras,C NA+","99X",-967.55,"kN",168.34,"kN",3.09,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CT2 Atras,C NA+","99XY",-841.69,"kN",149.28,"kN",1.7,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CT2 Atras,C NA+","99Y",1305.05,"kN",220.78,"kN",1.4,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CT2 Atras,C NA-","99S",921.54,"kN",156.94,"kN",1.86,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CT2 Atras,C NA-","99X",-725.28,"kN",122.82,"kN",2.2400000000000002,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CT2 Atras,C NA-","99XY",-583.23,"kN",101.36,"kN",0.86,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CT2 Atras,C NA-","99Y",1062.77,"kN",176.58,"kN",0.28999999999999998,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CT2 Del,C NA+","99S",1312.18,"kN",222.2,"kN",1.45,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CT2 Del,C NA+","99X",-832.64,"kN",147.65,"kN",1.71,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CT2 Del,C NA+","99XY",-974.66,"kN",169.65,"kN",3.02,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CT2 Del,C NA+","99Y",1170.71,"kN",202.21,"kN",2.88,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CT2 Del,C NA-","99S",1058.54,"kN",176.05,"kN",0.33,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CT2 Del,C NA-","99X",-588.15,"kN",102.02,"kN",0.83,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CT2 Del,C NA-","99XY",-721.02,"kN",122.21,"kN",2.16,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CT2 Del,C NA-","99Y",926.22,"kN",157.52000000000001,"kN",1.81,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CS 1  Amar Atras,C NA+","99S",1144.6099999999999,"kN",196.62,"kN",1.27,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CS 1  Amar Atras,C NA+","99X",-990.11,"kN",170.51,"kN",1.1100000000000001,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CS 1  Amar Atras,C NA+","99XY",-806.34,"kN",145.44,"kN",3.9,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CS 1  Amar Atras,C NA+","99Y",1329.61,"kN",226.38,"kN",4.08,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CS 1 Amar Atras,C NA-","99S",882.91,"kN",149.55000000000001,"kN",1.36,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CS 1 Amar Atras,C NA-","99X",-741.45,"kN",124.57,"kN",0.94,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CS 1 Amar Atras,C NA-","99XY",-544.62,"kN",96.93,"kN",3.01,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CS 1 Amar Atras,C NA-","99Y",1080.93,"kN",181.06,"kN",3.1,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CS 1  Amar Del,C NA+","99S",1271.46,"kN",216.56,"kN",2.0699999999999998,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CS 1  Amar Del,C NA+","99X",-925.73,"kN",161.47,"kN",2.14,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CS 1  Amar Del,C NA+","99XY",-932.11,"kN",162.68,"kN",2.06,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CS 1  Amar Del,C NA+","99Y",1264.97,"kN",215.23,"kN",2.0099999999999998,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CS 1 Amar Del,C NA-","99S",1009.79,"kN",169.18,"kN",1.01,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CS 1 Amar Del,C NA-","99X",-677.11,"kN",115.1,"kN",1.18,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CS 1 Amar Del,C NA-","99XY",-670.42,"kN",114.15,"kN",1.0900000000000001,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CS 1 Amar Del,C NA-","99Y",1016.33,"kN",170.03,"kN",0.94,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CS 2 Amar Atras,C NA+","99S",1144.74,"kN",198.35,"kN",3.64,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CS 2 Amar Atras,C NA+","99X",-990.37,"kN",172.75,"kN",3.77,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CS 2 Amar Atras,C NA+","99XY",-805.23,"kN",142.66,"kN",1.52,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CS 2 Amar Atras,C NA+","99Y",1328.62,"kN",224.5,"kN",0.87,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CS 2 Amar Atras,C NA-","99S",883.05,"kN",150.88999999999999,"kN",2.62,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CS 2 Amar Atras,C NA-","99X",-741.7,"kN",126.3,"kN",2.94,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CS 2 Amar Atras,C NA-","99XY",-543.51,"kN",94.5,"kN",1.1599999999999999,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CS 2 Amar Atras,C NA-","99Y",1079.93,"kN",179.52,"kN",0.69,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CS 2 Amar Del,C NA+","99S",1335.77,"kN",225.9,"kN",0.92,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CS 2 Amar Del,C NA+","99X",-799.48,"kN",141.47,"kN",1.47,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CS 2 Amar Del,C NA+","99XY",-997.12,"kN",173.93,"kN",3.65,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CS 2 Amar Del,C NA+","99Y",1139.1600000000001,"kN",197.14,"kN",3.58,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CS 2 Amar Del,C NA-","99S",1074.02,"kN",178.73,"kN",0.64,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CS 2 Amar Del,C NA-","99X",-550.82000000000005,"kN",95.46,"kN",1.05,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CS 2 Amar Del,C NA-","99XY",-735.36,"kN",125.33,"kN",2.81,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CS 2 Amar Del,C NA-","99Y",890.49,"kN",151.82,"kN",2.54,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CM 1 Amar Atras,C NA+","99S",1169.74,"kN",198.62,"kN",0.92,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CM 1 Amar Atras,C NA+","99X",-977.53,"kN",169.52,"kN",1.39,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CM 1 Amar Atras,C NA+","99XY",-831.82,"kN",147.69999999999999,"kN",4,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CM 1 Amar Atras,C NA+","99Y",1317.39,"kN",225.26,"kN",3.87,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CM 1 Amar Atras,C NA-","99S",908.05,"kN",151.53,"kN",1.1499999999999999,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CM 1 Amar Atras,C NA-","99X",-728.87,"kN",123.7,"kN",1.37,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CM 1 Amar Atras,C NA-","99XY",-570.11,"kN",99.22,"kN",3.17,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CM 1 Amar Atras,C NA-","99Y",1068.71,"kN",179.94,"kN",2.87,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CM 1 Amar Del,C NA+","99S",1271.46,"kN",216.56,"kN",2.0699999999999998,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CM 1 Amar Del,C NA+","99X",-925.73,"kN",161.47,"kN",2.14,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CM 1 Amar Del,C NA+","99XY",-932.11,"kN",162.68,"kN",2.06,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CM 1 Amar Del,C NA+","99Y",1264.97,"kN",215.23,"kN",2.0099999999999998,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CM 1 Amar Del,C NA-","99S",1009.79,"kN",169.18,"kN",1.01,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CM 1 Amar Del,C NA-","99X",-677.11,"kN",115.1,"kN",1.18,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CM 1 Amar Del,C NA-","99XY",-670.42,"kN",114.15,"kN",1.0900000000000001,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CM 1 Amar Del,C NA-","99Y",1016.33,"kN",170.03,"kN",0.94,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CM 2 Amar Atras,C NA+","99S",1170,"kN",200.71,"kN",3.98,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CM 2 Amar Atras,C NA+","99X",-977.7,"kN",171.74,"kN",3.79,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CM 2 Amar Atras,C NA+","99XY",-830.08,"kN",144.59,"kN",1.21,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CM 2 Amar Atras,C NA+","99Y",1315.54,"kN",223.42,"kN",1.07,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CM 2 Amar Atras,C NA-","99S",908.3,"kN",153.26,"kN",3.01,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CM 2 Amar Atras,C NA-","99X",-729.04,"kN",125.29,"kN",2.93,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CM 2 Amar Atras,C NA-","99XY",-568.37,"kN",96.48,"kN",1.06,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CM 2 Amar Atras,C NA-","99Y",1066.8699999999999,"kN",178.55,"kN",1.32,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CM 2 Amar Del,C NA+","99S",1322.73,"kN",224.82,"kN",1.0900000000000001,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CM 2 Amar Del,C NA+","99X",-824.28,"kN",143.4,"kN",1.1399999999999999,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CM 2 Amar Del,C NA+","99XY",-984.46,"kN",172.92,"kN",3.68,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CM 2 Amar Del,C NA+","99Y",1164.3900000000001,"kN",199.49,"kN",3.92,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CM 2 Amar Del,C NA-","99S",1061,"kN",177.75,"kN",1.27,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CM 2 Amar Del,C NA-","99X",-575.62,"kN",97.43,"kN",0.94,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CM 2 Amar Del,C NA-","99XY",-722.71,"kN",124.32,"kN",2.81,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CM 2 Amar Del,C NA-","99Y",915.72,"kN",154.18,"kN",2.94,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CI 1 Amar Atras,C NA+","99S",1190.6300000000001,"kN",199.97,"kN",0.59,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CI 1 Amar Atras,C NA+","99X",-960.3,"kN",167.84,"kN",1.77,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CI 1 Amar Atras,C NA+","99XY",-860.76,"kN",150.52000000000001,"kN",4.18,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CI 1 Amar Atras,C NA+","99Y",1308.21,"kN",224.61,"kN",3.72,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CI 1 Amar Atras,C NA-","99S",928.94,"kN",152.87,"kN",1.08,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CI 1 Amar Atras,C NA-","99X",-711.65,"kN",122.19,"kN",1.84,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CI 1 Amar Atras,C NA-","99XY",-599.05999999999995,"kN",102.08,"kN",3.42,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CI 1 Amar Atras,C NA-","99Y",1059.55,"kN",179.3,"kN",2.69,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CI 1 Amar Del,C NA+","99S",1271.46,"kN",216.56,"kN",2.0699999999999998,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CI 1 Amar Del,C NA+","99X",-925.73,"kN",161.47,"kN",2.14,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CI 1 Amar Del,C NA+","99XY",-932.11,"kN",162.68,"kN",2.06,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CI 1 Amar Del,C NA+","99Y",1264.97,"kN",215.23,"kN",2.0099999999999998,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CI 1 Amar Del,C NA-","99S",1009.79,"kN",169.18,"kN",1.01,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CI 1 Amar Del,C NA-","99X",-677.11,"kN",115.1,"kN",1.18,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CI 1 Amar Del,C NA-","99XY",-670.42,"kN",114.15,"kN",1.0900000000000001,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CI 1 Amar Del,C NA-","99Y",1016.33,"kN",170.03,"kN",0.94,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CI 2 Amar Atras,C NA+","99S",1197.44,"kN",202.89,"kN",3.79,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CI 2 Amar Atras,C NA+","99X",-967.24,"kN",170.52,"kN",3.29,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CI 2 Amar Atras,C NA+","99XY",-852.99,"kN",146.34,"kN",0.86,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CI 2 Amar Atras,C NA+","99Y",1300.55,"kN",222.09,"kN",1.25,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CI 2 Amar Atras,C NA-","99S",935.75,"kN",155.43,"kN",2.87,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CI 2 Amar Atras,C NA-","99X",-718.59,"kN",124.07,"kN",2.38,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CI 2 Amar Atras,C NA-","99XY",-591.29,"kN",98.08,"kN",0.52,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CI 2 Amar Atras,C NA-","99Y",1051.8900000000001,"kN",177.23,"kN",1.42,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CI 2 Amar Del,C NA+","99S",1307.5999999999999,"kN",223.47,"kN",1.27,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CI 2 Amar Del,C NA+","99X",-847.01,"kN",145.13999999999999,"kN",0.86,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CI 2 Amar Del,C NA+","99XY",-973.81,"kN",171.7,"kN",3.19,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CI 2 Amar Del,C NA+","99Y",1191.68,"kN",201.65,"kN",3.73,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CI 2 Amar Del,C NA-","99S",1045.8800000000001,"kN",176.41,"kN",1.37,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CI 2 Amar Del,C NA-","99X",-598.36,"kN",99.02,"kN",0.4,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CI 2 Amar Del,C NA-","99XY",-712.08,"kN",123.09,"kN",2.2799999999999998,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CI 2 Amar Del,C NA-","99Y",943.01,"kN",156.34,"kN",2.8,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CS Amar Atras (A4),C NA+","99S",1271.46,"kN",216.56,"kN",2.0699999999999998,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CS Amar Atras (A4),C NA+","99X",-925.73,"kN",161.47,"kN",2.14,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CS Amar Atras (A4),C NA+","99XY",-932.11,"kN",162.68,"kN",2.06,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CS Amar Atras (A4),C NA+","99Y",1264.97,"kN",215.23,"kN",2.0099999999999998,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CS Amar Atras (A4),C NA-","99S",1009.79,"kN",169.18,"kN",1.01,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CS Amar Atras (A4),C NA-","99X",-677.11,"kN",115.1,"kN",1.18,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CS Amar Atras (A4),C NA-","99XY",-670.42,"kN",114.15,"kN",1.0900000000000001,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CS Amar Atras (A4),C NA-","99Y",1016.33,"kN",170.03,"kN",0.94,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CS Amar Del (A4),C NA+","99S",1335.48,"kN",227.63,"kN",4.12,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CS Amar Del (A4),C NA+","99X",-799.83,"kN",144.32,"kN",4,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CS Amar Del (A4),C NA+","99XY",-995.58,"kN",171.67,"kN",1.18,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CS Amar Del (A4),C NA+","99Y",1138.27,"kN",195.34,"kN",1.24,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CS Amar Del (A4),C NA-","99S",1073.72,"kN",180.16,"kN",3.16,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CS Amar Del (A4),C NA-","99X",-551.16,"kN",97.96,"kN",3.12,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CS Amar Del (A4),C NA-","99XY",-733.81,"kN",123.57,"kN",1.05,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CS Amar Del (A4),C NA-","99Y",889.59,"kN",150.47,"kN",1.4,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CM Amar Atras (A4),C NA+","99S",1271.46,"kN",216.56,"kN",2.0699999999999998,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CM Amar Atras (A4),C NA+","99X",-925.73,"kN",161.47,"kN",2.14,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CM Amar Atras (A4),C NA+","99XY",-932.11,"kN",162.68,"kN",2.06,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CM Amar Atras (A4),C NA+","99Y",1264.97,"kN",215.23,"kN",2.0099999999999998,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CM Amar Atras (A4),C NA-","99S",1009.79,"kN",169.18,"kN",1.01,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CM Amar Atras (A4),C NA-","99X",-677.11,"kN",115.1,"kN",1.18,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CM Amar Atras (A4),C NA-","99XY",-670.42,"kN",114.15,"kN",1.0900000000000001,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CM Amar Atras (A4),C NA-","99Y",1016.33,"kN",170.03,"kN",0.94,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CM Amar Del (A4),C NA+","99S",1323.24,"kN",226.5,"kN",3.92,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CM Amar Del (A4),C NA+","99X",-825.18,"kN",146.57,"kN",4.1100000000000003,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CM Amar Del (A4),C NA+","99XY",-982.96,"kN",170.68,"kN",1.48,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CM Amar Del (A4),C NA+","99Y",1163.3,"kN",197.34,"kN",0.9,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CM Amar Del (A4),C NA-","99S",1061.5,"kN",179.03,"kN",2.93,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CM Amar Del (A4),C NA-","99X",-576.52,"kN",100.24,"kN",3.28,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CM Amar Del (A4),C NA-","99XY",-721.21,"kN",122.71,"kN",1.48,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CM Amar Del (A4),C NA-","99Y",914.63,"kN",152.44,"kN",1.2,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CI Amar Atras (A4),C NA+","99S",1271.46,"kN",216.56,"kN",2.0699999999999998,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CI Amar Atras (A4),C NA+","99X",-925.73,"kN",161.47,"kN",2.14,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CI Amar Atras (A4),C NA+","99XY",-932.11,"kN",162.68,"kN",2.06,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CI Amar Atras (A4),C NA+","99Y",1264.97,"kN",215.23,"kN",2.0099999999999998,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CI Amar Atras (A4),C NA-","99S",1009.79,"kN",169.18,"kN",1.01,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CI Amar Atras (A4),C NA-","99X",-677.11,"kN",115.1,"kN",1.18,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CI Amar Atras (A4),C NA-","99XY",-670.42,"kN",114.15,"kN",1.0900000000000001,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CI Amar Atras (A4),C NA-","99Y",1016.33,"kN",170.03,"kN",0.94,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CI Amar Del (A4),C NA+","99S",1314.3,"kN",225.9,"kN",3.77,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CI Amar Del (A4),C NA+","99X",-854.1,"kN",149.41,"kN",4.3,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CI Amar Del (A4),C NA+","99XY",-965.97,"kN",169.05,"kN",1.87,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","Rotura CI Amar Del (A4),C NA+","99Y",1184.22,"kN",198.7,"kN",0.56999999999999995,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CI Amar Del (A4),C NA-","99S",1052.58,"kN",178.43,"kN",2.76,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CI Amar Del (A4),C NA-","99X",-605.45000000000005,"kN",103.11,"kN",3.53,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CI Amar Del (A4),C NA-","99XY",-704.23,"kN",121.25,"kN",1.96,"kN-m",0]
["T-2","d4a4a-ab-vidrio_ed.l_v3.tow","-Rotura CI Amar Del (A4),C NA-","99Y",935.56,"kN",153.80000000000001,"kN",1.1299999999999999,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Viento,C NA+","101S",506.64,"kN",69.61,"kN",0.27,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Viento,C NA+","101X",-387.21,"kN",56.87,"kN",0.24,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Viento,C NA+","101XY",-388.11,"kN",56.95,"kN",0.24,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Viento,C NA+","101Y",505.84,"kN",69.5,"kN",0.27,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Viento,C NA-","101S",-395.1,"kN",56.44,"kN",0.3,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Viento,C NA-","101X",512.82000000000005,"kN",71.84,"kN",0.19,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Viento,C NA-","101XY",513.66999999999996,"kN",71.95,"kN",0.2,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Viento,C NA-","101Y",-394.22,"kN",56.34,"kN",0.31,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Hielo,C NA+","101S",73.430000000000007,"kN",8.8699999999999992,"kN",0.01,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Hielo,C NA+","101X",80.33,"kN",9.74,"kN",0.01,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Hielo,C NA+","101XY",80.34,"kN",9.74,"kN",0.01,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Hielo,C NA+","101Y",73.44,"kN",8.8800000000000008,"kN",0.01,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Viento+Hielo,C NA-","101S",-54.5,"kN",8.9700000000000006,"kN",0.08,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Viento+Hielo,C NA-","101X",207.87,"kN",27.62,"kN",0.04,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Viento+Hielo,C NA-","101XY",208.17,"kN",27.66,"kN",0.04,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Viento+Hielo,C NA-","101Y",-54.21,"kN",8.93,"kN",0.08,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Viento+Hielo,C NA+","101S",201.07,"kN",26.51,"kN",0.06,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Viento+Hielo,C NA+","101X",-47.13,"kN",8.33,"kN",7.0000000000000007E-2,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Viento+Hielo,C NA+","101XY",-47.42,"kN",8.36,"kN",7.0000000000000007E-2,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Viento+Hielo,C NA+","101Y",200.8,"kN",26.47,"kN",0.06,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Tiro Vertical,C NA+","101S",57.65,"kN",7.02,"kN",0.01,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Tiro Vertical,C NA+","101X",62.19,"kN",7.6,"kN",0.01,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Tiro Vertical,C NA+","101XY",62.2,"kN",7.6,"kN",0.01,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Tiro Vertical,C NA+","101Y",57.66,"kN",7.02,"kN",0.01,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Atras,C NA+","101S",-173.35,"kN",19.97,"kN",0.24,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Atras,C NA+","101X",-434.28,"kN",54.78,"kN",0.14000000000000001,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Atras,C NA+","101XY",335.01,"kN",39.08,"kN",0.24,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Atras,C NA+","101Y",580.71,"kN",73.37,"kN",0.32,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Atras,C NA-","101S",-441.05,"kN",55.38,"kN",0.13,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Atras,C NA-","101X",-167.15,"kN",19,"kN",0.27,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Atras,C NA-","101XY",587.01,"kN",74.45,"kN",0.3,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Atras,C NA-","101Y",329.28,"kN",38.619999999999997,"kN",0.27,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Del,C NA+","101S",580.47,"kN",73.33,"kN",0.31,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Del,C NA+","101X",335.76,"kN",39.18,"kN",0.24,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Del,C NA+","101XY",-434.06,"kN",54.75,"kN",0.14000000000000001,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Del,C NA+","101Y",-174.17,"kN",20.07,"kN",0.24,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Del,C NA-","101S",328.53,"kN",38.520000000000003,"kN",0.27,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Del,C NA-","101X",587.14,"kN",74.48,"kN",0.3,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Del,C NA-","101XY",-166.39,"kN",18.899999999999999,"kN",0.27,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Del,C NA-","101Y",-441.27,"kN",55.41,"kN",0.13,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Atras,C NA+","101S",93.19,"kN",14.87,"kN",0.32,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Atras,C NA+","101X",-159.94999999999999,"kN",19.96,"kN",0.16,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Atras,C NA+","101XY",68.760000000000005,"kN",8.6999999999999993,"kN",0.27,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Atras,C NA+","101Y",302.52,"kN",39.590000000000003,"kN",0.41,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Atras,C NA-","101S",-154.94,"kN",22.85,"kN",0.41,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Atras,C NA-","101X",88.17,"kN",17.03,"kN",0.25,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Atras,C NA-","101XY",315.98,"kN",38.869999999999997,"kN",0.16,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Atras,C NA-","101Y",55.3,"kN",6.82,"kN",0.31,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Del,C NA+","101S",303.23,"kN",39.68,"kN",0.41,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Del,C NA+","101X",68.83,"kN",8.7200000000000006,"kN",0.27,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Del,C NA+","101XY",-160.43,"kN",20.02,"kN",0.16,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Del,C NA+","101Y",93.38,"kN",14.89,"kN",0.32,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Del,C NA-","101S",54.15,"kN",6.76,"kN",0.31,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Del,C NA-","101X",316.83999999999997,"kN",38.950000000000003,"kN",0.16,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Del,C NA-","101XY",89.59,"kN",17.149999999999999,"kN",0.25,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Del,C NA-","101Y",-155.56,"kN",22.89,"kN",0.41,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Atras,C NA+","101S",81.89,"kN",16,"kN",0.27,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Atras,C NA+","101X",-147.75,"kN",22.31,"kN",0.38,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Atras,C NA+","101XY",61.65,"kN",7.08,"kN",0.33,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Atras,C NA+","101Y",308.76,"kN",37.729999999999997,"kN",0.14000000000000001,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Atras,C NA-","101S",-166.91,"kN",20.62,"kN",0.14000000000000001,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Atras,C NA-","101X",99.98,"kN",15.8,"kN",0.35,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Atras,C NA-","101XY",309.42,"kN",40.729999999999997,"kN",0.39,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Atras,C NA-","101Y",62.06,"kN",8.31,"kN",0.28999999999999998,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Del,C NA+","101S",309.89,"kN",37.85,"kN",0.14000000000000001,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Del,C NA+","101X",61.34,"kN",7.07,"kN",0.33,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Del,C NA+","101XY",-148.65,"kN",22.37,"kN",0.38,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Del,C NA+","101Y",82.47,"kN",16.03,"kN",0.27,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Del,C NA-","101S",61.31,"kN",8.2799999999999994,"kN",0.28999999999999998,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Del,C NA-","101X",309.85000000000002,"kN",40.78,"kN",0.39,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Del,C NA-","101XY",101,"kN",15.92,"kN",0.35,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Del,C NA-","101Y",-167.11,"kN",20.64,"kN",0.14000000000000001,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Atras,C NA+","101S",89.99,"kN",15.68,"kN",0.47,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Atras,C NA+","101X",-175.63,"kN",22.67,"kN",0.34,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Atras,C NA+","101XY",79.010000000000005,"kN",13.01,"kN",0.43,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Atras,C NA+","101Y",314.2,"kN",42.65,"kN",0.56000000000000005,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Atras,C NA-","101S",-168.67,"kN",25.17,"kN",0.46,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Atras,C NA-","101X",83.07,"kN",17.32,"kN",0.32,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Atras,C NA-","101XY",333.65,"kN",41.05,"kN",0.25,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Atras,C NA-","101Y",59.53,"kN",8.76,"kN",0.37,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Del,C NA+","101S",314.23,"kN",42.65,"kN",0.56000000000000005,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Del,C NA+","101X",79.53,"kN",13.03,"kN",0.43,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Del,C NA+","101XY",-175.65,"kN",22.67,"kN",0.34,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Del,C NA+","101Y",89.45,"kN",15.62,"kN",0.47,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Del,C NA-","101S",59.02,"kN",8.6999999999999993,"kN",0.37,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Del,C NA-","101X",333.57,"kN",41.04,"kN",0.25,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Del,C NA-","101XY",83.61,"kN",17.350000000000001,"kN",0.32,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Del,C NA-","101Y",-168.63,"kN",25.15,"kN",0.46,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Atras,C NA+","101S",76.47,"kN",16.36,"kN",0.34,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Atras,C NA+","101X",-161.65,"kN",24.69,"kN",0.44,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Atras,C NA+","101XY",66.099999999999994,"kN",9.09,"kN",0.39,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Atras,C NA+","101Y",326.66000000000003,"kN",39.97,"kN",0.23,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Atras,C NA-","101S",-182.89,"kN",23.36,"kN",0.31,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Atras,C NA-","101X",96.53,"kN",16.440000000000001,"kN",0.5,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Atras,C NA-","101XY",321.26,"kN",43.81,"kN",0.54,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Atras,C NA-","101Y",72.69,"kN",12.71,"kN",0.45,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Del,C NA+","101S",326.83999999999997,"kN",39.99,"kN",0.23,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Del,C NA+","101X",66.47,"kN",9.11,"kN",0.39,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Del,C NA+","101XY",-161.84,"kN",24.71,"kN",0.44,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Del,C NA+","101Y",76.09,"kN",16.32,"kN",0.34,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Del,C NA-","101S",72.31,"kN",12.7,"kN",0.45,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Del,C NA-","101X",321.02999999999997,"kN",43.79,"kN",0.54,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Del,C NA-","101XY",96.91,"kN",16.48,"kN",0.5,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Del,C NA-","101Y",-182.69,"kN",23.34,"kN",0.32,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Atras,C NA+","101S",114.24,"kN",17.28,"kN",0.48,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Atras,C NA+","101X",-153.81,"kN",22.44,"kN",0.47,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Atras,C NA+","101XY",57.73,"kN",15.6,"kN",0.55000000000000004,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Atras,C NA+","101Y",289.37,"kN",41.28,"kN",0.57999999999999996,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Atras,C NA-","101S",-144.21,"kN",24.07,"kN",0.49,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Atras,C NA-","101X",104.73,"kN",20.71,"kN",0.45,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Atras,C NA-","101XY",312.47000000000003,"kN",39.93,"kN",0.39,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Atras,C NA-","101Y",34.549999999999997,"kN",8.48,"kN",0.37,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Del,C NA+","101S",289.69,"kN",41.32,"kN",0.57999999999999996,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Del,C NA+","101X",57.95,"kN",15.62,"kN",0.55000000000000004,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Del,C NA+","101XY",-154.16,"kN",22.48,"kN",0.48,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Del,C NA+","101Y",114.02,"kN",17.27,"kN",0.48,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Del,C NA-","101S",34.32,"kN",8.4700000000000006,"kN",0.37,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Del,C NA-","101X",312.08999999999997,"kN",39.89,"kN",0.39,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Del,C NA-","101XY",104.95,"kN",20.73,"kN",0.44,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Del,C NA-","101Y",-143.85,"kN",24.04,"kN",0.49,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Atras,C NA+","101S",97.98,"kN",19.760000000000002,"kN",0.47,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Atras,C NA+","101X",-137.01,"kN",23.59,"kN",0.46,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Atras,C NA+","101XY",41.33,"kN",8.69,"kN",0.4,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Atras,C NA+","101Y",305.24,"kN",38.86,"kN",0.37,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Atras,C NA-","101S",-161.24,"kN",23.11,"kN",0.45,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Atras,C NA-","101X",120.97,"kN",18.07,"kN",0.5,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Atras,C NA-","101XY",296.62,"kN",42.44,"kN",0.56000000000000005,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Atras,C NA-","101Y",51.18,"kN",15.36,"kN",0.56999999999999995,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Del,C NA+","101S",305.32,"kN",38.869999999999997,"kN",0.37,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Del,C NA+","101X",41.79,"kN",8.7200000000000006,"kN",0.4,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Del,C NA+","101XY",-137.11000000000001,"kN",23.6,"kN",0.46,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Del,C NA+","101Y",97.51,"kN",19.72,"kN",0.47,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Del,C NA-","101S",50.72,"kN",15.37,"kN",0.56999999999999995,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Del,C NA-","101X",296.48,"kN",42.44,"kN",0.56000000000000005,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Del,C NA-","101XY",121.45,"kN",18.13,"kN",0.5,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Del,C NA-","101Y",-161.13999999999999,"kN",23.11,"kN",0.45,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Atras,C NA+","101S",135.54,"kN",17.37,"kN",0.35,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Atras,C NA+","101X",-129.08000000000001,"kN",20.95,"kN",0.48,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Atras,C NA+","101XY",32.86,"kN",15.28,"kN",0.55000000000000004,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Atras,C NA+","101Y",268.16000000000003,"kN",38.869999999999997,"kN",0.46,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Atras,C NA-","101S",-122.43,"kN",21.34,"kN",0.38,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Atras,C NA-","101X",128.75,"kN",21.98,"kN",0.45,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Atras,C NA-","101XY",288.24,"kN",38.32,"kN",0.4,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Atras,C NA-","101Y",12.93,"kN",5.4,"kN",0.25,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Del,C NA+","101S",268.29000000000002,"kN",38.869999999999997,"kN",0.46,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Del,C NA+","101X",33.270000000000003,"kN",15.27,"kN",0.55000000000000004,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Del,C NA+","101XY",-129.22,"kN",20.97,"kN",0.48,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Del,C NA+","101Y",135.11000000000001,"kN",17.309999999999999,"kN",0.35,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Del,C NA-","101S",12.51,"kN",5.36,"kN",0.25,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Del,C NA-","101X",288.06,"kN",38.299999999999997,"kN",0.4,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Del,C NA-","101XY",129.18,"kN",22.01,"kN",0.45,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Del,C NA-","101Y",-122.29,"kN",21.32,"kN",0.38,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Atras,C NA+","101S",122.13,"kN",21.07,"kN",0.48,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Atras,C NA+","101X",-115.34,"kN",20.89,"kN",0.36,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Atras,C NA+","101XY",19.53,"kN",5.61,"kN",0.28000000000000003,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Atras,C NA+","101Y",281.16000000000003,"kN",37.29,"kN",0.38,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Atras,C NA-","101S",-136.37,"kN",21.63,"kN",0.46,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Atras,C NA-","101X",142.16,"kN",18.28,"kN",0.38,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Atras,C NA-","101XY",275.24,"kN",40.020000000000003,"kN",0.44,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Atras,C NA-","101Y",26.46,"kN",15.15,"kN",0.56999999999999995,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Del,C NA+","101S",281.27,"kN",37.299999999999997,"kN",0.38,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Del,C NA+","101X",19.97,"kN",5.64,"kN",0.28000000000000003,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Del,C NA+","101XY",-115.45,"kN",20.9,"kN",0.36,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Del,C NA+","101Y",121.68,"kN",21.02,"kN",0.48,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Del,C NA-","101S",26.01,"kN",15.18,"kN",0.57999999999999996,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Del,C NA-","101X",275.08,"kN",40.020000000000003,"kN",0.44,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Del,C NA-","101XY",142.62,"kN",18.34,"kN",0.38,"kN-m",0]
["T-3","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Del,C NA-","101Y",-136.26,"kN",21.63,"kN",0.46,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Viento,C NA+","91S",1464.33,"kN",229.51,"kN",1.66,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Viento,C NA+","91X",-1252.02,"kN",201.51,"kN",1.54,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Viento,C NA+","91XY",-1259.73,"kN",202.48,"kN",1.53,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Viento,C NA+","91Y",1456.61,"kN",228.52,"kN",1.65,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Viento,C NA-","91S",628.9,"kN",89.14,"kN",0.69,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Viento,C NA-","91X",-391.85,"kN",52.7,"kN",0.54,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Viento,C NA-","91XY",-424.3,"kN",57.45,"kN",0.56000000000000005,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Viento,C NA-","91Y",596.44000000000005,"kN",84.4,"kN",0.68,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Hielo,C NA+","91S",1073.25,"kN",163.16999999999999,"kN",0.54,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Hielo,C NA+","91X",-834.86,"kN",129.07,"kN",0.57999999999999996,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Hielo,C NA+","91XY",-839.35,"kN",129.56,"kN",0.59,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Hielo,C NA+","91Y",1068.77,"kN",162.69,"kN",0.54,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Viento+Hielo,C NA-","91S",989.86,"kN",149.25,"kN",0.35,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Viento+Hielo,C NA-","91X",-738.62,"kN",112.79,"kN",0.42,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Viento+Hielo,C NA-","91XY",-755.96,"kN",115.19,"kN",0.43,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Viento+Hielo,C NA-","91Y",972.52,"kN",146.85,"kN",0.34,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Viento+Hielo,C NA+","91S",1214.54,"kN",185.79,"kN",0.77,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Viento+Hielo,C NA+","91X",-971.62,"kN",151.47,"kN",0.77,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Viento+Hielo,C NA+","91XY",-980.65,"kN",152.63,"kN",0.78,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Viento+Hielo,C NA+","91Y",1205.52,"kN",184.64,"kN",0.76,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Tiro Vertical,C NA+","91S",710.04,"kN",108,"kN",0.42,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Tiro Vertical,C NA+","91X",-597.17999999999995,"kN",92.47,"kN",0.41,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Tiro Vertical,C NA+","91XY",-505.35,"kN",78.5,"kN",0.43,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Tiro Vertical,C NA+","91Y",801.8,"kN",121.96,"kN",0.34,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Desequilibrio Amar Atras,C NA+","91S",673.07,"kN",104.06,"kN",0.92,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Desequilibrio Amar Atras,C NA+","91X",-1267.92,"kN",196.21,"kN",0.56999999999999995,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Desequilibrio Amar Atras,C NA+","91XY",-439.62,"kN",71.5,"kN",0.9,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Desequilibrio Amar Atras,C NA+","91Y",1501.33,"kN",229.41,"kN",0.5,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Desequilibrio Amar Atras,C NA-","91S",448.3,"kN",67.47,"kN",0.53,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Desequilibrio Amar Atras,C NA-","91X",-1034.77,"kN",157.68,"kN",0.18,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Desequilibrio Amar Atras,C NA-","91XY",-214.85,"kN",34.340000000000003,"kN",0.57999999999999996,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Desequilibrio Amar Atras,C NA-","91Y",1268.17,"kN",191.72,"kN",0.08,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Desequilibrio Amar Del,C NA+","91S",1509.74,"kN",230.48,"kN",0.5,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Desequilibrio Amar Del,C NA+","91X",-432.14,"kN",70.55,"kN",0.89,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Desequilibrio Amar Del,C NA+","91XY",-1275.19,"kN",197.12,"kN",0.56999999999999995,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Desequilibrio Amar Del,C NA+","91Y",666.75,"kN",103.28,"kN",0.91,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Desequilibrio Amar Del,C NA-","91S",1284.98,"kN",194.06,"kN",0.06,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Desequilibrio Amar Del,C NA-","91X",-199.09,"kN",32.25,"kN",0.56000000000000005,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Desequilibrio Amar Del,C NA-","91XY",-1050.43,"kN",159.85,"kN",0.18,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Desequilibrio Amar Del,C NA-","91Y",433.7,"kN",65.47,"kN",0.52,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CT1 Atras,C NA+","91S",1110.31,"kN",171.97,"kN",0.47,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CT1 Atras,C NA+","91X",-1024.8599999999999,"kN",157.78,"kN",0.27,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CT1 Atras,C NA+","91XY",-877.92,"kN",140.32,"kN",1.45,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CT1 Atras,C NA+","91Y",1257.78,"kN",192.06,"kN",1.62,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CT1 Atras,C NA-","91S",889.72,"kN",136.11000000000001,"kN",0.55000000000000004,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CT1 Atras,C NA-","91X",-799.42,"kN",120.21,"kN",0.17,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CT1 Atras,C NA-","91XY",-657.34,"kN",103.34,"kN",1.0900000000000001,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CT1 Atras,C NA-","91Y",1032.3499999999999,"kN",155.19,"kN",1.25,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CT1 Del,C NA+","91S",1265.48,"kN",193.03,"kN",1.6,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CT1 Del,C NA+","91X",-871.9,"kN",139.54,"kN",1.42,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CT1 Del,C NA+","91XY",-1032.23,"kN",158.75,"kN",0.28000000000000003,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CT1 Del,C NA+","91Y",1104.6500000000001,"kN",171.29,"kN",0.49,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CT1 Del,C NA-","91S",1047.1500000000001,"kN",157.25,"kN",1.23,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CT1 Del,C NA-","91X",-642.34,"kN",101.24,"kN",1.06,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CT1 Del,C NA-","91XY",-813.89,"kN",122.27,"kN",0.14000000000000001,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CT1 Del,C NA-","91Y",875.08,"kN",134.07,"kN",0.54,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CT2 Atras,C NA+","91S",1109.1099999999999,"kN",173.07,"kN",1.45,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CT2 Atras,C NA+","91X",-1023.85,"kN",159.22,"kN",1.62,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CT2 Atras,C NA+","91XY",-876.19,"kN",138.81,"kN",0.59,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CT2 Atras,C NA+","91Y",1256.25,"kN",190.83,"kN",0.23,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CT2 Atras,C NA-","91S",888.54,"kN",136.99,"kN",1.02,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CT2 Atras,C NA-","91X",-798.3,"kN",121.44,"kN",1.32,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CT2 Atras,C NA-","91XY",-655.61,"kN",102.11,"kN",0.52,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CT2 Atras,C NA-","91Y",1030.7,"kN",154.09,"kN",0.24,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CT2 Del,C NA+","91S",1264.6300000000001,"kN",191.89,"kN",0.24,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CT2 Del,C NA+","91X",-870.92,"kN",138.13,"kN",0.6,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CT2 Del,C NA+","91XY",-1031.8800000000001,"kN",160.19,"kN",1.6,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CT2 Del,C NA+","91Y",1104.19,"kN",172.4,"kN",1.42,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CT2 Del,C NA-","91S",1046.18,"kN",156.25,"kN",0.23,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CT2 Del,C NA-","91X",-641.37,"kN",100.08,"kN",0.52,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CT2 Del,C NA-","91XY",-813.43,"kN",123.49,"kN",1.31,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CT2 Del,C NA-","91Y",874.64,"kN",135,"kN",0.99,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CS 1  Amar Atras,C NA+","91S",1074.3,"kN",166.15,"kN",0.79,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CS 1  Amar Atras,C NA+","91X",-1047.6300000000001,"kN",161.21,"kN",0.56000000000000005,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CS 1  Amar Atras,C NA+","91XY",-840.94,"kN",135.66999999999999,"kN",2.02,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CS 1  Amar Atras,C NA+","91Y",1281.81,"kN",196.53,"kN",2.17,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CS 1 Amar Atras,C NA-","91S",849.59,"kN",129.94,"kN",1.06,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CS 1 Amar Atras,C NA-","91X",-814.59,"kN",122.91,"kN",0.78,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CS 1 Amar Atras,C NA-","91XY",-616.23,"kN",98.24,"kN",1.69,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CS 1 Amar Atras,C NA-","91Y",1048.76,"kN",158.68,"kN",1.79,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CS 1  Amar Del,C NA+","91S",1290.57,"kN",197.65,"kN",2.1800000000000002,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CS 1  Amar Del,C NA+","91X",-831.63,"kN",134.5,"kN",2.0099999999999998,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CS 1  Amar Del,C NA+","91XY",-1056.18,"kN",162.30000000000001,"kN",0.53,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CS 1  Amar Del,C NA+","91Y",1065.22,"kN",165.02,"kN",0.81,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CS 1 Amar Del,C NA-","91S",1065.8599999999999,"kN",161.04,"kN",1.8,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CS 1 Amar Del,C NA-","91X",-598.61,"kN",95.86,"kN",1.68,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CS 1 Amar Del,C NA-","91XY",-831.46,"kN",125.26,"kN",0.76,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CS 1 Amar Del,C NA-","91Y",832.21,"kN",127.55,"kN",1.07,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CS 2 Amar Atras,C NA+","91S",1074.8699999999999,"kN",168.4,"kN",2.0299999999999998,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CS 2 Amar Atras,C NA+","91X",-1048.77,"kN",163.82,"kN",2.16,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CS 2 Amar Atras,C NA+","91XY",-840.71,"kN",132.9,"kN",0.88,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CS 2 Amar Atras,C NA+","91Y",1282.1400000000001,"kN",194.61,"kN",0.5,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CS 2 Amar Atras,C NA-","91S",850.16,"kN",131.81,"kN",1.61,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CS 2 Amar Atras,C NA-","91X",-815.73,"kN",125.1,"kN",1.86,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CS 2 Amar Atras,C NA-","91XY",-616,"kN",95.95,"kN",1.01,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CS 2 Amar Atras,C NA-","91Y",1049.0899999999999,"kN",157.09,"kN",0.85,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CS 2 Amar Del,C NA+","91S",1291.48,"kN",195.78,"kN",0.48,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CS 2 Amar Del,C NA+","91X",-832.02,"kN",131.79,"kN",0.9,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CS 2 Amar Del,C NA+","91XY",-1057.8900000000001,"kN",164.97,"kN",2.17,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CS 2 Amar Del,C NA+","91Y",1066.42,"kN",167.32,"kN",2.0099999999999998,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CS 2 Amar Del,C NA-","91S",1066.77,"kN",159.52000000000001,"kN",0.85,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CS 2 Amar Del,C NA-","91X",-599,"kN",93.59,"kN",1.03,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CS 2 Amar Del,C NA-","91XY",-833.18,"kN",127.47,"kN",1.87,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CS 2 Amar Del,C NA-","91Y",833.4,"kN",129.5,"kN",1.6,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CM 1 Amar Atras,C NA+","91S",1104.76,"kN",168.32,"kN",0.88,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CM 1 Amar Atras,C NA+","91X",-1030.1300000000001,"kN",160.02000000000001,"kN",1.1000000000000001,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CM 1 Amar Atras,C NA+","91XY",-872.34,"kN",138.76,"kN",2.4,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CM 1 Amar Atras,C NA+","91Y",1265.32,"kN",195.51,"kN",2.27,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CM 1 Amar Atras,C NA-","91S",880.05,"kN",132.18,"kN",1.23,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CM 1 Amar Atras,C NA-","91X",-797.09,"kN",121.99,"kN",1.31,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CM 1 Amar Atras,C NA-","91XY",-647.64,"kN",101.43,"kN",2.09,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CM 1 Amar Atras,C NA-","91Y",1032.28,"kN",157.66999999999999,"kN",1.88,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CM 1 Amar Del,C NA+","91S",1274.03,"kN",196.63,"kN",2.2799999999999998,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CM 1 Amar Del,C NA+","91X",-862.94,"kN",137.58000000000001,"kN",2.38,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CM 1 Amar Del,C NA+","91XY",-1038.6099999999999,"kN",161.1,"kN",1.07,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CM 1 Amar Del,C NA+","91Y",1095.5899999999999,"kN",167.18,"kN",0.89,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CM 1 Amar Del,C NA-","91S",1049.33,"kN",160.02000000000001,"kN",1.89,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CM 1 Amar Del,C NA-","91X",-629.92999999999995,"kN",99.06,"kN",2.08,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CM 1 Amar Del,C NA-","91XY",-813.91,"kN",124.32,"kN",1.29,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CM 1 Amar Del,C NA-","91Y",862.58,"kN",129.78,"kN",1.24,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CM 2 Amar Atras,C NA+","91S",1106.4100000000001,"kN",171.35,"kN",2.42,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CM 2 Amar Atras,C NA+","91X",-1032.3599999999999,"kN",162.87,"kN",2.27,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CM 2 Amar Atras,C NA+","91XY",-871.22,"kN",135.08000000000001,"kN",0.93,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CM 2 Amar Atras,C NA+","91Y",1264.77,"kN",193.47,"kN",1.04,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CM 2 Amar Atras,C NA-","91S",881.7,"kN",134.81,"kN",2.0299999999999998,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CM 2 Amar Atras,C NA-","91X",-799.32,"kN",124.16,"kN",1.96,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CM 2 Amar Atras,C NA-","91XY",-646.52,"kN",98.24,"kN",1.1599999999999999,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CM 2 Amar Atras,C NA-","91Y",1031.74,"kN",156.12,"kN",1.38,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CM 2 Amar Del,C NA+","91S",1274.22,"kN",194.65,"kN",1.02,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CM 2 Amar Del,C NA+","91X",-862.55,"kN",133.97,"kN",0.96,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CM 2 Amar Del,C NA+","91XY",-1041.57,"kN",164.02,"kN",2.2799999999999998,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CM 2 Amar Del,C NA+","91Y",1097.98,"kN",170.27,"kN",2.4,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CM 2 Amar Del,C NA-","91S",1049.51,"kN",158.56,"kN",1.37,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CM 2 Amar Del,C NA-","91X",-629.54,"kN",95.89,"kN",1.18,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CM 2 Amar Del,C NA-","91XY",-816.87,"kN",126.54,"kN",1.97,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CM 2 Amar Del,C NA-","91Y",864.97,"kN",132.52000000000001,"kN",2.02,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CI 1 Amar Atras,C NA+","91S",1131.69,"kN",169.89,"kN",0.55000000000000004,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CI 1 Amar Atras,C NA+","91X",-1009.21,"kN",158.24,"kN",1.19,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CI 1 Amar Atras,C NA+","91XY",-907.43,"kN",141.34,"kN",2.3199999999999998,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CI 1 Amar Atras,C NA+","91Y",1252.6199999999999,"kN",194.38,"kN",1.9,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CI 1 Amar Atras,C NA-","91S",906.99,"kN",133.63999999999999,"kN",0.97,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CI 1 Amar Atras,C NA-","91X",-776.18,"kN",120.23,"kN",1.38,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CI 1 Amar Atras,C NA-","91XY",-682.73,"kN",103.97,"kN",2.0499999999999998,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CI 1 Amar Atras,C NA-","91Y",1019.59,"kN",156.53,"kN",1.49,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CI 1 Amar Del,C NA+","91S",1261.4000000000001,"kN",195.51,"kN",1.91,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CI 1 Amar Del,C NA+","91X",-898.03,"kN",140.16,"kN",2.2999999999999998,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CI 1 Amar Del,C NA+","91XY",-1017.77,"kN",159.32,"kN",1.1599999999999999,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CI 1 Amar Del,C NA+","91Y",1122.56,"kN",168.75,"kN",0.56000000000000005,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CI 1 Amar Del,C NA-","91S",1036.7,"kN",158.9,"kN",1.49,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CI 1 Amar Del,C NA-","91X",-665.02,"kN",101.59,"kN",2.0299999999999998,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CI 1 Amar Del,C NA-","91XY",-793.07,"kN",122.56,"kN",1.35,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CI 1 Amar Del,C NA-","91Y",889.55,"kN",131.24,"kN",0.97,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CI 2 Amar Atras,C NA+","91S",1141.47,"kN",173.99,"kN",2.35,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CI 2 Amar Atras,C NA+","91X",-1019.37,"kN",161.6,"kN",1.9,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CI 2 Amar Atras,C NA+","91XY",-898.04,"kN",136.63999999999999,"kN",0.57999999999999996,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CI 2 Amar Atras,C NA+","91Y",1243.6099999999999,"kN",191.66,"kN",1.1299999999999999,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CI 2 Amar Atras,C NA-","91S",916.77,"kN",137.43,"kN",1.99,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CI 2 Amar Atras,C NA-","91X",-786.34,"kN",122.85,"kN",1.57,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CI 2 Amar Atras,C NA-","91XY",-673.34,"kN",99.62,"kN",0.88,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CI 2 Amar Atras,C NA-","91Y",1010.59,"kN",154.33000000000001,"kN",1.43,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CI 2 Amar Del,C NA+","91S",1253.03,"kN",192.84,"kN",1.1100000000000001,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CI 2 Amar Del,C NA+","91X",-889.28,"kN",135.52000000000001,"kN",0.6,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CI 2 Amar Del,C NA+","91XY",-1028.54,"kN",162.75,"kN",1.91,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CI 2 Amar Del,C NA+","91Y",1132.96,"kN",172.9,"kN",2.33,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CI 2 Amar Del,C NA-","91S",1028.33,"kN",156.76,"kN",1.42,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CI 2 Amar Del,C NA-","91X",-656.28,"kN",97.26,"kN",0.89,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CI 2 Amar Del,C NA-","91XY",-803.84,"kN",125.24,"kN",1.58,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CI 2 Amar Del,C NA-","91Y",899.95,"kN",135.12,"kN",1.98,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CS Amar Atras (A4),C NA+","91S",1214.54,"kN",185.79,"kN",0.77,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CS Amar Atras (A4),C NA+","91X",-971.62,"kN",151.47,"kN",0.77,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CS Amar Atras (A4),C NA+","91XY",-980.65,"kN",152.63,"kN",0.78,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CS Amar Atras (A4),C NA+","91Y",1205.52,"kN",184.64,"kN",0.76,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CS Amar Atras (A4),C NA-","91S",989.86,"kN",149.25,"kN",0.35,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CS Amar Atras (A4),C NA-","91X",-738.62,"kN",112.79,"kN",0.42,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CS Amar Atras (A4),C NA-","91XY",-755.96,"kN",115.19,"kN",0.43,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CS Amar Atras (A4),C NA-","91Y",972.52,"kN",146.85,"kN",0.34,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CS Amar Del (A4),C NA+","91S",1214.54,"kN",185.79,"kN",0.77,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CS Amar Del (A4),C NA+","91X",-971.62,"kN",151.47,"kN",0.77,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CS Amar Del (A4),C NA+","91XY",-980.65,"kN",152.63,"kN",0.78,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CS Amar Del (A4),C NA+","91Y",1205.52,"kN",184.64,"kN",0.76,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CS Amar Del (A4),C NA-","91S",989.86,"kN",149.25,"kN",0.35,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CS Amar Del (A4),C NA-","91X",-738.62,"kN",112.79,"kN",0.42,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CS Amar Del (A4),C NA-","91XY",-755.96,"kN",115.19,"kN",0.43,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CS Amar Del (A4),C NA-","91Y",972.52,"kN",146.85,"kN",0.34,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CM Amar Atras (A4),C NA+","91S",1214.54,"kN",185.79,"kN",0.77,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CM Amar Atras (A4),C NA+","91X",-971.62,"kN",151.47,"kN",0.77,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CM Amar Atras (A4),C NA+","91XY",-980.65,"kN",152.63,"kN",0.78,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CM Amar Atras (A4),C NA+","91Y",1205.52,"kN",184.64,"kN",0.76,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CM Amar Atras (A4),C NA-","91S",989.86,"kN",149.25,"kN",0.35,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CM Amar Atras (A4),C NA-","91X",-738.62,"kN",112.79,"kN",0.42,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CM Amar Atras (A4),C NA-","91XY",-755.96,"kN",115.19,"kN",0.43,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CM Amar Atras (A4),C NA-","91Y",972.52,"kN",146.85,"kN",0.34,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CM Amar Del (A4),C NA+","91S",1214.54,"kN",185.79,"kN",0.77,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CM Amar Del (A4),C NA+","91X",-971.62,"kN",151.47,"kN",0.77,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CM Amar Del (A4),C NA+","91XY",-980.65,"kN",152.63,"kN",0.78,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CM Amar Del (A4),C NA+","91Y",1205.52,"kN",184.64,"kN",0.76,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CM Amar Del (A4),C NA-","91S",989.86,"kN",149.25,"kN",0.35,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CM Amar Del (A4),C NA-","91X",-738.62,"kN",112.79,"kN",0.42,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CM Amar Del (A4),C NA-","91XY",-755.96,"kN",115.19,"kN",0.43,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CM Amar Del (A4),C NA-","91Y",972.52,"kN",146.85,"kN",0.34,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CI Amar Atras (A4),C NA+","91S",1214.54,"kN",185.79,"kN",0.77,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CI Amar Atras (A4),C NA+","91X",-971.62,"kN",151.47,"kN",0.77,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CI Amar Atras (A4),C NA+","91XY",-980.65,"kN",152.63,"kN",0.78,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CI Amar Atras (A4),C NA+","91Y",1205.52,"kN",184.64,"kN",0.76,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CI Amar Atras (A4),C NA-","91S",989.86,"kN",149.25,"kN",0.35,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CI Amar Atras (A4),C NA-","91X",-738.62,"kN",112.79,"kN",0.42,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CI Amar Atras (A4),C NA-","91XY",-755.96,"kN",115.19,"kN",0.43,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CI Amar Atras (A4),C NA-","91Y",972.52,"kN",146.85,"kN",0.34,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CI Amar Del (A4),C NA+","91S",1214.54,"kN",185.79,"kN",0.77,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CI Amar Del (A4),C NA+","91X",-971.62,"kN",151.47,"kN",0.77,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CI Amar Del (A4),C NA+","91XY",-980.65,"kN",152.63,"kN",0.78,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","Rotura CI Amar Del (A4),C NA+","91Y",1205.52,"kN",184.64,"kN",0.76,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CI Amar Del (A4),C NA-","91S",989.86,"kN",149.25,"kN",0.35,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CI Amar Del (A4),C NA-","91X",-738.62,"kN",112.79,"kN",0.42,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CI Amar Del (A4),C NA-","91XY",-755.96,"kN",115.19,"kN",0.43,"kN-m",0]
["T-4","d4a3-aa-vidrio_ed.g_v4.tow","-Rotura CI Amar Del (A4),C NA-","91Y",972.52,"kN",146.85,"kN",0.34,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Viento,C NA+","101S",456.21,"kN",63.65,"kN",0.3,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Viento,C NA+","101X",-317.68,"kN",48.69,"kN",0.27,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Viento,C NA+","101XY",-320.57,"kN",48.99,"kN",0.26,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Viento,C NA+","101Y",453.51,"kN",63.29,"kN",0.28999999999999998,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Viento,C NA-","101S",-324.18,"kN",48.17,"kN",0.34,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Viento,C NA-","101X",464.44,"kN",66.23,"kN",0.23,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Viento,C NA-","101XY",460.09,"kN",65.650000000000006,"kN",0.22,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Viento,C NA-","101Y",-328.87,"kN",48.67,"kN",0.33,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Hielo,C NA+","101S",79.08,"kN",9.52,"kN",0.01,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Hielo,C NA+","101X",86.86,"kN",10.53,"kN",0.01,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Hielo,C NA+","101XY",86.85,"kN",10.53,"kN",0.01,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Hielo,C NA+","101Y",79.08,"kN",9.52,"kN",0.01,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Viento+Hielo,C NA-","101S",-31.58,"kN",6.08,"kN",7.0000000000000007E-2,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Viento+Hielo,C NA-","101X",198.74,"kN",26.31,"kN",0.04,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Viento+Hielo,C NA-","101XY",198.04,"kN",26.22,"kN",0.04,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Viento+Hielo,C NA-","101Y",-32.29,"kN",6.16,"kN",7.0000000000000007E-2,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Viento+Hielo,C NA+","101S",190.49,"kN",24.97,"kN",0.05,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Viento+Hielo,C NA+","101X",-23.91,"kN",5.39,"kN",0.06,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Viento+Hielo,C NA+","101XY",-24.04,"kN",5.41,"kN",0.06,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Viento+Hielo,C NA+","101Y",190.36,"kN",24.96,"kN",0.05,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Tiro Vertical,C NA+","101S",62.25,"kN",7.54,"kN",0.01,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Tiro Vertical,C NA+","101X",67.489999999999995,"kN",8.24,"kN",0.01,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Tiro Vertical,C NA+","101XY",67.48,"kN",8.24,"kN",0.01,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Tiro Vertical,C NA+","101Y",62.24,"kN",7.54,"kN",0.01,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Atras,C NA+","101S",-185.28,"kN",21.44,"kN",0.2,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Atras,C NA+","101X",-408.41,"kN",51.54,"kN",0.09,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Atras,C NA+","101XY",357.29,"kN",41.75,"kN",0.2,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Atras,C NA+","101Y",568.54999999999995,"kN",71.47,"kN",0.27,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Atras,C NA-","101S",-416.51,"kN",52.34,"kN",0.09,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Atras,C NA-","101X",-176.61,"kN",20.11,"kN",0.23,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Atras,C NA-","101XY",576.11,"kN",72.760000000000005,"kN",0.26,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Atras,C NA-","101Y",349.17,"kN",40.950000000000003,"kN",0.23,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Del,C NA+","101S",567.86,"kN",71.41,"kN",0.27,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Del,C NA+","101X",355.46,"kN",41.54,"kN",0.2,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Del,C NA+","101XY",-410.39,"kN",51.79,"kN",0.1,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Del,C NA+","101Y",-185.87,"kN",21.51,"kN",0.2,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Del,C NA-","101S",348.99,"kN",40.950000000000003,"kN",0.23,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Del,C NA-","101X",574.91,"kN",72.62,"kN",0.26,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Del,C NA-","101XY",-178.93,"kN",20.41,"kN",0.23,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Del,C NA-","101Y",-417.91,"kN",52.5,"kN",0.09,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Atras,C NA+","101S",86.71,"kN",13.91,"kN",0.32,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Atras,C NA+","101X",-133.97,"kN",16.739999999999998,"kN",0.16,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Atras,C NA+","101XY",87.95,"kN",9.82,"kN",0.26,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Atras,C NA+","101Y",289.98,"kN",37.770000000000003,"kN",0.4,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Atras,C NA-","101S",-130.25,"kN",19.809999999999999,"kN",0.4,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Atras,C NA-","101X",84,"kN",16.149999999999999,"kN",0.24,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Atras,C NA-","101XY",304.14,"kN",37.26,"kN",0.16,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Atras,C NA-","101Y",72.78,"kN",8.42,"kN",0.3,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Del,C NA+","101S",289.81,"kN",37.72,"kN",0.4,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Del,C NA+","101X",87.56,"kN",9.7899999999999991,"kN",0.26,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Del,C NA+","101XY",-134.55000000000001,"kN",16.78,"kN",0.16,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Del,C NA+","101Y",86.33,"kN",13.85,"kN",0.32,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Del,C NA-","101S",74.31,"kN",8.5,"kN",0.3,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Del,C NA-","101X",303.14999999999998,"kN",37.19,"kN",0.16,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Del,C NA-","101XY",81.7,"kN",15.97,"kN",0.25,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Del,C NA-","101Y",-130.02000000000001,"kN",19.84,"kN",0.4,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Atras,C NA+","101S",76.08,"kN",14.9,"kN",0.26,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Atras,C NA+","101X",-122.37,"kN",19.16,"kN",0.37,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Atras,C NA+","101XY",80.760000000000005,"kN",8.98,"kN",0.33,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Atras,C NA+","101Y",296.22000000000003,"kN",36.01,"kN",0.14000000000000001,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Atras,C NA-","101S",-141.44,"kN",17.489999999999998,"kN",0.14000000000000001,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Atras,C NA-","101X",95.29,"kN",15.05,"kN",0.34,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Atras,C NA-","101XY",297.39,"kN",39.01,"kN",0.37,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Atras,C NA-","101Y",79.45,"kN",9.17,"kN",0.28000000000000003,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Del,C NA+","101S",295,"kN",35.909999999999997,"kN",0.14000000000000001,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Del,C NA+","101X",81.41,"kN",8.99,"kN",0.33,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Del,C NA+","101XY",-121.91,"kN",19.16,"kN",0.37,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Del,C NA+","101Y",74.680000000000007,"kN",14.81,"kN",0.26,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Del,C NA-","101S",79.930000000000007,"kN",9.2100000000000009,"kN",0.28000000000000003,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Del,C NA-","101X",297.47000000000003,"kN",38.99,"kN",0.37,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Del,C NA-","101XY",94.04,"kN",14.89,"kN",0.34,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Del,C NA-","101Y",-142.28,"kN",17.559999999999999,"kN",0.14000000000000001,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Atras,C NA+","101S",78.83,"kN",14.43,"kN",0.46,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Atras,C NA+","101X",-152.08000000000001,"kN",19.84,"kN",0.33,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Atras,C NA+","101XY",102.35,"kN",14.03,"kN",0.41,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Atras,C NA+","101Y",303.69,"kN",41.03,"kN",0.55000000000000004,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Atras,C NA-","101S",-145.63,"kN",22.58,"kN",0.47,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Atras,C NA-","101X",73.47,"kN",16.260000000000002,"kN",0.32,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Atras,C NA-","101XY",323.52,"kN",39.68,"kN",0.26,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Atras,C NA-","101Y",81.430000000000007,"kN",10.93,"kN",0.38,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Del,C NA+","101S",304.27,"kN",41.06,"kN",0.55000000000000004,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Del,C NA+","101X",101.3,"kN",13.98,"kN",0.41,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Del,C NA+","101XY",-153.37,"kN",19.96,"kN",0.33,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Del,C NA+","101Y",79.25,"kN",14.47,"kN",0.46,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Del,C NA-","101S",82.55,"kN",10.98,"kN",0.38,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Del,C NA-","101X",323.08999999999997,"kN",39.659999999999997,"kN",0.26,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Del,C NA-","101XY",71.7,"kN",16.13,"kN",0.32,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Del,C NA-","101Y",-145.87,"kN",22.65,"kN",0.47,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Atras,C NA+","101S",65.13,"kN",15.13,"kN",0.35,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Atras,C NA+","101X",-137.88,"kN",22.03,"kN",0.45,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Atras,C NA+","101XY",89.7,"kN",11.58,"kN",0.41,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Atras,C NA+","101Y",315.83999999999997,"kN",38.479999999999997,"kN",0.24,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Atras,C NA-","101S",-159.93,"kN",20.62,"kN",0.31,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Atras,C NA-","101X",87.23,"kN",15.35,"kN",0.49,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Atras,C NA-","101XY",311.31,"kN",42.31,"kN",0.53,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Atras,C NA-","101Y",94.18,"kN",13.53,"kN",0.44,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Del,C NA+","101S",315.20999999999998,"kN",38.44,"kN",0.24,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Del,C NA+","101X",89.87,"kN",11.52,"kN",0.4,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Del,C NA+","101XY",-137.96,"kN",22.06,"kN",0.45,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Del,C NA+","101Y",64.33,"kN",15.08,"kN",0.35,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Del,C NA-","101S",94.09,"kN",13.53,"kN",0.44,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Del,C NA-","101X",312.08,"kN",42.36,"kN",0.53,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Del,C NA-","101XY",86.67,"kN",15.28,"kN",0.49,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Del,C NA-","101Y",-161.38999999999999,"kN",20.76,"kN",0.31,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Atras,C NA+","101S",103.49,"kN",16.059999999999999,"kN",0.47,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Atras,C NA+","101X",-130.6,"kN",19.88,"kN",0.47,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Atras,C NA+","101XY",80.69,"kN",16.04,"kN",0.54,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Atras,C NA+","101Y",279.14999999999998,"kN",39.71,"kN",0.56000000000000005,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Atras,C NA-","101S",-120.78,"kN",21.55,"kN",0.49,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Atras,C NA-","101X",94.82,"kN",19.7,"kN",0.45,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Atras,C NA-","101XY",301.95,"kN",38.57,"kN",0.4,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Atras,C NA-","101Y",56.74,"kN",10.33,"kN",0.38,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Del,C NA+","101S",279.49,"kN",39.69,"kN",0.56000000000000005,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Del,C NA+","101X",79.900000000000006,"kN",16,"kN",0.54,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Del,C NA+","101XY",-131.62,"kN",19.96,"kN",0.47,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Del,C NA+","101Y",103.63,"kN",16.059999999999999,"kN",0.47,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Del,C NA-","101S",57.63,"kN",10.32,"kN",0.38,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Del,C NA-","101X",301.77999999999997,"kN",38.58,"kN",0.4,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Del,C NA-","101XY",93.3,"kN",19.61,"kN",0.45,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Del,C NA-","101Y",-121.3,"kN",21.64,"kN",0.49,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Atras,C NA+","101S",86.54,"kN",18.600000000000001,"kN",0.47,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Atras,C NA+","101X",-113.1,"kN",21,"kN",0.47,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Atras,C NA+","101XY",65.040000000000006,"kN",10.85,"kN",0.41,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Atras,C NA+","101Y",294.25,"kN",37.42,"kN",0.38,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Atras,C NA-","101S",-138.4,"kN",20.59,"kN",0.44,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Atras,C NA-","101X",111.84,"kN",16.98,"kN",0.49,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Atras,C NA-","101XY",286.76,"kN",40.96,"kN",0.54,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Atras,C NA-","101Y",72.510000000000005,"kN",15.65,"kN",0.56000000000000005,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Del,C NA+","101S",293.61,"kN",37.380000000000003,"kN",0.38,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Del,C NA+","101X",65.23,"kN",10.78,"kN",0.41,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Del,C NA+","101XY",-113.19,"kN",21.05,"kN",0.47,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Del,C NA+","101Y",85.73,"kN",18.559999999999999,"kN",0.47,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Del,C NA-","101S",72.42,"kN",15.63,"kN",0.56000000000000005,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Del,C NA-","101X",287.56,"kN",40.99,"kN",0.54,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Del,C NA-","101XY",111.27,"kN",16.899999999999999,"kN",0.5,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Del,C NA-","101Y",-139.86000000000001,"kN",20.72,"kN",0.44,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Atras,C NA+","101S",124.61,"kN",15.96,"kN",0.35,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Atras,C NA+","101X",-105.66,"kN",18.43,"kN",0.48,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Atras,C NA+","101XY",56.07,"kN",15.39,"kN",0.53,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Atras,C NA+","101Y",257.64,"kN",37.25,"kN",0.45,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Atras,C NA-","101S",-99.28,"kN",18.73,"kN",0.38,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Atras,C NA-","101X",119.17,"kN",20.94,"kN",0.45,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Atras,C NA-","101XY",277.87,"kN",36.979999999999997,"kN",0.41,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Atras,C NA-","101Y",34.89,"kN",7.2,"kN",0.26,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Del,C NA+","101S",258.14999999999998,"kN",37.28,"kN",0.45,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Del,C NA+","101X",55.14,"kN",15.37,"kN",0.53,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Del,C NA+","101XY",-106.85,"kN",18.55,"kN",0.48,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Del,C NA+","101Y",124.92,"kN",15.99,"kN",0.35,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Del,C NA-","101S",35.950000000000003,"kN",7.24,"kN",0.26,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Del,C NA-","101X",277.56,"kN",36.97,"kN",0.41,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Del,C NA-","101XY",117.47,"kN",20.82,"kN",0.45,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Del,C NA-","101Y",-99.62,"kN",18.8,"kN",0.39,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Atras,C NA+","101S",110.81,"kN",19.850000000000001,"kN",0.48,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Atras,C NA+","101X",-91.51,"kN",18.2,"kN",0.37,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Atras,C NA+","101XY",43.19,"kN",7.82,"kN",0.28999999999999998,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Atras,C NA+","101Y",270.16000000000003,"kN",35.86,"kN",0.39,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Atras,C NA-","101S",-113.54,"kN",19.18,"kN",0.46,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Atras,C NA-","101X",133.04,"kN",17.100000000000001,"kN",0.37,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Atras,C NA-","101XY",265.26,"kN",38.54,"kN",0.43,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Atras,C NA-","101Y",47.89,"kN",15.16,"kN",0.56000000000000005,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Del,C NA+","101S",269.58999999999997,"kN",35.83,"kN",0.39,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Del,C NA+","101X",43.34,"kN",7.74,"kN",0.28999999999999998,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Del,C NA+","101XY",-91.65,"kN",18.25,"kN",0.37,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Del,C NA+","101Y",110.05,"kN",19.82,"kN",0.48,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Del,C NA-","101S",47.86,"kN",15.14,"kN",0.56000000000000005,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Del,C NA-","101X",266.02,"kN",38.57,"kN",0.43,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Del,C NA-","101XY",132.41,"kN",16.989999999999998,"kN",0.38,"kN-m",0]
["T-5","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Del,C NA-","101Y",-114.95,"kN",19.3,"kN",0.46,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Viento,C NA+","83P",1540.64,"kN",273.16000000000003,"kN",5.99,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Viento,C NA+","83X",-1273.1300000000001,"kN",230.51,"kN",5.85,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Viento,C NA+","83XY",-1317.18,"kN",238.78,"kN",5.93,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Viento,C NA+","83Y",1496.4,"kN",264.83999999999997,"kN",5.94,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Viento,C NA-","83P",583.92999999999995,"kN",96.25,"kN",0.53,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Viento,C NA-","83X",-375.65,"kN",59.36,"kN",0.17,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Viento,C NA-","83XY",-360.29,"kN",57.59,"kN",0.34,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Viento,C NA-","83Y",598.75,"kN",97.92,"kN",0.39,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Hielo,C NA+","83P",1113.1500000000001,"kN",193.62,"kN",3.48,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Hielo,C NA+","83X",-800.58,"kN",141.52000000000001,"kN",3.14,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Hielo,C NA+","83XY",-851.54,"kN",150.94,"kN",3.11,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Hielo,C NA+","83Y",1061.33,"kN",183.81,"kN",3.27,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Viento+Hielo,C NA-","83P",999.39,"kN",172.98,"kN",2.91,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Viento+Hielo,C NA-","83X",-716.08,"kN",125.33,"kN",2.57,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Viento+Hielo,C NA-","83XY",-738.63,"kN",130.07,"kN",2.5499999999999998,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Viento+Hielo,C NA-","83Y",976.15,"kN",167.96,"kN",2.75,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Viento+Hielo,C NA+","83P",1262.22,"kN",220.3,"kN",4.0999999999999996,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Viento+Hielo,C NA+","83X",-958.98,"kN",170.08,"kN",3.78,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Viento+Hielo,C NA+","83XY",-1001.52,"kN",178.21,"kN",3.8,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Viento+Hielo,C NA+","83Y",1219.1099999999999,"kN",211.94,"kN",3.96,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Tiro Vertical,C NA+","83P",865.46,"kN",150.49,"kN",2.72,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Tiro Vertical,C NA+","83X",-401.89,"kN",73.12,"kN",2.36,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Tiro Vertical,C NA+","83XY",-631.64,"kN",111.92,"kN",2.19,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Tiro Vertical,C NA+","83Y",632.59,"kN",109.97,"kN",1.99,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Desequilibrio Amar Atras,C NA+","83P",778.33,"kN",136.58000000000001,"kN",2.48,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Desequilibrio Amar Atras,C NA+","83X",-1185.21,"kN",208.07,"kN",3.51,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Desequilibrio Amar Atras,C NA+","83XY",-517.95000000000005,"kN",98.08,"kN",4.28,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Desequilibrio Amar Atras,C NA+","83Y",1455.59,"kN",252.79,"kN",4.88,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Desequilibrio Amar Atras,C NA-","83P",515.46,"kN",89.23,"kN",1.29,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Desequilibrio Amar Atras,C NA-","83X",-942.21,"kN",163.63,"kN",2.58,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Desequilibrio Amar Atras,C NA-","83XY",-255.01,"kN",51.22,"kN",3.18,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Desequilibrio Amar Atras,C NA-","83Y",1212.54,"kN",208.83,"kN",3.67,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Desequilibrio Amar Del,C NA+","83P",1495.29,"kN",260.52,"kN",5.01,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Desequilibrio Amar Del,C NA+","83X",-482.79,"kN",92.04,"kN",4.49,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Desequilibrio Amar Del,C NA+","83XY",-1226.6500000000001,"kN",216.15,"kN",3.79,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Desequilibrio Amar Del,C NA+","83Y",740.49,"kN",129.32,"kN",2.35,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Desequilibrio Amar Del,C NA-","83P",1232.1400000000001,"kN",213.17,"kN",3.81,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Desequilibrio Amar Del,C NA-","83X",-239.73,"kN",48.96,"kN",3.49,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Desequilibrio Amar Del,C NA-","83XY",-963.44,"kN",168.3,"kN",2.92,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Desequilibrio Amar Del,C NA-","83Y",497.37,"kN",85.27,"kN",1.1399999999999999,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CT1 Atras,C NA+","83P",1166.69,"kN",206.08,"kN",3.68,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CT1 Atras,C NA+","83X",-1000.22,"kN",175.07,"kN",2.96,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CT1 Atras,C NA+","83XY",-907.29,"kN",166.07,"kN",5.03,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CT1 Atras,C NA+","83Y",1260.51,"kN",218.98,"kN",5.58,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CT1 Atras,C NA-","83P",907.29,"kN",159.35,"kN",2.74,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CT1 Atras,C NA-","83X",-764.58,"kN",131.44,"kN",1.78,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CT1 Atras,C NA-","83XY",-647.86,"kN",118.45,"kN",3.79,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CT1 Atras,C NA-","83Y",1024.8399999999999,"kN",176.01,"kN",4.4400000000000004,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CT1 Del,C NA+","83P",1306.1099999999999,"kN",227.64,"kN",5.71,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CT1 Del,C NA+","83X",-858.52,"kN",157.33000000000001,"kN",5.2,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CT1 Del,C NA+","83XY",-1045.92,"kN",183.7,"kN",3.1,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CT1 Del,C NA+","83Y",1116.57,"kN",196.57,"kN",3.39,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CT1 Del,C NA-","83P",1053.24,"kN",181.74,"kN",4.5999999999999996,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CT1 Del,C NA-","83X",-620.36,"kN",113.33,"kN",4.04,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CT1 Del,C NA-","83XY",-792.97,"kN",137.1,"kN",2,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CT1 Del,C NA-","83Y",878.33,"kN",153.38999999999999,"kN",2.4900000000000002,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CT2 Atras,C NA+","83P",1167.03,"kN",207.66,"kN",5.17,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CT2 Atras,C NA+","83X",-1000.8,"kN",177.29,"kN",5.16,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CT2 Atras,C NA+","83XY",-906.25,"kN",164.09,"kN",3.56,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CT2 Atras,C NA+","83Y",1259.75,"kN",217.18,"kN",3.3,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CT2 Atras,C NA-","83P",907.68,"kN",160.82,"kN",3.97,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CT2 Atras,C NA-","83X",-765.05,"kN",133.57,"kN",4.05,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CT2 Atras,C NA-","83XY",-646.83000000000004,"kN",116.56,"kN",2.56,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CT2 Atras,C NA-","83Y",1023.93,"kN",174.28,"kN",2.09,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CT2 Del,C NA+","83P",1303.83,"kN",225.74,"kN",3.48,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CT2 Del,C NA+","83X",-855.77,"kN",154.72999999999999,"kN",3.33,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CT2 Del,C NA+","83XY",-1045.07,"kN",185.66,"kN",5.13,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CT2 Del,C NA+","83Y",1115.3,"kN",198.28,"kN",5.18,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CT2 Del,C NA-","83P",1050.79,"kN",179.86,"kN",2.29,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CT2 Del,C NA-","83X",-617.62,"kN",110.73,"kN",2.29,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CT2 Del,C NA-","83XY",-792.01,"kN",138.91999999999999,"kN",3.94,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CT2 Del,C NA-","83Y",877.12,"kN",154.94,"kN",3.97,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CS 1  Amar Atras,C NA+","83P",1131.03,"kN",199.54,"kN",3.7,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CS 1  Amar Atras,C NA+","83X",-1018.14,"kN",177.84,"kN",2.84,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CS 1  Amar Atras,C NA+","83XY",-870.63,"kN",161.33000000000001,"kN",6.24,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CS 1  Amar Atras,C NA+","83Y",1280.54,"kN",223.7,"kN",6.93,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CS 1 Amar Atras,C NA-","83P",868.18,"kN",152.53,"kN",3.18,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CS 1 Amar Atras,C NA-","83X",-775.2,"kN",133.46,"kN",2.2200000000000002,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CS 1 Amar Atras,C NA-","83XY",-607.72,"kN",113.44,"kN",5.07,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CS 1 Amar Atras,C NA-","83Y",1037.55,"kN",179.71,"kN",5.83,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CS 1  Amar Del,C NA+","83P",1262.22,"kN",220.3,"kN",4.0999999999999996,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CS 1  Amar Del,C NA+","83X",-958.98,"kN",170.08,"kN",3.78,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CS 1  Amar Del,C NA+","83XY",-1001.52,"kN",178.21,"kN",3.8,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CS 1  Amar Del,C NA+","83Y",1219.1099999999999,"kN",211.94,"kN",3.96,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CS 1 Amar Del,C NA-","83P",999.39,"kN",172.98,"kN",2.91,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CS 1 Amar Del,C NA-","83X",-716.08,"kN",125.33,"kN",2.57,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CS 1 Amar Del,C NA-","83XY",-738.63,"kN",130.07,"kN",2.5499999999999998,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CS 1 Amar Del,C NA-","83Y",976.15,"kN",167.96,"kN",2.75,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CS 2 Amar Atras,C NA+","83P",1134.8800000000001,"kN",202.72,"kN",6.06,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CS 2 Amar Atras,C NA+","83X",-1022.85,"kN",181.94,"kN",6.17,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CS 2 Amar Atras,C NA+","83XY",-872.07,"kN",157.47999999999999,"kN",3.48,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CS 2 Amar Atras,C NA+","83Y",1282.8800000000001,"kN",220.62,"kN",2.91,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CS 2 Amar Atras,C NA-","83P",872.03,"kN",155.44,"kN",4.91,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CS 2 Amar Atras,C NA-","83X",-779.92,"kN",137.26,"kN",5.0999999999999996,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CS 2 Amar Atras,C NA-","83XY",-609.16999999999996,"kN",109.69,"kN",2.88,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CS 2 Amar Atras,C NA-","83Y",1039.8900000000001,"kN",176.87,"kN",2.11,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CS 2 Amar Del,C NA+","83P",1323.9,"kN",228.81,"kN",3.22,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CS 2 Amar Del,C NA+","83X",-832.14,"kN",149.58000000000001,"kN",3.08,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CS 2 Amar Del,C NA+","83XY",-1063.73,"kN",189.56,"kN",5.92,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CS 2 Amar Del,C NA+","83Y",1093.9000000000001,"kN",194.83,"kN",5.99,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CS 2 Amar Del,C NA-","83P",1060.96,"kN",181.66,"kN",2.38,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CS 2 Amar Del,C NA-","83X",-589.19000000000005,"kN",105.09,"kN",2.39,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CS 2 Amar Del,C NA-","83XY",-800.74,"kN",141.44,"kN",4.7699999999999996,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CS 2 Amar Del,C NA-","83Y",850.89,"kN",150.83000000000001,"kN",4.82,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CM 1 Amar Atras,C NA+","83P",1163.48,"kN",202.32,"kN",3.23,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CM 1 Amar Atras,C NA+","83X",-1002.5,"kN",176.75,"kN",3.32,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CM 1 Amar Atras,C NA+","83XY",-903.67,"kN",164.13,"kN",6.31,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CM 1 Amar Atras,C NA+","83Y",1265.57,"kN",222.05,"kN",6.59,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CM 1 Amar Atras,C NA-","83P",900.63,"kN",155.29,"kN",2.72,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CM 1 Amar Atras,C NA-","83X",-759.57,"kN",132.49,"kN",2.89,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CM 1 Amar Atras,C NA-","83XY",-640.77,"kN",116.28,"kN",5.2,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CM 1 Amar Atras,C NA-","83Y",1022.59,"kN",178.04,"kN",5.45,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CM 1 Amar Del,C NA+","83P",1262.22,"kN",220.3,"kN",4.0999999999999996,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CM 1 Amar Del,C NA+","83X",-958.98,"kN",170.08,"kN",3.78,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CM 1 Amar Del,C NA+","83XY",-1001.52,"kN",178.21,"kN",3.8,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CM 1 Amar Del,C NA+","83Y",1219.1099999999999,"kN",211.94,"kN",3.96,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CM 1 Amar Del,C NA-","83P",999.39,"kN",172.98,"kN",2.91,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CM 1 Amar Del,C NA-","83X",-716.08,"kN",125.33,"kN",2.57,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CM 1 Amar Del,C NA-","83XY",-738.63,"kN",130.07,"kN",2.5499999999999998,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CM 1 Amar Del,C NA-","83Y",976.15,"kN",167.96,"kN",2.75,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CM 2 Amar Atras,C NA+","83P",1167.99,"kN",205.77,"kN",6.4,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CM 2 Amar Atras,C NA+","83X",-1007.61,"kN",180.56,"kN",6.14,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CM 2 Amar Atras,C NA+","83XY",-904.41,"kN",160.16999999999999,"kN",3.1,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CM 2 Amar Atras,C NA+","83Y",1266.94,"kN",219.4,"kN",3.31,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CM 2 Amar Atras,C NA-","83P",905.14,"kN",158.54,"kN",5.33,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CM 2 Amar Atras,C NA-","83X",-764.69,"kN",135.88,"kN",5.05,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CM 2 Amar Atras,C NA-","83XY",-641.51,"kN",112.43,"kN",2.64,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CM 2 Amar Atras,C NA-","83Y",1023.96,"kN",175.79,"kN",2.86,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CM 2 Amar Del,C NA+","83P",1308.24,"kN",227.62,"kN",3.64,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CM 2 Amar Del,C NA+","83X",-863.69,"kN",152.18,"kN",2.68,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CM 2 Amar Del,C NA+","83XY",-1048.76,"kN",188.21,"kN",5.92,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CM 2 Amar Del,C NA+","83Y",1126.2,"kN",197.84,"kN",6.37,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CM 2 Amar Del,C NA-","83P",1045.32,"kN",180.6,"kN",3.09,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CM 2 Amar Del,C NA-","83X",-620.75,"kN",107.74,"kN",2.12,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CM 2 Amar Del,C NA-","83XY",-785.79,"kN",140.09,"kN",4.74,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CM 2 Amar Del,C NA-","83Y",883.21,"kN",153.88,"kN",5.27,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CI 1 Amar Atras,C NA+","83P",1188.29,"kN",203.12,"kN",2.58,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CI 1 Amar Atras,C NA+","83X",-978.92,"kN",173.73,"kN",3.79,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CI 1 Amar Atras,C NA+","83XY",-943.69,"kN",168.79,"kN",6.53,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CI 1 Amar Atras,C NA+","83Y",1257.27,"kN",222.26,"kN",6.48,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CI 1 Amar Atras,C NA-","83P",925.45,"kN",156.08000000000001,"kN",2.2000000000000002,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CI 1 Amar Atras,C NA-","83X",-736,"kN",129.65,"kN",3.54,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CI 1 Amar Atras,C NA-","83XY",-680.79,"kN",120.98,"kN",5.48,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CI 1 Amar Atras,C NA-","83Y",1014.3,"kN",178.24,"kN",5.31,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CI 1 Amar Del,C NA+","83P",1262.22,"kN",220.3,"kN",4.0999999999999996,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CI 1 Amar Del,C NA+","83X",-958.98,"kN",170.08,"kN",3.78,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CI 1 Amar Del,C NA+","83XY",-1001.52,"kN",178.21,"kN",3.8,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CI 1 Amar Del,C NA+","83Y",1219.1099999999999,"kN",211.94,"kN",3.96,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CI 1 Amar Del,C NA-","83P",999.39,"kN",172.98,"kN",2.91,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CI 1 Amar Del,C NA-","83X",-716.08,"kN",125.33,"kN",2.57,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CI 1 Amar Del,C NA-","83XY",-738.63,"kN",130.07,"kN",2.5499999999999998,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CI 1 Amar Del,C NA-","83Y",976.15,"kN",167.96,"kN",2.75,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CI 2 Amar Atras,C NA+","83P",1204.6300000000001,"kN",209.11,"kN",6.03,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CI 2 Amar Atras,C NA+","83X",-995.88,"kN",179.45,"kN",5.47,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CI 2 Amar Atras,C NA+","83XY",-932.45,"kN",161.79,"kN",2.33,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CI 2 Amar Atras,C NA+","83Y",1246.68,"kN",217.12,"kN",3.52,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CI 2 Amar Atras,C NA-","83P",941.79,"kN",161.85,"kN",4.9800000000000004,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CI 2 Amar Atras,C NA-","83X",-752.96,"kN",134.71,"kN",4.3099999999999996,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CI 2 Amar Atras,C NA-","83XY",-669.56,"kN",113.9,"kN",1.71,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CI 2 Amar Atras,C NA-","83Y",1003.71,"kN",173.52,"kN",3.06,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CI 2 Amar Del,C NA+","83P",1288.51,"kN",225.4,"kN",3.84,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CI 2 Amar Del,C NA+","83X",-891.21,"kN",153.84,"kN",2.02,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CI 2 Amar Del,C NA+","83XY",-1037.3900000000001,"kN",187.22,"kN",5.34,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CI 2 Amar Del,C NA+","83Y",1162.1199999999999,"kN",201.09,"kN",6.01,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CI 2 Amar Del,C NA-","83P",1025.6300000000001,"kN",178.39,"kN",3.29,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CI 2 Amar Del,C NA-","83X",-648.28,"kN",109.27,"kN",1.22,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CI 2 Amar Del,C NA-","83XY",-774.44,"kN",139.07,"kN",4.1100000000000003,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CI 2 Amar Del,C NA-","83Y",919.13,"kN",157.12,"kN",4.95,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CS Amar Atras (A4),C NA+","83P",1262.22,"kN",220.3,"kN",4.0999999999999996,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CS Amar Atras (A4),C NA+","83X",-958.98,"kN",170.08,"kN",3.78,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CS Amar Atras (A4),C NA+","83XY",-1001.52,"kN",178.21,"kN",3.8,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CS Amar Atras (A4),C NA+","83Y",1219.1099999999999,"kN",211.94,"kN",3.96,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CS Amar Atras (A4),C NA-","83P",999.39,"kN",172.98,"kN",2.91,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CS Amar Atras (A4),C NA-","83X",-716.08,"kN",125.33,"kN",2.57,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CS Amar Atras (A4),C NA-","83XY",-738.63,"kN",130.07,"kN",2.5499999999999998,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CS Amar Atras (A4),C NA-","83Y",976.15,"kN",167.96,"kN",2.75,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CS Amar Del (A4),C NA+","83P",1322.92,"kN",231.69,"kN",6.84,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CS Amar Del (A4),C NA+","83X",-831.73,"kN",154.05000000000001,"kN",6.35,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CS Amar Del (A4),C NA+","83XY",-1060.42,"kN",186.16,"kN",3.22,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CS Amar Del (A4),C NA+","83Y",1091.1500000000001,"kN",191.52,"kN",3.33,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CS Amar Del (A4),C NA-","83P",1059.98,"kN",184.38,"kN",5.75,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CS Amar Del (A4),C NA-","83X",-588.78,"kN",109.59,"kN",5.25,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CS Amar Del (A4),C NA-","83XY",-797.42,"kN",138.41,"kN",2.65,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CS Amar Del (A4),C NA-","83Y",848.14,"kN",147.87,"kN",2.86,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CM Amar Atras (A4),C NA+","83P",1262.22,"kN",220.3,"kN",4.0999999999999996,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CM Amar Atras (A4),C NA+","83X",-958.98,"kN",170.08,"kN",3.78,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CM Amar Atras (A4),C NA+","83XY",-1001.52,"kN",178.21,"kN",3.8,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CM Amar Atras (A4),C NA+","83Y",1219.1099999999999,"kN",211.94,"kN",3.96,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CM Amar Atras (A4),C NA-","83P",999.39,"kN",172.98,"kN",2.91,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CM Amar Atras (A4),C NA-","83X",-716.08,"kN",125.33,"kN",2.57,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CM Amar Atras (A4),C NA-","83XY",-738.63,"kN",130.07,"kN",2.5499999999999998,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CM Amar Atras (A4),C NA-","83Y",976.15,"kN",167.96,"kN",2.75,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CM Amar Del (A4),C NA+","83P",1308.17,"kN",230.07,"kN",6.52,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CM Amar Del (A4),C NA+","83X",-864.01,"kN",156.80000000000001,"kN",6.46,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CM Amar Del (A4),C NA+","83XY",-1045.02,"kN",185.11,"kN",3.73,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CM Amar Del (A4),C NA+","83Y",1122.8399999999999,"kN",194.24,"kN",2.86,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CM Amar Del (A4),C NA-","83P",1045.25,"kN",182.75,"kN",5.41,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CM Amar Del (A4),C NA-","83X",-621.07000000000005,"kN",112.39,"kN",5.43,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CM Amar Del (A4),C NA-","83XY",-782.05,"kN",137.49,"kN",3.32,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CM Amar Del (A4),C NA-","83Y",879.84,"kN",150.57,"kN",2.41,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CI Amar Atras (A4),C NA+","83P",1262.22,"kN",220.3,"kN",4.0999999999999996,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CI Amar Atras (A4),C NA+","83X",-958.98,"kN",170.08,"kN",3.78,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CI Amar Atras (A4),C NA+","83XY",-1001.52,"kN",178.21,"kN",3.8,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CI Amar Atras (A4),C NA+","83Y",1219.1099999999999,"kN",211.94,"kN",3.96,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CI Amar Atras (A4),C NA-","83P",999.39,"kN",172.98,"kN",2.91,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CI Amar Atras (A4),C NA-","83X",-716.08,"kN",125.33,"kN",2.57,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CI Amar Atras (A4),C NA-","83XY",-738.63,"kN",130.07,"kN",2.5499999999999998,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CI Amar Atras (A4),C NA-","83Y",976.15,"kN",167.96,"kN",2.75,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CI Amar Del (A4),C NA+","83P",1300.1199999999999,"kN",230.31,"kN",6.44,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CI Amar Del (A4),C NA+","83X",-903.21,"kN",161.4,"kN",6.71,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CI Amar Del (A4),C NA+","83XY",-1022.02,"kN",182.21,"kN",4.21,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","Rotura CI Amar Del (A4),C NA+","83Y",1147.1400000000001,"kN",195.03,"kN",2.23,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CI Amar Del (A4),C NA-","83P",1037.23,"kN",182.98,"kN",5.29,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CI Amar Del (A4),C NA-","83X",-660.28,"kN",117.02,"kN",5.74,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CI Amar Del (A4),C NA-","83XY",-759.08,"kN",134.77000000000001,"kN",3.96,"kN-m",0]
["T-6","d4a4a-a0-vidrio_ed.l_v3.tow","-Rotura CI Amar Del (A4),C NA-","83Y",904.15,"kN",151.35,"kN",1.91,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Viento,C NA+","117S",604.41,"kN",83.28,"kN",0.39,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Viento,C NA+","117X",-437.14,"kN",64.680000000000007,"kN",0.28999999999999998,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Viento,C NA+","117XY",-438.02,"kN",64.739999999999995,"kN",0.28999999999999998,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Viento,C NA+","117Y",603.9,"kN",83.18,"kN",0.38,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Viento,C NA-","117S",-443.93,"kN",64.17,"kN",0.44,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Viento,C NA-","117X",609.41999999999996,"kN",85.5,"kN",0.16,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Viento,C NA-","117XY",610.61,"kN",85.62,"kN",0.15,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Viento,C NA-","117Y",-442.96,"kN",64.03,"kN",0.44,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Hielo,C NA+","117S",100.83,"kN",12.3,"kN",0.02,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Hielo,C NA+","117X",106.64,"kN",13.05,"kN",0.02,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Hielo,C NA+","117XY",106.68,"kN",13.05,"kN",0.02,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Hielo,C NA+","117Y",100.87,"kN",12.31,"kN",0.02,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Viento+Hielo,C NA-","117S",-51.36,"kN",8.6199999999999992,"kN",0.09,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Viento+Hielo,C NA-","117X",259.12,"kN",34.04,"kN",0.03,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Viento+Hielo,C NA-","117XY",259.52,"kN",34.08,"kN",0.03,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Viento+Hielo,C NA-","117Y",-51.06,"kN",8.57,"kN",0.09,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Viento+Hielo,C NA+","117S",253.43,"kN",33.04,"kN",7.0000000000000007E-2,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Viento+Hielo,C NA+","117X",-45.08,"kN",8.11,"kN",0.06,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Viento+Hielo,C NA+","117XY",-45.37,"kN",8.1300000000000008,"kN",0.06,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Viento+Hielo,C NA+","117Y",253.24,"kN",33.01,"kN",7.0000000000000007E-2,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Tiro Vertical,C NA+","117S",77.959999999999994,"kN",9.6199999999999992,"kN",0.01,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Tiro Vertical,C NA+","117X",81.58,"kN",10.08,"kN",0.01,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Tiro Vertical,C NA+","117XY",81.599999999999994,"kN",10.09,"kN",0.01,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Tiro Vertical,C NA+","117Y",77.98,"kN",9.6199999999999992,"kN",0.01,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Desequilibrio Susp Atras,C NA+","117S",-125.04,"kN",13.06,"kN",0.19,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Desequilibrio Susp Atras,C NA+","117X",-434.33,"kN",54.48,"kN",0.1,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Desequilibrio Susp Atras,C NA+","117XY",339.18,"kN",39.049999999999997,"kN",0.21,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Desequilibrio Susp Atras,C NA+","117Y",633.41,"kN",79.209999999999994,"kN",0.31,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Desequilibrio Susp Atras,C NA-","117S",-440.03,"kN",54.96,"kN",0.09,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Desequilibrio Susp Atras,C NA-","117X",-119.94,"kN",12.17,"kN",0.23,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Desequilibrio Susp Atras,C NA-","117XY",638.70000000000005,"kN",80.16,"kN",0.27,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Desequilibrio Susp Atras,C NA-","117Y",334.49,"kN",38.67,"kN",0.24,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Desequilibrio Susp Del,C NA+","117S",633.21,"kN",79.19,"kN",0.31,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Desequilibrio Susp Del,C NA+","117X",339.98,"kN",39.15,"kN",0.21,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Desequilibrio Susp Del,C NA+","117XY",-434.1,"kN",54.44,"kN",0.1,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Desequilibrio Susp Del,C NA+","117Y",-125.67,"kN",13.15,"kN",0.19,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Desequilibrio Susp Del,C NA-","117S",333.88,"kN",38.6,"kN",0.24,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Desequilibrio Susp Del,C NA-","117X",638.72,"kN",80.180000000000007,"kN",0.27,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Desequilibrio Susp Del,C NA-","117XY",-119.11,"kN",12.07,"kN",0.24,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Desequilibrio Susp Del,C NA-","117Y",-440.07,"kN",54.96,"kN",0.09,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CT1 Atras,C NA+","117S",144.09,"kN",20.77,"kN",0.23,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CT1 Atras,C NA+","117X",-160.19,"kN",20.2,"kN",0.13,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CT1 Atras,C NA+","117XY",73.2,"kN",8.5399999999999991,"kN",0.22,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CT1 Atras,C NA+","117Y",355,"kN",45.51,"kN",0.37,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CT1 Atras,C NA-","117S",-152.15,"kN",21.91,"kN",0.36,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CT1 Atras,C NA-","117X",136.05000000000001,"kN",21.94,"kN",0.2,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CT1 Atras,C NA-","117XY",368.87,"kN",45.83,"kN",0.13,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CT1 Atras,C NA-","117Y",59.33,"kN",6.04,"kN",0.23,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CT1 Del,C NA+","117S",355.47,"kN",45.59,"kN",0.37,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CT1 Del,C NA+","117X",73.52,"kN",8.6,"kN",0.22,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CT1 Del,C NA+","117XY",-160.41,"kN",20.239999999999998,"kN",0.13,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CT1 Del,C NA+","117Y",144.21,"kN",20.8,"kN",0.23,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CT1 Del,C NA-","117S",57.83,"kN",5.9,"kN",0.23,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CT1 Del,C NA-","117X",370.1,"kN",45.95,"kN",0.13,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CT1 Del,C NA-","117XY",138,"kN",22.11,"kN",0.2,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CT1 Del,C NA-","117Y",-153.13,"kN",21.96,"kN",0.35,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CT2 Atras,C NA+","117S",130.76,"kN",20.98,"kN",0.24,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CT2 Atras,C NA+","117X",-146.21,"kN",21.48,"kN",0.31,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CT2 Atras,C NA+","117XY",64.78,"kN",6.3,"kN",0.28000000000000003,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CT2 Atras,C NA+","117Y",362.79,"kN",44.8,"kN",0.1,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CT2 Atras,C NA-","117S",-166.29,"kN",20.76,"kN",0.08,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CT2 Atras,C NA-","117X",149.72,"kN",21.68,"kN",0.28000000000000003,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CT2 Atras,C NA-","117XY",360.94,"kN",46.56,"kN",0.32,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CT2 Atras,C NA-","117Y",67.75,"kN",8.16,"kN",0.26,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CT2 Del,C NA+","117S",364.29,"kN",44.95,"kN",0.1,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CT2 Del,C NA+","117X",64.150000000000006,"kN",6.24,"kN",0.28000000000000003,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CT2 Del,C NA+","117XY",-147.47999999999999,"kN",21.57,"kN",0.3,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CT2 Del,C NA+","117Y",131.83000000000001,"kN",21.05,"kN",0.24,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CT2 Del,C NA-","117S",67.28,"kN",8.16,"kN",0.26,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CT2 Del,C NA-","117X",361.03,"kN",46.59,"kN",0.32,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CT2 Del,C NA-","117XY",150.63,"kN",21.8,"kN",0.28000000000000003,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CT2 Del,C NA-","117Y",-166.15,"kN",20.75,"kN",0.08,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CS 1  Susp Atras,C NA+","117S",147.06,"kN",21.3,"kN",0.32,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CS 1  Susp Atras,C NA+","117X",-170.63,"kN",22.01,"kN",0.25,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CS 1  Susp Atras,C NA+","117XY",77.510000000000005,"kN",11.51,"kN",0.32,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CS 1  Susp Atras,C NA+","117Y",361.56,"kN",47.31,"kN",0.46,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CS 1 Susp Atras,C NA-","117S",-160.27000000000001,"kN",23.3,"kN",0.39,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CS 1 Susp Atras,C NA-","117X",136.72999999999999,"kN",22.23,"kN",0.24,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CS 1 Susp Atras,C NA-","117XY",380.98,"kN",47.36,"kN",0.19,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CS 1 Susp Atras,C NA-","117Y",58.06,"kN",6.95,"kN",0.26,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CS 1  Susp Del,C NA+","117S",361.31,"kN",47.29,"kN",0.46,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CS 1  Susp Del,C NA+","117X",78.25,"kN",11.58,"kN",0.32,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CS 1  Susp Del,C NA+","117XY",-170.44,"kN",22,"kN",0.25,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CS 1  Susp Del,C NA+","117Y",146.38999999999999,"kN",21.23,"kN",0.32,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CS 1 Susp Del,C NA-","117S",57.34,"kN",6.84,"kN",0.25,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CS 1 Susp Del,C NA-","117X",381,"kN",47.36,"kN",0.19,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CS 1 Susp Del,C NA-","117XY",137.58000000000001,"kN",22.29,"kN",0.24,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CS 1 Susp Del,C NA-","117Y",-160.41999999999999,"kN",23.28,"kN",0.38,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CS 2 Susp Atras,C NA+","117S",131.37,"kN",21.29,"kN",0.28999999999999998,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CS 2 Susp Atras,C NA+","117X",-154.29,"kN",22.89,"kN",0.34,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CS 2 Susp Atras,C NA+","117XY",63.53,"kN",7.22,"kN",0.31,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CS 2 Susp Atras,C NA+","117Y",374.88,"kN",46.35,"kN",0.15,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CS 2 Susp Atras,C NA-","117S",-176.81,"kN",22.59,"kN",0.2,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CS 2 Susp Atras,C NA-","117X",152.66,"kN",22.16,"kN",0.37,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CS 2 Susp Atras,C NA-","117XY",367.41,"kN",48.35,"kN",0.41,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CS 2 Susp Atras,C NA-","117Y",72.23,"kN",11.2,"kN",0.37,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CS 2 Susp Del,C NA+","117S",375.22,"kN",46.39,"kN",0.14000000000000001,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CS 2 Susp Del,C NA+","117X",63.68,"kN",7.19,"kN",0.31,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CS 2 Susp Del,C NA+","117XY",-154.74,"kN",22.91,"kN",0.33,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CS 2 Susp Del,C NA+","117Y",131.34,"kN",21.26,"kN",0.28000000000000003,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CS 2 Susp Del,C NA-","117S",72.11,"kN",11.23,"kN",0.37,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CS 2 Susp Del,C NA-","117X",366.83,"kN",48.29,"kN",0.41,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CS 2 Susp Del,C NA-","117XY",152.87,"kN",22.19,"kN",0.37,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CS 2 Susp Del,C NA-","117Y",-176.31,"kN",22.54,"kN",0.2,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CM 1 Susp Atras,C NA+","117S",166.91,"kN",22.74,"kN",0.33,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CM 1 Susp Atras,C NA+","117X",-153.56,"kN",21.6,"kN",0.35,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CM 1 Susp Atras,C NA+","117XY",60.74,"kN",13.38,"kN",0.41,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CM 1 Susp Atras,C NA+","117Y",341.38,"kN",46.05,"kN",0.47,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CM 1 Susp Atras,C NA-","117S",-140.21,"kN",22.29,"kN",0.4,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CM 1 Susp Atras,C NA-","117X",153.65,"kN",24.53,"kN",0.33,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CM 1 Susp Atras,C NA-","117XY",364.33,"kN",46.37,"kN",0.28000000000000003,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CM 1 Susp Atras,C NA-","117Y",37.700000000000003,"kN",6.54,"kN",0.26,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CM 1 Susp Del,C NA+","117S",341.33,"kN",46.06,"kN",0.47,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CM 1 Susp Del,C NA+","117X",61.29,"kN",13.44,"kN",0.41,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CM 1 Susp Del,C NA+","117XY",-153.57,"kN",21.62,"kN",0.35,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CM 1 Susp Del,C NA+","117Y",166.45,"kN",22.69,"kN",0.33,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CM 1 Susp Del,C NA-","117S",37.18,"kN",6.45,"kN",0.25,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CM 1 Susp Del,C NA-","117X",364.16,"kN",46.35,"kN",0.28000000000000003,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CM 1 Susp Del,C NA-","117XY",154.31,"kN",24.57,"kN",0.33,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CM 1 Susp Del,C NA-","117Y",-140.15,"kN",22.26,"kN",0.4,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CM 2 Susp Atras,C NA+","117S",148.16,"kN",23.58,"kN",0.38,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CM 2 Susp Atras,C NA+","117X",-134.11000000000001,"kN",21.89,"kN",0.35,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CM 2 Susp Atras,C NA+","117XY",43.4,"kN",6.72,"kN",0.31,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CM 2 Susp Atras,C NA+","117Y",358.02,"kN",45.35,"kN",0.24,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CM 2 Susp Atras,C NA-","117S",-159.91999999999999,"kN",22.18,"kN",0.3,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CM 2 Susp Atras,C NA-","117X",172.68,"kN",23.61,"kN",0.38,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CM 2 Susp Atras,C NA-","117XY",347.4,"kN",47.1,"kN",0.42,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CM 2 Susp Atras,C NA-","117Y",55.3,"kN",13.11,"kN",0.46,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CM 2 Susp Del,C NA+","117S",358.35,"kN",45.39,"kN",0.23,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CM 2 Susp Del,C NA+","117X",43.56,"kN",6.68,"kN",0.31,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CM 2 Susp Del,C NA+","117XY",-134.54,"kN",21.9,"kN",0.35,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CM 2 Susp Del,C NA+","117Y",148.12,"kN",23.55,"kN",0.38,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CM 2 Susp Del,C NA-","117S",55.16,"kN",13.14,"kN",0.46,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CM 2 Susp Del,C NA-","117X",346.85,"kN",47.05,"kN",0.42,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CM 2 Susp Del,C NA-","117XY",172.92,"kN",23.65,"kN",0.38,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CM 2 Susp Del,C NA-","117Y",-159.43,"kN",22.14,"kN",0.3,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CI 1 Susp Atras,C NA+","117S",183.92,"kN",23.37,"kN",0.24,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CI 1 Susp Atras,C NA+","117X",-133.71,"kN",20.309999999999999,"kN",0.35,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CI 1 Susp Atras,C NA+","117XY",40.79,"kN",12.96,"kN",0.4,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CI 1 Susp Atras,C NA+","117Y",324.43,"kN",44.31,"kN",0.38,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CI 1 Susp Atras,C NA-","117S",-123,"kN",20.22,"kN",0.32,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CI 1 Susp Atras,C NA-","117X",173.07,"kN",25.74,"kN",0.33,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CI 1 Susp Atras,C NA-","117XY",344.76,"kN",44.99,"kN",0.28999999999999998,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CI 1 Susp Atras,C NA-","117Y",20.59,"kN",4.0999999999999996,"kN",0.17,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CI 1 Susp Del,C NA+","117S",324.27999999999997,"kN",44.29,"kN",0.38,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CI 1 Susp Del,C NA+","117X",41.47,"kN",13,"kN",0.4,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CI 1 Susp Del,C NA+","117XY",-133.58000000000001,"kN",20.3,"kN",0.35,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CI 1 Susp Del,C NA+","117Y",183.34,"kN",23.29,"kN",0.24,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CI 1 Susp Del,C NA-","117S",19.96,"kN",3.99,"kN",0.16,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CI 1 Susp Del,C NA-","117X",344.73,"kN",44.99,"kN",0.28999999999999998,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CI 1 Susp Del,C NA-","117XY",173.87,"kN",25.81,"kN",0.33,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CI 1 Susp Del,C NA-","117Y",-123.06,"kN",20.21,"kN",0.32,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CI 2 Susp Atras,C NA+","117S",167.7,"kN",24.83,"kN",0.39,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CI 2 Susp Atras,C NA+","117X",-117.03,"kN",19.84,"kN",0.28000000000000003,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CI 2 Susp Atras,C NA+","117XY",26.09,"kN",4.28,"kN",0.22,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CI 2 Susp Atras,C NA+","117Y",338.66,"kN",44.01,"kN",0.24,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CI 2 Susp Atras,C NA-","117S",-139.91999999999999,"kN",20.87,"kN",0.3,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CI 2 Susp Atras,C NA-","117X",189.54,"kN",24.27,"kN",0.28999999999999998,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CI 2 Susp Atras,C NA-","117XY",330.28,"kN",45.34,"kN",0.34,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CI 2 Susp Atras,C NA-","117Y",35.520000000000003,"kN",12.76,"kN",0.45,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CI 2 Susp Del,C NA+","117S",338.95,"kN",44.05,"kN",0.24,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CI 2 Susp Del,C NA+","117X",26.32,"kN",4.25,"kN",0.22,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CI 2 Susp Del,C NA+","117XY",-117.38,"kN",19.850000000000001,"kN",0.28000000000000003,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","Rotura CI 2 Susp Del,C NA+","117Y",167.62,"kN",24.79,"kN",0.38,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CI 2 Susp Del,C NA-","117S",35.340000000000003,"kN",12.8,"kN",0.45,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CI 2 Susp Del,C NA-","117X",329.79,"kN",45.29,"kN",0.34,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CI 2 Susp Del,C NA-","117XY",189.85,"kN",24.31,"kN",0.28999999999999998,"kN-m",0]
["T-7","d4s1_cadenav-ac_ed.b_v2.tow","-Rotura CI 2 Susp Del,C NA-","117Y",-139.47999999999999,"kN",20.84,"kN",0.3,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Viento,C NA+","101S",578.88,"kN",78.91,"kN",0.28000000000000003,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Viento,C NA+","101X",-452.83,"kN",65.44,"kN",0.25,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Viento,C NA+","101XY",-451.96,"kN",65.349999999999994,"kN",0.25,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Viento,C NA+","101Y",579.66999999999996,"kN",79.02,"kN",0.28000000000000003,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Viento,C NA-","101S",-452.7,"kN",64.06,"kN",0.31,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Viento,C NA-","101X",578.75,"kN",80.39,"kN",0.2,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Viento,C NA-","101XY",579.54,"kN",80.5,"kN",0.2,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Viento,C NA-","101Y",-451.83,"kN",63.97,"kN",0.32,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Hielo,C NA+","101S",84.62,"kN",10.220000000000001,"kN",0.01,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Hielo,C NA+","101X",84.62,"kN",10.220000000000001,"kN",0.01,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Hielo,C NA+","101XY",84.62,"kN",10.220000000000001,"kN",0.01,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Hielo,C NA+","101Y",84.62,"kN",10.220000000000001,"kN",0.01,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Viento+Hielo,C NA-","101S",-64.239999999999995,"kN",10.42,"kN",0.08,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Viento+Hielo,C NA-","101X",233.2,"kN",30.9,"kN",0.05,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Viento+Hielo,C NA-","101XY",233.29,"kN",30.91,"kN",0.05,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Viento+Hielo,C NA-","101Y",-64.14,"kN",10.41,"kN",0.08,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Viento+Hielo,C NA+","101S",233.2,"kN",30.64,"kN",0.06,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Viento+Hielo,C NA+","101X",-64.25,"kN",10.69,"kN",7.0000000000000007E-2,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Viento+Hielo,C NA+","101XY",-64.150000000000006,"kN",10.68,"kN",7.0000000000000007E-2,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Viento+Hielo,C NA+","101Y",233.29,"kN",30.65,"kN",0.06,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Tiro Vertical,C NA+","101S",64.58,"kN",7.86,"kN",0.01,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Tiro Vertical,C NA+","101X",64.58,"kN",7.86,"kN",0.01,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Tiro Vertical,C NA+","101XY",64.58,"kN",7.86,"kN",0.01,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Tiro Vertical,C NA+","101Y",64.58,"kN",7.86,"kN",0.01,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Atras,C NA+","101S",-134.87,"kN",15.09,"kN",0.25,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Atras,C NA+","101X",-444.43,"kN",56.2,"kN",0.14000000000000001,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Atras,C NA+","101XY",313.72000000000003,"kN",36.340000000000003,"kN",0.26,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Atras,C NA+","101Y",606.65,"kN",76.78,"kN",0.34,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Atras,C NA-","101S",-444.44,"kN",55.98,"kN",0.12,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Atras,C NA-","101X",-134.86000000000001,"kN",14.82,"kN",0.28000000000000003,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Atras,C NA-","101XY",606.62,"kN",77.03,"kN",0.31,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Atras,C NA-","101Y",313.75,"kN",36.520000000000003,"kN",0.28000000000000003,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Del,C NA+","101S",605.65,"kN",76.680000000000007,"kN",0.34,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Del,C NA+","101X",312.58,"kN",36.22,"kN",0.26,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Del,C NA+","101XY",-445.36,"kN",56.31,"kN",0.15,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Del,C NA+","101Y",-135.49,"kN",15.18,"kN",0.26,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Del,C NA-","101S",312.61,"kN",36.4,"kN",0.28000000000000003,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Del,C NA-","101X",605.62,"kN",76.92,"kN",0.31,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Del,C NA-","101XY",-135.47,"kN",14.91,"kN",0.28000000000000003,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Del,C NA-","101Y",-445.38,"kN",56.09,"kN",0.13,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Atras,C NA+","101S",120.71,"kN",18.27,"kN",0.34,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Atras,C NA+","101X",-181.07,"kN",22.69,"kN",0.17,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Atras,C NA+","101XY",57.51,"kN",8.58,"kN",0.28999999999999998,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Atras,C NA+","101Y",338.88,"kN",44.25,"kN",0.43,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Atras,C NA-","101S",-169.83,"kN",24.9,"kN",0.43,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Atras,C NA-","101X",110.01,"kN",19.82,"kN",0.26,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Atras,C NA-","101XY",346.91,"kN",42.69,"kN",0.17,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Atras,C NA-","101Y",48.93,"kN",6.33,"kN",0.32,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Del,C NA+","101S",337.76,"kN",44.08,"kN",0.43,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Del,C NA+","101X",57.53,"kN",8.56,"kN",0.28999999999999998,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Del,C NA+","101XY",-180.81,"kN",22.63,"kN",0.17,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Del,C NA+","101Y",119.81,"kN",18.149999999999999,"kN",0.34,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Del,C NA-","101S",50.06,"kN",6.34,"kN",0.32,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Del,C NA-","101X",344.68,"kN",42.48,"kN",0.17,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Del,C NA-","101XY",108.01,"kN",19.670000000000002,"kN",0.27,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Del,C NA-","101Y",-168.47,"kN",24.82,"kN",0.43,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Atras,C NA+","101S",110.1,"kN",19.53,"kN",0.28000000000000003,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Atras,C NA+","101X",-169.83,"kN",25.19,"kN",0.4,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Atras,C NA+","101XY",48.92,"kN",6.06,"kN",0.35,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Atras,C NA+","101Y",346.83,"kN",42.44,"kN",0.15,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Atras,C NA-","101S",-181.05,"kN",22.48,"kN",0.15,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Atras,C NA-","101X",120.78,"kN",18.45,"kN",0.36,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Atras,C NA-","101XY",338.79,"kN",44.51,"kN",0.41,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Atras,C NA-","101Y",57.51,"kN",8.4499999999999993,"kN",0.31,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Del,C NA+","101S",344.61,"kN",42.23,"kN",0.14000000000000001,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Del,C NA+","101X",50.04,"kN",6.06,"kN",0.35,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Del,C NA+","101XY",-168.46,"kN",25.11,"kN",0.4,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Del,C NA+","101Y",108.09,"kN",19.39,"kN",0.28999999999999998,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Del,C NA-","101S",57.52,"kN",8.44,"kN",0.31,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Del,C NA-","101X",337.67,"kN",44.35,"kN",0.41,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Del,C NA-","101XY",119.88,"kN",18.329999999999998,"kN",0.36,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Del,C NA-","101Y",-180.79,"kN",22.43,"kN",0.15,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Atras,C NA+","101S",124.11,"kN",19.25,"kN",0.47,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Atras,C NA+","101X",-189.54,"kN",24.47,"kN",0.33,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Atras,C NA+","101XY",60.71,"kN",12.64,"kN",0.44,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Atras,C NA+","101Y",343.6,"kN",46.39,"kN",0.56999999999999995,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Atras,C NA-","101S",-176.47,"kN",26.27,"kN",0.46,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Atras,C NA-","101X",111.76,"kN",20.46,"kN",0.32,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Atras,C NA-","101XY",356.84,"kN",44.02,"kN",0.24,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Atras,C NA-","101Y",46.74,"kN",7.46,"kN",0.36,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Del,C NA+","101S",343.67,"kN",46.37,"kN",0.56999999999999995,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Del,C NA+","101X",59.96,"kN",12.62,"kN",0.44,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Del,C NA+","101XY",-190.11,"kN",24.52,"kN",0.34,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Del,C NA+","101Y",124.41,"kN",19.27,"kN",0.47,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Del,C NA-","101S",46.74,"kN",7.41,"kN",0.36,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Del,C NA-","101X",356.17,"kN",43.97,"kN",0.24,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Del,C NA-","101XY",111.31,"kN",20.440000000000001,"kN",0.32,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Del,C NA-","101Y",-176.29,"kN",26.28,"kN",0.46,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Atras,C NA+","101S",111.82,"kN",20.170000000000002,"kN",0.34,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Atras,C NA+","101X",-176.5,"kN",26.58,"kN",0.44,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Atras,C NA+","101XY",46.76,"kN",7.2,"kN",0.38,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Atras,C NA+","101Y",356.8,"kN",43.79,"kN",0.22,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Atras,C NA-","101S",-189.57,"kN",24.31,"kN",0.31,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Atras,C NA-","101X",124.17,"kN",19.38,"kN",0.49,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Atras,C NA-","101XY",343.53,"kN",46.66,"kN",0.54,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Atras,C NA-","101Y",60.75,"kN",12.48,"kN",0.46,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Del,C NA+","101S",356.12,"kN",43.74,"kN",0.22,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Del,C NA+","101X",46.75,"kN",7.15,"kN",0.38,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Del,C NA+","101XY",-176.32,"kN",26.58,"kN",0.44,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Del,C NA+","101Y",111.37,"kN",20.149999999999999,"kN",0.34,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Del,C NA-","101S",60,"kN",12.46,"kN",0.46,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Del,C NA-","101X",343.59,"kN",46.64,"kN",0.54,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Del,C NA-","101XY",124.47,"kN",19.399999999999999,"kN",0.49,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Del,C NA-","101Y",-190.14,"kN",24.35,"kN",0.31,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Atras,C NA+","101S",148.08000000000001,"kN",20.88,"kN",0.48,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Atras,C NA+","101X",-168.32,"kN",24.1,"kN",0.47,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Atras,C NA+","101XY",39.630000000000003,"kN",15.57,"kN",0.56000000000000005,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Atras,C NA+","101Y",319.48,"kN",45.04,"kN",0.57999999999999996,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Atras,C NA-","101S",-152.28,"kN",25.15,"kN",0.48,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Atras,C NA-","101X",132.83000000000001,"kN",23.6,"kN",0.44,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Atras,C NA-","101XY",335.9,"kN",42.83,"kN",0.38,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Atras,C NA-","101Y",22.42,"kN",7.5,"kN",0.36,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Del,C NA+","101S",319.62,"kN",45.03,"kN",0.57999999999999996,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Del,C NA+","101X",38.82,"kN",15.56,"kN",0.56000000000000005,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Del,C NA+","101XY",-168.96,"kN",24.16,"kN",0.47,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Del,C NA+","101Y",148.44,"kN",20.91,"kN",0.48,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Del,C NA-","101S",22.5,"kN",7.45,"kN",0.36,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Del,C NA-","101X",335.15,"kN",42.76,"kN",0.38,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Del,C NA-","101XY",132.30000000000001,"kN",23.57,"kN",0.44,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Del,C NA-","101Y",-152.02000000000001,"kN",25.15,"kN",0.48,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Atras,C NA+","101S",132.9,"kN",23.31,"kN",0.46,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Atras,C NA+","101X",-152.33000000000001,"kN",25.46,"kN",0.46,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Atras,C NA+","101XY",22.45,"kN",7.27,"kN",0.39,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Atras,C NA+","101Y",335.85,"kN",42.62,"kN",0.36,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Atras,C NA-","101S",-168.36,"kN",23.97,"kN",0.45,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Atras,C NA-","101X",148.15,"kN",21.02,"kN",0.5,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Atras,C NA-","101XY",319.39,"kN",45.31,"kN",0.56000000000000005,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Atras,C NA-","101Y",39.69,"kN",15.38,"kN",0.57999999999999996,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Del,C NA+","101S",335.09,"kN",42.55,"kN",0.35,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Del,C NA+","101X",22.53,"kN",7.22,"kN",0.39,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Del,C NA+","101XY",-152.07,"kN",25.47,"kN",0.46,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Del,C NA+","101Y",132.37,"kN",23.28,"kN",0.46,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Del,C NA-","101S",38.880000000000003,"kN",15.37,"kN",0.57999999999999996,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Del,C NA-","101X",319.52999999999997,"kN",45.3,"kN",0.56000000000000005,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Del,C NA-","101XY",148.51,"kN",21.05,"kN",0.5,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Del,C NA-","101Y",-169,"kN",24.03,"kN",0.45,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Atras,C NA+","101S",168.89,"kN",21.3,"kN",0.36,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Atras,C NA+","101X",-143.96,"kN",22.6,"kN",0.48,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Atras,C NA+","101XY",15.27,"kN",15.54,"kN",0.55000000000000004,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Atras,C NA+","101Y",298.68,"kN",42.71,"kN",0.47,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Atras,C NA-","101S",-130.97999999999999,"kN",22.54,"kN",0.38,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Atras,C NA-","101X",156.41999999999999,"kN",24.96,"kN",0.45,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Atras,C NA-","101XY",312.27,"kN",41.26,"kN",0.39,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Atras,C NA-","101Y",1.1599999999999999,"kN",4.7,"kN",0.25,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Del,C NA+","101S",298.77,"kN",42.69,"kN",0.47,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Del,C NA+","101X",14.51,"kN",15.53,"kN",0.55000000000000004,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Del,C NA+","101XY",-144.54,"kN",22.66,"kN",0.48,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Del,C NA+","101Y",169.19,"kN",21.32,"kN",0.36,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Del,C NA-","101S",1.2,"kN",4.66,"kN",0.24,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Del,C NA-","101X",311.57,"kN",41.21,"kN",0.39,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Del,C NA-","101XY",155.93,"kN",24.94,"kN",0.45,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Del,C NA-","101Y",-130.77000000000001,"kN",22.55,"kN",0.38,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Atras,C NA+","101S",156.47999999999999,"kN",24.67,"kN",0.47,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Atras,C NA+","101X",-131.02000000000001,"kN",22.85,"kN",0.36,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Atras,C NA+","101XY",1.2,"kN",4.5199999999999996,"kN",0.27,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Atras,C NA+","101Y",312.22000000000003,"kN",41.06,"kN",0.37,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Atras,C NA-","101S",-144,"kN",22.48,"kN",0.46,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Atras,C NA-","101X",168.95,"kN",21.48,"kN",0.38,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Atras,C NA-","101XY",298.60000000000002,"kN",42.98,"kN",0.45,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Atras,C NA-","101Y",15.33,"kN",15.32,"kN",0.57999999999999996,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Del,C NA+","101S",311.52,"kN",41,"kN",0.37,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Del,C NA+","101X",1.23,"kN",4.4800000000000004,"kN",0.27,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Del,C NA+","101XY",-130.82,"kN",22.85,"kN",0.36,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Del,C NA+","101Y",155.99,"kN",24.64,"kN",0.47,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Del,C NA-","101S",14.57,"kN",15.32,"kN",0.57999999999999996,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Del,C NA-","101X",298.69,"kN",42.96,"kN",0.45,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Del,C NA-","101XY",169.25,"kN",21.5,"kN",0.38,"kN-m",0]
["T-8","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Del,C NA-","101Y",-144.59,"kN",22.54,"kN",0.46,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Viento,C NA+","101S",657.24,"kN",89.03,"kN",0.28000000000000003,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Viento,C NA+","101X",-520.95000000000005,"kN",74.41,"kN",0.25,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Viento,C NA+","101XY",-521.28,"kN",74.45,"kN",0.25,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Viento,C NA+","101Y",656.95,"kN",88.99,"kN",0.28000000000000003,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Viento,C NA-","101S",-520.79999999999995,"kN",73.040000000000006,"kN",0.32,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Viento,C NA-","101X",657.09,"kN",90.5,"kN",0.21,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Viento,C NA-","101XY",656.8,"kN",90.46,"kN",0.2,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Viento,C NA-","101Y",-521.13,"kN",73.08,"kN",0.32,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Hielo,C NA+","101S",93.15,"kN",11.23,"kN",0.01,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Hielo,C NA+","101X",93.15,"kN",11.23,"kN",0.01,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Hielo,C NA+","101XY",93.15,"kN",11.23,"kN",0.01,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Hielo,C NA+","101Y",93.15,"kN",11.23,"kN",0.01,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Viento+Hielo,C NA-","101S",-79.260000000000005,"kN",12.55,"kN",0.09,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Viento+Hielo,C NA-","101X",265.31,"kN",35.04,"kN",0.05,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Viento+Hielo,C NA-","101XY",265.27999999999997,"kN",35.03,"kN",0.05,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Viento+Hielo,C NA-","101Y",-79.290000000000006,"kN",12.55,"kN",0.09,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Viento+Hielo,C NA+","101S",265.32,"kN",34.78,"kN",7.0000000000000007E-2,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Viento+Hielo,C NA+","101X",-79.260000000000005,"kN",12.82,"kN",0.08,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Viento+Hielo,C NA+","101XY",-79.3,"kN",12.82,"kN",0.08,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Viento+Hielo,C NA+","101Y",265.27999999999997,"kN",34.770000000000003,"kN",7.0000000000000007E-2,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Tiro Vertical,C NA+","101S",69.59,"kN",8.4499999999999993,"kN",0.01,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Tiro Vertical,C NA+","101X",69.59,"kN",8.4499999999999993,"kN",0.01,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Tiro Vertical,C NA+","101XY",69.59,"kN",8.4499999999999993,"kN",0.01,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Tiro Vertical,C NA+","101Y",69.59,"kN",8.4499999999999993,"kN",0.01,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Atras,C NA+","101S",-103.5,"kN",11.08,"kN",0.27,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Atras,C NA+","101X",-460.75,"kN",58.42,"kN",0.15,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Atras,C NA+","101XY",299.02999999999997,"kN",34.44,"kN",0.28000000000000003,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Atras,C NA+","101Y",638.35,"kN",80.92,"kN",0.36,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Atras,C NA-","101S",-460.77,"kN",58.2,"kN",0.13,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Atras,C NA-","101X",-103.48,"kN",10.8,"kN",0.28999999999999998,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Atras,C NA-","101XY",638.30999999999995,"kN",81.17,"kN",0.33,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Atras,C NA-","101Y",299.06,"kN",34.61,"kN",0.28999999999999998,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Del,C NA+","101S",638.69000000000005,"kN",80.95,"kN",0.36,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Del,C NA+","101X",299.31,"kN",34.46,"kN",0.28000000000000003,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Del,C NA+","101XY",-460.55,"kN",58.4,"kN",0.15,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Desequilibrio Susp Del,C NA+","101Y",-103.28,"kN",11.05,"kN",0.27,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Del,C NA-","101S",299.33999999999997,"kN",34.630000000000003,"kN",0.28999999999999998,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Del,C NA-","101X",638.65,"kN",81.2,"kN",0.33,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Del,C NA-","101XY",-103.26,"kN",10.77,"kN",0.28999999999999998,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Desequilibrio Susp Del,C NA-","101Y",-460.57,"kN",58.18,"kN",0.13,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Atras,C NA+","101S",151.61000000000001,"kN",22.02,"kN",0.34,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Atras,C NA+","101X",-195.99,"kN",24.71,"kN",0.16,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Atras,C NA+","101XY",43.03,"kN",8.58,"kN",0.3,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Atras,C NA+","101Y",370.01,"kN",48.19,"kN",0.44,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Atras,C NA-","101S",-183.86,"kN",26.89,"kN",0.43,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Atras,C NA-","101X",140.12,"kN",23.56,"kN",0.27,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Atras,C NA-","101XY",377.16,"kN",46.6,"kN",0.16,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Atras,C NA-","101Y",35.229999999999997,"kN",5.31,"kN",0.32,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Del,C NA+","101S",369.59,"kN",48.15,"kN",0.44,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Del,C NA+","101X",43.45,"kN",8.58,"kN",0.3,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Del,C NA+","101XY",-195.63,"kN",24.67,"kN",0.16,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT1 Del,C NA+","101Y",151.13,"kN",21.97,"kN",0.34,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Del,C NA-","101S",35.729999999999997,"kN",5.31,"kN",0.32,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Del,C NA-","101X",376.67,"kN",46.55,"kN",0.16,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Del,C NA-","101XY",139.56,"kN",23.51,"kN",0.27,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT1 Del,C NA-","101Y",-183.42,"kN",26.85,"kN",0.43,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Atras,C NA+","101S",140.19999999999999,"kN",23.28,"kN",0.28999999999999998,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Atras,C NA+","101X",-183.86,"kN",27.18,"kN",0.41,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Atras,C NA+","101XY",35.21,"kN",5.08,"kN",0.34,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Atras,C NA+","101Y",377.09,"kN",46.36,"kN",0.14000000000000001,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Atras,C NA-","101S",-195.97,"kN",24.5,"kN",0.14000000000000001,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Atras,C NA-","101X",151.68,"kN",22.22,"kN",0.36,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Atras,C NA-","101XY",369.92,"kN",48.46,"kN",0.41,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Atras,C NA-","101Y",43.02,"kN",8.39,"kN",0.31,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Del,C NA+","101S",376.6,"kN",46.31,"kN",0.14000000000000001,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Del,C NA+","101X",35.71,"kN",5.08,"kN",0.34,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Del,C NA+","101XY",-183.42,"kN",27.15,"kN",0.41,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CT2 Del,C NA+","101Y",139.65,"kN",23.23,"kN",0.28999999999999998,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Del,C NA-","101S",43.44,"kN",8.39,"kN",0.31,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Del,C NA-","101X",369.51,"kN",48.42,"kN",0.41,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Del,C NA-","101XY",151.19999999999999,"kN",22.17,"kN",0.36,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CT2 Del,C NA-","101Y",-195.61,"kN",24.46,"kN",0.14000000000000001,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Atras,C NA+","101S",156.21,"kN",22.9,"kN",0.47,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Atras,C NA+","101X",-205.28,"kN",26.49,"kN",0.34,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Atras,C NA+","101XY",45.61,"kN",12.81,"kN",0.45,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Atras,C NA+","101Y",375.8,"kN",50.46,"kN",0.57999999999999996,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Atras,C NA-","101S",-191.73,"kN",28.3,"kN",0.46,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Atras,C NA-","101X",143.52000000000001,"kN",24.19,"kN",0.32,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Atras,C NA-","101XY",388.59,"kN",48.07,"kN",0.23,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Atras,C NA-","101Y",31.95,"kN",6.33,"kN",0.35,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Del,C NA+","101S",375.81,"kN",50.47,"kN",0.57999999999999996,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Del,C NA+","101X",45.82,"kN",12.81,"kN",0.45,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Del,C NA+","101XY",-205.15,"kN",26.48,"kN",0.34,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 1  Susp Del,C NA+","101Y",156.13,"kN",22.9,"kN",0.47,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Del,C NA-","101S",31.94,"kN",6.34,"kN",0.35,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Del,C NA-","101X",388.81,"kN",48.09,"kN",0.23,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Del,C NA-","101XY",143.66,"kN",24.2,"kN",0.32,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 1 Susp Del,C NA-","101Y",-191.81,"kN",28.31,"kN",0.46,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Atras,C NA+","101S",143.59,"kN",23.91,"kN",0.34,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Atras,C NA+","101X",-191.77,"kN",28.61,"kN",0.44,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Atras,C NA+","101XY",31.97,"kN",6.1,"kN",0.37,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Atras,C NA+","101Y",388.55,"kN",47.83,"kN",0.21,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Atras,C NA-","101S",-205.31,"kN",26.32,"kN",0.31,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Atras,C NA-","101X",156.27000000000001,"kN",23.06,"kN",0.5,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Atras,C NA-","101XY",375.72,"kN",50.73,"kN",0.55000000000000004,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Atras,C NA-","101Y",45.66,"kN",12.61,"kN",0.47,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Del,C NA+","101S",388.77,"kN",47.85,"kN",0.21,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Del,C NA+","101X",31.96,"kN",6.12,"kN",0.37,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Del,C NA+","101XY",-191.85,"kN",28.61,"kN",0.44,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CS 2 Susp Del,C NA+","101Y",143.72999999999999,"kN",23.92,"kN",0.34,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Del,C NA-","101S",45.86,"kN",12.61,"kN",0.47,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Del,C NA-","101X",375.73,"kN",50.74,"kN",0.55000000000000004,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Del,C NA-","101XY",156.19,"kN",23.05,"kN",0.5,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CS 2 Susp Del,C NA-","101Y",-205.18,"kN",26.31,"kN",0.31,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Atras,C NA+","101S",180.27,"kN",24.56,"kN",0.48,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Atras,C NA+","101X",-184,"kN",25.99,"kN",0.47,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Atras,C NA+","101XY",24.41,"kN",16.02,"kN",0.56999999999999995,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Atras,C NA+","101Y",351.65,"kN",49.09,"kN",0.59,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Atras,C NA-","101S",-167.4,"kN",27.14,"kN",0.48,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Atras,C NA-","101X",164.62,"kN",27.18,"kN",0.44,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Atras,C NA-","101XY",367.54,"kN",46.79,"kN",0.37,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Atras,C NA-","101Y",7.58,"kN",6.84,"kN",0.35,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Del,C NA+","101S",351.63,"kN",49.09,"kN",0.59,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Del,C NA+","101X",24.64,"kN",16.02,"kN",0.56999999999999995,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Del,C NA+","101XY",-183.83,"kN",25.97,"kN",0.47,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 1 Susp Del,C NA+","101Y",180.17,"kN",24.55,"kN",0.48,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Del,C NA-","101S",7.55,"kN",6.85,"kN",0.35,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Del,C NA-","101X",367.78,"kN",46.81,"kN",0.37,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Del,C NA-","101XY",164.78,"kN",27.19,"kN",0.44,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 1 Susp Del,C NA-","101Y",-167.5,"kN",27.15,"kN",0.48,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Atras,C NA+","101S",164.69,"kN",26.89,"kN",0.46,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Atras,C NA+","101X",-167.45,"kN",27.45,"kN",0.46,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Atras,C NA+","101XY",7.61,"kN",6.68,"kN",0.38,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Atras,C NA+","101Y",367.49,"kN",46.57,"kN",0.35,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Atras,C NA-","101S",-184.04,"kN",25.85,"kN",0.45,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Atras,C NA-","101X",180.34,"kN",24.72,"kN",0.5,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Atras,C NA-","101XY",351.56,"kN",49.36,"kN",0.56999999999999995,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Atras,C NA-","101Y",24.48,"kN",15.79,"kN",0.59,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Del,C NA+","101S",367.73,"kN",46.59,"kN",0.35,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Del,C NA+","101X",7.58,"kN",6.69,"kN",0.38,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Del,C NA+","101XY",-167.55,"kN",27.45,"kN",0.46,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CM 2 Susp Del,C NA+","101Y",164.85,"kN",26.9,"kN",0.46,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Del,C NA-","101S",24.7,"kN",15.8,"kN",0.59,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Del,C NA-","101X",351.54,"kN",49.36,"kN",0.56999999999999995,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Del,C NA-","101XY",180.24,"kN",24.71,"kN",0.5,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CM 2 Susp Del,C NA-","101Y",-183.88,"kN",25.83,"kN",0.45,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Atras,C NA+","101S",201.08,"kN",25.19,"kN",0.36,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Atras,C NA+","101X",-159.47999999999999,"kN",24.45,"kN",0.48,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Atras,C NA+","101XY",-0.04,"kN",16.2,"kN",0.56000000000000005,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Atras,C NA+","101Y",330.77,"kN",46.78,"kN",0.48,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Atras,C NA-","101S",-146.04,"kN",24.58,"kN",0.38,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Atras,C NA-","101X",188.24,"kN",28.61,"kN",0.44,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Atras,C NA-","101XY",343.91,"kN",45.22,"kN",0.39,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Atras,C NA-","101Y",-13.79,"kN",4.68,"kN",0.24,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Del,C NA+","101S",330.76,"kN",46.79,"kN",0.48,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Del,C NA+","101X",0.18,"kN",16.2,"kN",0.56000000000000005,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Del,C NA+","101XY",-159.34,"kN",24.43,"kN",0.48,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 1 Susp Del,C NA+","101Y",201,"kN",25.19,"kN",0.36,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Del,C NA-","101S",-13.8,"kN",4.6900000000000004,"kN",0.24,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Del,C NA-","101X",344.13,"kN",45.24,"kN",0.39,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Del,C NA-","101XY",188.39,"kN",28.62,"kN",0.44,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 1 Susp Del,C NA-","101Y",-146.12,"kN",24.58,"kN",0.38,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Atras,C NA+","101S",188.31,"kN",28.32,"kN",0.47,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Atras,C NA+","101X",-146.08000000000001,"kN",24.88,"kN",0.36,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Atras,C NA+","101XY",-13.76,"kN",4.62,"kN",0.26,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Atras,C NA+","101Y",343.87,"kN",45.01,"kN",0.36,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Atras,C NA-","101S",-159.53,"kN",24.31,"kN",0.46,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Atras,C NA-","101X",201.14,"kN",25.39,"kN",0.38,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Atras,C NA-","101XY",330.69,"kN",47.05,"kN",0.46,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Atras,C NA-","101Y",0.02,"kN",15.96,"kN",0.59,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Del,C NA+","101S",344.09,"kN",45.03,"kN",0.36,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Del,C NA+","101X",-13.77,"kN",4.63,"kN",0.26,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Del,C NA+","101XY",-146.16,"kN",24.88,"kN",0.36,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","Rotura CI 2 Susp Del,C NA+","101Y",188.45,"kN",28.33,"kN",0.47,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Del,C NA-","101S",0.24,"kN",15.96,"kN",0.59,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Del,C NA-","101X",330.68,"kN",47.06,"kN",0.46,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Del,C NA-","101XY",201.06,"kN",25.38,"kN",0.38,"kN-m",0]
["T-9","d4s1_cadenav-aa_ed.b_v2.tow","-Rotura CI 2 Susp Del,C NA-","101Y",-159.38,"kN",24.3,"kN",0.46,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Viento,C NA+","117S",786.61,"kN",106.51,"kN",0.48,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Viento,C NA+","117X",-579.59,"kN",83.35,"kN",0.41,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Viento,C NA+","117XY",-581.87,"kN",83.65,"kN",0.41,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Viento,C NA+","117Y",784.29,"kN",106.24,"kN",0.49,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Viento,C NA-","117S",-579.44000000000005,"kN",82.02,"kN",0.56999999999999995,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Viento,C NA-","117X",786.47,"kN",108.1,"kN",0.26,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Viento,C NA-","117XY",784.14,"kN",107.84,"kN",0.26,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Viento,C NA-","117Y",-581.72,"kN",82.32,"kN",0.56999999999999995,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Hielo,C NA+","117S",131.56,"kN",15.94,"kN",0.02,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Hielo,C NA+","117X",131.56,"kN",15.94,"kN",0.02,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Hielo,C NA+","117XY",131.54,"kN",15.93,"kN",0.02,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Hielo,C NA+","117Y",131.55000000000001,"kN",15.94,"kN",0.02,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Viento+Hielo,C NA-","117S",-73.239999999999995,"kN",11.79,"kN",0.12,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Viento+Hielo,C NA-","117X",337.3,"kN",43.81,"kN",0.05,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Viento+Hielo,C NA-","117XY",337,"kN",43.78,"kN",0.06,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Viento+Hielo,C NA-","117Y",-73.489999999999995,"kN",11.84,"kN",0.13,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Viento+Hielo,C NA+","117S",337.31,"kN",43.54,"kN",0.1,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Viento+Hielo,C NA+","117X",-73.25,"kN",12.07,"kN",0.09,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Viento+Hielo,C NA+","117XY",-73.5,"kN",12.12,"kN",0.09,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Viento+Hielo,C NA+","117Y",337.01,"kN",43.52,"kN",0.1,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Tiro Vertical,C NA+","117S",98.41,"kN",12.03,"kN",0.01,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Tiro Vertical,C NA+","117X",98.41,"kN",12.03,"kN",0.01,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Tiro Vertical,C NA+","117XY",98.4,"kN",12.03,"kN",0.01,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Tiro Vertical,C NA+","117Y",98.4,"kN",12.03,"kN",0.01,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Desequilibrio Susp Atras,C NA+","117S",-43.86,"kN",3.17,"kN",0.18,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Desequilibrio Susp Atras,C NA+","117X",-460.57,"kN",57.87,"kN",0.11,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Desequilibrio Susp Atras,C NA+","117XY",310.86,"kN",34.97,"kN",0.28000000000000003,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Desequilibrio Susp Atras,C NA+","117Y",719.48,"kN",90.3,"kN",0.34,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Desequilibrio Susp Atras,C NA-","117S",-460.62,"kN",57.65,"kN",7.0000000000000007E-2,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Desequilibrio Susp Atras,C NA-","117X",-43.81,"kN",2.89,"kN",0.23,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Desequilibrio Susp Atras,C NA-","117XY",719.4,"kN",90.55,"kN",0.28999999999999998,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Desequilibrio Susp Atras,C NA-","117Y",310.93,"kN",35.159999999999997,"kN",0.31,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Desequilibrio Susp Del,C NA+","117S",719.14,"kN",90.26,"kN",0.34,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Desequilibrio Susp Del,C NA+","117X",310.22000000000003,"kN",34.89,"kN",0.27,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Desequilibrio Susp Del,C NA+","117XY",-461.6,"kN",58,"kN",0.11,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Desequilibrio Susp Del,C NA+","117Y",-44.64,"kN",3.26,"kN",0.18,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Desequilibrio Susp Del,C NA-","117S",310.3,"kN",35.08,"kN",0.31,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Desequilibrio Susp Del,C NA-","117X",719.06,"kN",90.51,"kN",0.28999999999999998,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Desequilibrio Susp Del,C NA-","117XY",-44.59,"kN",2.98,"kN",0.23,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Desequilibrio Susp Del,C NA-","117Y",-461.65,"kN",57.78,"kN",7.0000000000000007E-2,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CT1 Atras,C NA+","117S",223.41,"kN",30.14,"kN",0.27,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CT1 Atras,C NA+","117X",-184.52,"kN",23.25,"kN",0.14000000000000001,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CT1 Atras,C NA+","117XY",43.41,"kN",7.55,"kN",0.3,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CT1 Atras,C NA+","117Y",440.85,"kN",56.58,"kN",0.44,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CT1 Atras,C NA-","117S",-176.97,"kN",25.67,"kN",0.43,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CT1 Atras,C NA-","117X",216.46,"kN",32.07,"kN",0.26,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CT1 Atras,C NA-","117XY",443.2,"kN",54.75,"kN",0.14000000000000001,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CT1 Atras,C NA-","117Y",40.47,"kN",4.1100000000000003,"kN",0.26,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CT1 Del,C NA+","117S",440.36,"kN",56.48,"kN",0.44,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CT1 Del,C NA+","117X",43.67,"kN",7.48,"kN",0.28999999999999998,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CT1 Del,C NA+","117XY",-184.73,"kN",23.26,"kN",0.14000000000000001,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CT1 Del,C NA+","117Y",222.36,"kN",30,"kN",0.26,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CT1 Del,C NA-","117S",41.9,"kN",4.2,"kN",0.26,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CT1 Del,C NA-","117X",441.47,"kN",54.58,"kN",0.14000000000000001,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CT1 Del,C NA-","117XY",214.23,"kN",31.88,"kN",0.26,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CT1 Del,C NA-","117Y",-175.94,"kN",25.63,"kN",0.43,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CT2 Atras,C NA+","117S",216.6,"kN",31.8,"kN",0.3,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CT2 Atras,C NA+","117X",-177.02,"kN",25.96,"kN",0.38,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CT2 Atras,C NA+","117XY",40.5,"kN",3.84,"kN",0.31,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CT2 Atras,C NA+","117Y",443.09,"kN",54.49,"kN",0.09,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CT2 Atras,C NA-","117S",-184.55,"kN",23.04,"kN",0.09,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CT2 Atras,C NA-","117X",223.53,"kN",30.38,"kN",0.32,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CT2 Atras,C NA-","117XY",440.71,"kN",56.84,"kN",0.39,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CT2 Atras,C NA-","117Y",43.47,"kN",7.36,"kN",0.34,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CT2 Del,C NA+","117S",441.35,"kN",54.32,"kN",0.09,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CT2 Del,C NA+","117X",41.92,"kN",3.92,"kN",0.31,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CT2 Del,C NA+","117XY",-175.99,"kN",25.93,"kN",0.38,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CT2 Del,C NA+","117Y",214.37,"kN",31.61,"kN",0.31,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CT2 Del,C NA-","117S",43.72,"kN",7.3,"kN",0.33,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CT2 Del,C NA-","117X",440.22,"kN",56.75,"kN",0.39,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CT2 Del,C NA-","117XY",222.47,"kN",30.24,"kN",0.32,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CT2 Del,C NA-","117Y",-184.76,"kN",23.05,"kN",0.09,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CS 1  Susp Atras,C NA+","117S",225.64,"kN",30.16,"kN",0.38,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CS 1  Susp Atras,C NA+","117X",-193.98,"kN",24.65,"kN",0.28999999999999998,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CS 1  Susp Atras,C NA+","117XY",45.81,"kN",10.89,"kN",0.43,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CS 1  Susp Atras,C NA+","117Y",449.68,"kN",58.81,"kN",0.56999999999999995,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CS 1 Susp Atras,C NA-","117S",-186.43,"kN",27.21,"kN",0.46,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CS 1 Susp Atras,C NA-","117X",218.89,"kN",32.44,"kN",0.3,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CS 1 Susp Atras,C NA-","117XY",455.62,"kN",56.22,"kN",0.2,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CS 1 Susp Atras,C NA-","117Y",39.07,"kN",5.08,"kN",0.28999999999999998,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CS 1  Susp Del,C NA+","117S",450.24,"kN",58.84,"kN",0.56000000000000005,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CS 1  Susp Del,C NA+","117X",45.43,"kN",10.84,"kN",0.42,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CS 1  Susp Del,C NA+","117XY",-194.84,"kN",24.73,"kN",0.28999999999999998,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CS 1  Susp Del,C NA+","117Y",225.65,"kN",30.14,"kN",0.38,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CS 1 Susp Del,C NA-","117S",39.49,"kN",5.13,"kN",0.28999999999999998,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CS 1 Susp Del,C NA-","117X",455.38,"kN",56.2,"kN",0.21,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CS 1 Susp Del,C NA-","117XY",218.09,"kN",32.39,"kN",0.31,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CS 1 Susp Del,C NA-","117Y",-186.49,"kN",27.26,"kN",0.46,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CS 2 Susp Atras,C NA+","117S",219.02,"kN",32.17,"kN",0.35,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CS 2 Susp Atras,C NA+","117X",-186.52,"kN",27.52,"kN",0.41,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CS 2 Susp Atras,C NA+","117XY",39.14,"kN",4.8099999999999996,"kN",0.34,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CS 2 Susp Atras,C NA+","117Y",455.52,"kN",55.96,"kN",0.16,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CS 2 Susp Atras,C NA-","117S",-194.08,"kN",24.47,"kN",0.24,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CS 2 Susp Atras,C NA-","117X",225.77,"kN",30.38,"kN",0.43,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CS 2 Susp Atras,C NA-","117XY",449.52,"kN",59.08,"kN",0.51,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CS 2 Susp Atras,C NA-","117Y",45.94,"kN",10.7,"kN",0.47,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CS 2 Susp Del,C NA+","117S",455.28,"kN",55.94,"kN",0.16,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CS 2 Susp Del,C NA+","117X",39.56,"kN",4.8600000000000003,"kN",0.34,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CS 2 Susp Del,C NA+","117XY",-186.58,"kN",27.57,"kN",0.41,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CS 2 Susp Del,C NA+","117Y",218.21,"kN",32.119999999999997,"kN",0.36,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CS 2 Susp Del,C NA-","117S",45.56,"kN",10.64,"kN",0.47,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CS 2 Susp Del,C NA-","117X",450.08,"kN",59.11,"kN",0.51,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CS 2 Susp Del,C NA-","117XY",225.78,"kN",30.37,"kN",0.43,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CS 2 Susp Del,C NA-","117Y",-194.95,"kN",24.55,"kN",0.24,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CM 1 Susp Atras,C NA+","117S",244.93,"kN",31.42,"kN",0.39,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CM 1 Susp Atras,C NA+","117X",-176.12,"kN",23.92,"kN",0.42,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CM 1 Susp Atras,C NA+","117XY",27.95,"kN",13.47,"kN",0.53,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CM 1 Susp Atras,C NA+","117Y",430.39,"kN",57.72,"kN",0.57999999999999996,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CM 1 Susp Atras,C NA-","117S",-166.95,"kN",26.31,"kN",0.48,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CM 1 Susp Atras,C NA-","117X",236.62,"kN",34.67,"kN",0.42,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CM 1 Susp Atras,C NA-","117XY",437.84,"kN",54.91,"kN",0.33,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CM 1 Susp Atras,C NA-","117Y",19.649999999999999,"kN",5.16,"kN",0.28000000000000003,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CM 1 Susp Del,C NA+","117S",431.02,"kN",57.76,"kN",0.56999999999999995,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CM 1 Susp Del,C NA+","117X",27.5,"kN",13.43,"kN",0.53,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CM 1 Susp Del,C NA+","117XY",-177.07,"kN",24,"kN",0.42,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CM 1 Susp Del,C NA+","117Y",245,"kN",31.41,"kN",0.39,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CM 1 Susp Del,C NA-","117S",20.149999999999999,"kN",5.21,"kN",0.28000000000000003,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CM 1 Susp Del,C NA-","117X",437.51,"kN",54.89,"kN",0.33,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CM 1 Susp Del,C NA-","117XY",235.72,"kN",34.619999999999997,"kN",0.42,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CM 1 Susp Del,C NA-","117Y",-166.93,"kN",26.36,"kN",0.48,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CM 2 Susp Atras,C NA+","117S",236.77,"kN",34.39,"kN",0.47,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CM 2 Susp Atras,C NA+","117X",-167.07,"kN",26.63,"kN",0.43,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CM 2 Susp Atras,C NA+","117XY",19.75,"kN",4.9400000000000004,"kN",0.33,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CM 2 Susp Atras,C NA+","117Y",437.71,"kN",54.66,"kN",0.28000000000000003,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CM 2 Susp Atras,C NA-","117S",-176.25,"kN",23.77,"kN",0.37,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CM 2 Susp Atras,C NA-","117X",245.08,"kN",31.65,"kN",0.44,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CM 2 Susp Atras,C NA-","117XY",430.21,"kN",57.98,"kN",0.52,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CM 2 Susp Atras,C NA-","117Y",28.11,"kN",13.25,"kN",0.57999999999999996,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CM 2 Susp Del,C NA+","117S",437.38,"kN",54.64,"kN",0.28000000000000003,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CM 2 Susp Del,C NA+","117X",20.25,"kN",4.9800000000000004,"kN",0.34,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CM 2 Susp Del,C NA+","117XY",-167.06,"kN",26.67,"kN",0.43,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CM 2 Susp Del,C NA+","117Y",235.87,"kN",34.340000000000003,"kN",0.47,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CM 2 Susp Del,C NA-","117S",27.65,"kN",13.2,"kN",0.57999999999999996,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CM 2 Susp Del,C NA-","117X",430.84,"kN",58.02,"kN",0.52,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CM 2 Susp Del,C NA-","117XY",245.16,"kN",31.64,"kN",0.44,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CM 2 Susp Del,C NA-","117Y",-177.2,"kN",23.85,"kN",0.36,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CI 1 Susp Atras,C NA+","117S",262.41000000000003,"kN",32.39,"kN",0.28000000000000003,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CI 1 Susp Atras,C NA+","117X",-156.53,"kN",22.7,"kN",0.43,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CI 1 Susp Atras,C NA+","117XY",8.48,"kN",13.59,"kN",0.53,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CI 1 Susp Atras,C NA+","117Y",412.79,"kN",55.89,"kN",0.47,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CI 1 Susp Atras,C NA-","117S",-149.25,"kN",24.24,"kN",0.39,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CI 1 Susp Atras,C NA-","117X",255.7,"kN",35.880000000000003,"kN",0.42,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CI 1 Susp Atras,C NA-","117XY",418.81,"kN",53.67,"kN",0.34,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CI 1 Susp Atras,C NA-","117Y",1.9,"kN",2.98,"kN",0.17,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CI 1 Susp Del,C NA+","117S",413.33,"kN",55.92,"kN",0.47,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CI 1 Susp Del,C NA+","117X",8.11,"kN",13.55,"kN",0.52,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CI 1 Susp Del,C NA+","117XY",-157.4,"kN",22.78,"kN",0.43,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CI 1 Susp Del,C NA+","117Y",262.38,"kN",32.369999999999997,"kN",0.28000000000000003,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CI 1 Susp Del,C NA-","117S",2.3199999999999998,"kN",3.01,"kN",0.17,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CI 1 Susp Del,C NA-","117X",418.55,"kN",53.65,"kN",0.34,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CI 1 Susp Del,C NA-","117XY",254.87,"kN",35.82,"kN",0.43,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CI 1 Susp Del,C NA-","117Y",-149.32,"kN",24.29,"kN",0.39,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CI 2 Susp Atras,C NA+","117S",255.83,"kN",35.590000000000003,"kN",0.48,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CI 2 Susp Atras,C NA+","117X",-149.36000000000001,"kN",24.55,"kN",0.34,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CI 2 Susp Atras,C NA+","117XY",1.98,"kN",2.83,"kN",0.23,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CI 2 Susp Atras,C NA+","117Y",418.7,"kN",53.43,"kN",0.28999999999999998,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CI 2 Susp Atras,C NA-","117S",-156.65,"kN",22.55,"kN",0.38,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CI 2 Susp Atras,C NA-","117X",262.55,"kN",32.630000000000003,"kN",0.33,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CI 2 Susp Atras,C NA-","117XY",412.63,"kN",56.14,"kN",0.42,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CI 2 Susp Atras,C NA-","117Y",8.6199999999999992,"kN",13.35,"kN",0.57999999999999996,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CI 2 Susp Del,C NA+","117S",418.44,"kN",53.41,"kN",0.28999999999999998,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CI 2 Susp Del,C NA+","117X",2.4,"kN",2.86,"kN",0.23,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CI 2 Susp Del,C NA+","117XY",-149.43,"kN",24.6,"kN",0.35,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","Rotura CI 2 Susp Del,C NA+","117Y",255,"kN",35.54,"kN",0.48,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CI 2 Susp Del,C NA-","117S",8.25,"kN",13.31,"kN",0.56999999999999995,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CI 2 Susp Del,C NA-","117X",413.17,"kN",56.18,"kN",0.42,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CI 2 Susp Del,C NA-","117XY",262.52,"kN",32.619999999999997,"kN",0.33,"kN-m",0]
["T-10","d4s2_cadenav-ac_ed.a_v1.tow","-Rotura CI 2 Susp Del,C NA-","117Y",-157.52000000000001,"kN",22.64,"kN",0.38,"kN-m",0]

{"sheet":"PLSLinea","index":1,"n_rows":11,"n_cols":36,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["structure_number","station","units3","height_adjust","units4","units5","units6","x_easting","units7","y_northing","units8","centerline_z_elevation","units9","units10","ahead_span","units11","line_angle","units12","sets_in_xy_structure_line_angle_calculation","transverse_axis_azimuth","units13","structure_name","structure_description","struct_height","units14","units15","structure_specific_material","units16","automatic_structure_group_membership","manual_structure_group_membership","structure_comment_1","structure_comment_2","structure_comment_3","structure_comment_4","structure_comment_5","structure_comment_6"]
["T-1",69.742000000000004,"m",0.03,"m","m","deg",522205.00900000002,"m",4156947.49,"m",711.524,"m","m",330.26900000000001,"m","0.0012","deg","1-60",350.94990000000001,"deg","F:\\Cimentaciones\\Cimentaciones DIL\\XLM\\XML Baza Caparacena\\d4a4f-aa-vidrio_ed.l_v3.tow","D4A4F-AA",49.375,"m","m",0,"N","'All', 'Has DE', 'All sets DE', 'Angle', 'TOWER', 'TOWER has DE', 'TOWER angle'",null,"T-1"]
["T-2",400.01100000000002,"m",0.51,"m","m","deg",521878.85100000002,"m",4156895.5430000001,"m",712.65599999999995,"m","m",417.97699999999998,"m","35.8875","deg","1-60",8.8942999999999994,"deg","F:\\Cimentaciones\\Cimentaciones DIL\\XLM\\XML Baza Caparacena\\d4a4a-ab-vidrio_ed.l_v3.tow","D4A4A-AB",54.375,"m","m",0,"N","'All', 'Has DE', 'All sets DE', 'Angle', 'TOWER', 'TOWER has DE', 'TOWER angle'",null,"T-2"]
["T-3",817.98800000000006,"m",0.06,"m","m","deg",521505.89600000001,"m",4157084.247,"m",715.34199999999998,"m","m",344.97500000000002,"m",null,"deg","1-60",26.838100000000001,"deg","F:\\Cimentaciones\\Cimentaciones DIL\\XLM\\XML Baza Caparacena\\d4s1_cadenav-aa_ed.b_v2.tow","D4S1V-AA",50.43,"m","m",0,"N","'All', 'No DE', 'Not all sets DE', 'TOWER', 'TOWER no DE'",null,"T-3"]
["T-4",1162.963,"m",7.0000000000000007E-2,"m","m","deg",521198.08000000002,"m",4157239.9929999998,"m",717.54399999999998,"m","m",289.44600000000003,"m","32.6617","deg","1-60",43.168900000000001,"deg","F:\\Cimentaciones\\Cimentaciones DIL\\XLM\\XML Baza Caparacena\\d4a3-aa-vidrio_ed.g_v4.tow","D4A3-AA",49.375,"m","m",0,"N","'All', 'Has DE', 'All sets DE', 'Angle', 'TOWER', 'TOWER has DE', 'TOWER angle'",null,"T-4","ANC"]
["T-5",1452.4090000000001,"m",0.08,"m","m","deg",521051.174,"m",4157489.3879999998,"m",718.97900000000004,"m","m",350.84100000000001,"m",null,"deg","1-60",59.499699999999997,"deg","F:\\Cimentaciones\\Cimentaciones DIL\\XLM\\XML Baza Caparacena\\d4s1_cadenav-aa_ed.b_v2.tow","D4S1V-AA",50.43,"m","m",0,"N","'All', 'No DE', 'Not all sets DE', 'TOWER', 'TOWER no DE'",null,"T-5"]
["T-6",1803.25,"m",0.18,"m","m","deg",520873.10700000002,"m",4157791.682,"m",707.11800000000005,"m","m",480.59199999999998,"m","38.5126","deg","1-60",78.756,"deg","F:\\Cimentaciones\\Cimentaciones DIL\\XLM\\XML Baza Caparacena\\d4a4a-a0-vidrio_ed.l_v3.tow","D4A4A-A0",44.375,"m","m",0,"N","'All', 'Has DE', 'All sets DE', 'Angle', 'TOWER', 'TOWER has DE', 'TOWER angle'",null,"T-6","ANC"]
["T-7",2283.8420000000001,"m",0.04,"m","m","deg",520940.09499999997,"m",4158267.5819999999,"m",704.57899999999995,"m","m",397.10199999999998,"m",null,"deg","1-60",98.012299999999996,"deg","F:\\Cimentaciones\\Cimentaciones DIL\\XLM\\XML Baza Caparacena\\d4s1_cadenav-ac_ed.b_v2.tow","D4S1V-AC",60.43,"m","m",0,"N","'All', 'No DE', 'Not all sets DE', 'TOWER', 'TOWER no DE'",null,"T-7"]
["T-8",2680.944,"m",0.04,"m","m","deg",520995.44500000001,"m",4158660.8080000002,"m",704.88599999999997,"m","m",519.32500000000005,"m",null,"deg","1-60",98.012299999999996,"deg","F:\\Cimentaciones\\Cimentaciones DIL\\XLM\\XML Baza Caparacena\\d4s1_cadenav-aa_ed.b_v2.tow","D4S1V-AA",50.43,"m","m",0,"N","'All', 'No DE', 'Not all sets DE', 'TOWER', 'TOWER no DE'",null,"T-8"]
["T-9",3200.2689999999998,"m",7.0000000000000007E-2,"m","m","deg",521067.83199999999,"m",4159175.0630000001,"m",700.86900000000003,"m","m",569.19899999999996,"m",null,"deg","1-60",98.012299999999996,"deg","F:\\Cimentaciones\\Cimentaciones DIL\\XLM\\XML Baza Caparacena\\d4s1_cadenav-aa_ed.b_v2.tow","D4S1V-AA",50.43,"m","m",0,"N","'All', 'No DE', 'Not all sets DE', 'TOWER', 'TOWER no DE'",null,"T-9"]
["T-10",3769.4679999999998,"m",0.05,"m","m","deg",521147.17,"m",4159738.7059999998,"m",700.02599999999995,"m","m",678.23,"m",null,"deg","1-60",98.012299999999996,"deg","F:\\Cimentaciones\\Cimentaciones DIL\\XLM\\XML Baza Caparacena\\d4s2_cadenav-ac_ed.a_v1.tow","D4S2V-AC",60.43,"m","m",0,"N","'All', 'No DE', 'Not all sets DE', 'TOWER', 'TOWER no DE'",null,"T-10"]

{"sheet":"INLI_ObraCivil","index":2,"n_rows":288,"n_cols":27,"rows_kept":288,"cut":false,"hidden":true,"merged":[[12,26,12,27],[13,26,13,27],[14,26,14,27],[15,26,15,27],[16,26,16,27],[17,26,17,27],[9,1,9,27],[10,13,10,16],[10,17,10,20],[10,21,10,24],[11,6,11,9],[11,26,11,27],[24,26,24,27],[25,26,25,27],[26,26,26,27],[27,26,27,27],[28,26,28,27],[29,26,29,27],[18,26,18,27],[19,26,19,27],[20,26,20,27],[21,26,21,27],[22,26,22,27],[23,26,23,27],[36,26,36,27],[37,26,37,27],[38,26,38,27],[39,26,39,27],[40,26,40,27],[41,26,41,27],[30,26,30,27],[31,26,31,27],[32,26,32,27],[33,26,33,27],[34,26,34,27],[35,26,35,27],[48,26,48,27],[49,26,49,27],[50,26,50,27],[51,26,51,27],[52,26,52,27],[53,26,53,27],[42,26,42,27],[43,26,43,27],[44,26,44,27],[45,26,45,27],[46,26,46,27],[47,26,47,27],[60,26,60,27],[61,26,61,27],[62,26,62,27],[63,26,63,27],[64,26,64,27],[65,26,65,27],[54,26,54,27],[55,26,55,27],[56,26,56,27],[57,26,57,27],[58,26,58,27],[59,26,59,27],[72,26,72,27],[73,26,73,27],[74,26,74,27],[75,26,75,27],[76,26,76,27],[77,26,77,27],[66,26,66,27],[67,26,67,27],[68,26,68,27],[69,26,69,27],[70,26,70,27],[71,26,71,27],[84,26,84,27],[85,26,85,27],[86,26,86,27],[87,26,87,27],[88,26,88,27],[89,26,89,27],[78,26,78,27],[79,26,79,27],[80,26,80,27],[81,26,81,27],[82,26,82,27],[83,26,83,27],[96,26,96,27],[97,26,97,27],[98,26,98,27],[99,26,99,27],[100,26,100,27],[101,26,101,27],[90,26,90,27],[91,26,91,27],[92,26,92,27],[93,26,93,27],[94,26,94,27],[95,26,95,27],[108,26,108,27],[109,26,109,27],[110,26,110,27],[111,26,111,27],[112,26,112,27],[113,26,113,27],[102,26,102,27],[103,26,103,27],[104,26,104,27],[105,26,105,27],[106,26,106,27],[107,26,107,27],[120,26,120,27],[121,26,121,27],[122,26,122,27],[123,26,123,27],[124,26,124,27],[125,26,125,27],[114,26,114,27],[115,26,115,27],[116,26,116,27],[117,26,117,27],[118,26,118,27],[119,26,119,27],[132,26,132,27],[133,26,133,27],[134,26,134,27],[135,26,135,27],[136,26,136,27],[137,26,137,27],[126,26,126,27],[127,26,127,27],[128,26,128,27],[129,26,129,27],[130,26,130,27],[131,26,131,27],[144,26,144,27],[145,26,145,27],[146,26,146,27],[147,26,147,27],[148,26,148,27],[149,26,149,27],[138,26,138,27],[139,26,139,27],[140,26,140,27],[141,26,141,27],[142,26,142,27],[143,26,143,27],[156,26,156,27],[157,26,157,27],[158,26,158,27],[159,26,159,27],[160,26,160,27],[161,26,161,27],[150,26,150,27],[151,26,151,27],[152,26,152,27],[153,26,153,27],[154,26,154,27],[155,26,155,27],[174,26,174,27],[168,26,168,27],[169,26,169,27],[170,26,170,27],[171,26,171,27],[172,26,172,27],[173,26,173,27],[162,26,162,27],[163,26,163,27],[164,26,164,27],[165,26,165,27],[166,26,166,27],[167,26,167,27]]}
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Departamento de Ingeniería de Líneas"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"05/08/2020"]
[]
[null,"Proyecto de línea",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Edición"]
[null,"Código: J-0054-L0772",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Número:  1"]
[null,"Descripción Línea: Fuendetodos -Mezquita",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fecha: 10/02/2011"]
[null,"Tensión (kV): 400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Tipo: Alternativa de proyecto"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Descripción: Migración"]
[null,"DATOS OBRA CIVIL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Nivelaciones consideradas (cm)",null,null,null,"Explanaciones (cm)",null,null,null,"Realces (cm)"]
[null,"Nº Apoyo","Tipología","Tipo de Apoyo","Apoyo (Observaciones)","Cód. Altura norm","Patas (cm)","Patas (cm)","Patas (cm)","Patas (cm)","Cimentación","Toma de Tierra","Tomar Cota (cm)","Pata 1","Pata 2","Pata 3","Pata 4","Pata 1","Pata 2","Pata 3","Pata 4","Pata 1","Pata 2","Pata 3","Pata 4","Hormigonado/Apoyo (m3)","Excavación/Apoyo (m3)"]
[null,"1","A","APOYO D4A2",null,"A0","0","0","0","0","PEN","F",-1,-10,-1,-11,-7,0,0,0,0,null,null,null,null,41.36,40.119999999999997]
[null,"2","A","APOYO D4A4F",null,"AA","0","0","M","M","PEN","NF",30,27,22,-38,-44,0,0,14,10,null,null,null,null,105.04,103.52]
[null,"3","S","APOYO D4S2",null,"A0","M","0","M","+","PEN","NF",66,-18,61,-18,-100,0,0,0,0,null,null,null,null,30.48,29.68]
[null,"4","S","APOYO D4S2",null,"AB","P","M","L","0","PEN","NF",47,148,-46,-212,19,18,0,0,0,null,null,null,25,30.48,29.68]
[null,"5","S","APOYO D4S2",null,"AD","0","M","M","0","PEN","NF",34,32,-32,-50,1,0,16,0,0,null,null,null,50,30.48,29.68]
[null,"6","A","APOYO D4A3",null,"AA","M","M","0","0","PEN","NF",29,-54,-44,24,5,0,10,0,1,null,null,null,75,66.08,64.84]
[null,"7","S","APOYO D4S2",null,"AE","P","M","+","0","PEN","NF",27,75,-64,-134,28,0,0,4,1,25,null,null,100,30.48,29.68]
[null,"8","S","APOYO D4S2",null,"AD","0","0","0","0","PEN","NF",-7,-7,-17,-16,-17,0,0,0,0,null,null,null,null,30.48,29.68]
[null,"9","S","APOYO D4S2",null,"AC","0","0","0","0","PEN","NF",-4,-14,-10,-4,4,0,0,0,8,null,null,null,null,30.48,29.68]
[null,"10","S","APOYO D4S1",null,"AC","+",0,0,0,"PEN","NF",-8,0,-14,-18,-14,8,0,0,0,75,null,null,null,25.04,24.24]
[null,"11","A","APOYO D4A3",null,"AE","0","0","0","0","PEN","NF",16,-19,-15,17,-17,0,0,1,0,25,25,null,25,66.08,64.84]
[null,"12","S","APOYO D4S2",null,"AF","0","0","0","0","PEN","NF",12,-23,-14,21,7,0,0,9,0,25,25,null,null,30.48,29.68]
[null,"13","S","APOYO D4S1",null,"AB","0","0","0","0","PEN","NF",1,-1,-5,-26,-23,0,0,0,1,null,null,25,25,25.04,24.24]
[null,"14","S","APOYO D4S1",null,"AC","0","0","0","0","PEN","NF",7,-20,2,1,-18,0,0,0,0,25,null,null,25,25.04,24.24]
[null,"15","S","APOYO D4S2",null,"AD","0","0","0","0","PEN","NF",-1,9,-6,-36,-10,10,0,0,0,null,null,25,null,30.48,29.68]
[null,"16","A","APOYO D4A3",null,"AC","0","0","0","0","PEN","NF",8,-27,9,12,-17,0,1,4,0,25,null,null,25,66.08,64.84]
[null,"17","S","APOYO D4S1",null,"AC","0","0","0","0","PEN","NF",9,-26,-25,16,12,0,0,7,3,25,25,null,null,25.04,24.24]
[null,"18","S","APOYO D4S1",null,"AB","0","0","0","0","PEN","NF",-10,-13,-3,-20,-11,0,7,0,0,null,null,null,null,25.04,24.24]
[null,"19","S","APOYO D4S1",null,"AA","M","M","0","0","PEN","NF",17,-46,-44,-5,10,20,22,3,0,null,null,25,null,25.04,24.24]
[null,"20","S","APOYO D4S1",null,"AA","0","0","0","0","PEN","NF",0,0,0,0,0,0,0,0,0,null,null,null,null,25.04,24.24]
[null,"21","S","APOYO D4S1",null,"AB","0","0","0","0","PEN","NF",3,-28,-1,8,-7,0,0,5,0,25,null,null,null,25.04,24.24]
[null,"22","S","APOYO D4S2",null,"AC","0","0","0","0","PEN","NF",1,-9,15,13,-33,0,14,12,0,null,null,null,25,30.48,29.68]
[null,"23","S","APOYO D4S2",null,"AB","0","0","0","0","PEN","NF",0,0,0,0,0,0,0,0,0,null,null,null,null,30.48,29.68]
[null,"24","A","APOYO D4A4A",null,"A0","0","0","0","0","PEN","NF",-2,-34,-12,20,0,0,0,22,2,25,null,null,null,105.04,103.52]
[null,"25","S","APOYO D4S1",null,"AA","M","0","0","0","PEN","NF",34,-33,24,30,-24,16,0,0,0,null,null,null,50,25.04,24.24]
[null,"26","S","APOYO D4S1",null,"AB","0","M","M","0","PEN","NF",44,13,-40,-38,38,0,0,0,0,25,null,null,null,25.04,24.24]
[null,"27","S","APOYO D4S2",null,"AF","0","M","M","0","PEN","NF",43,48,-25,-62,8,5,15,4,0,null,null,25,25,30.48,29.68]
[null,"28","S","APOYO D4S2",null,"AB","*","*","0","0","PEN","NF",122,-220,-190,129,112,0,20,7,0,null,null,null,null,30.48,29.68]
[null,"29","S","APOYO D4S2",null,"AE","0","P","0","M","PEN","NF",-13,-15,45,-16,-99,0,0,0,0,null,25,null,null,30.48,29.68]
[null,"30","A","APOYO D4A4A",null,"AD","0","0","0","0","PEN","NF",12,-12,-17,13,2,1,0,1,0,25,25,null,null,105.04,103.52]
[null,"31","S","APOYO D4S1",null,"AD","0","M","M","0","PEN","NF",44,45,-46,-74,10,1,0,0,0,null,null,25,25,25.04,24.24]
[null,"32","S","APOYO D4S1",null,"AB","0","M","M","0","PEN","NF",24,-7,-60,-30,14,0,0,29,0,25,null,null,null,25.04,24.24]
[null,"33","S","APOYO D4S1",null,"AA","0","0","0","0","PEN","NF",10,-15,-20,9,3,0,0,0,0,25,25,null,null,25.04,24.24]
[null,"34","S","APOYO D4S1",null,"AA","0","0","0","0","PEN","NF",7,-28,-21,10,-3,0,0,3,0,25,25,null,null,25.04,24.24]
[null,"35","S","APOYO D4S1",null,"AB","0","0","0","0","PEN","NF",-7,-34,-17,-7,-7,0,0,0,0,25,null,null,null,25.04,24.24]
[null,"36","S","APOYO D4S1",null,"AA","0","0","0","0","PEN","NF",0,0,0,0,0,0,0,0,0,null,null,null,null,25.04,24.24]
[null,"37","S","APOYO D4S1",null,"AB","P","0","+","0","PEN","NF",9,108,8,-166,-25,16,0,0,0,null,null,null,25,25.04,24.24]
[null,"38","S","APOYO D4S2",null,"AD","0","0","0","0","PEN","NF",5,-27,5,4,-25,0,0,0,0,25,null,null,25,30.48,29.68]
[null,"39","S","APOYO D4S1",null,"AE","P","0","0","0","PEN","NF",5,33,-20,-27,0,0,0,0,0,50,25,25,null,25.04,24.24]
[null,"40","S","APOYO D4S1",null,"AB","0","0","0","0","PEN","NF",-10,-9,-17,-20,3,1,0,0,13,null,null,null,null,25.04,24.24]
[null,"41","S","APOYO D4S1",null,"AA","0","0","M","M","PEN","NF",55,-2,47,-20,-63,0,0,8,0,50,null,null,25,25.04,24.24]
[null,"42","A","APOYO D4A3",null,"AA","0","0","0","0","PEN","NF",-7,-15,-6,-17,-31,0,1,0,1,null,null,null,25,66.08,64.84]
[null,"43","S","APOYO D4S2",null,"AE","0","0","0","+","PEN","NF",5,7,28,-24,-170,2,23,0,0,null,null,25,null,30.48,29.68]
[null,"44","S","APOYO D4S2",null,"AE","0","0","0","0","PEN","NF",5,-21,-20,1,0,0,0,0,0,25,25,null,null,30.48,29.68]
[null,"45","S","APOYO D4S2",null,"AC","0","0","0","0","PEN","NF",-5,-15,-7,-15,-3,0,0,0,2,null,null,null,null,30.48,29.68]
[null,"46","S","APOYO D4S1",null,"AC","0","0","0","0","PEN","NF",-5,-15,7,2,-14,0,12,7,0,null,null,null,null,25.04,24.24]
[null,"47","S","APOYO D4S1",null,"AA","0","0","M","M","PEN","NF",13,3,15,-62,-54,0,2,8,16,null,null,null,null,25.04,24.24]
[null,"48","S","APOYO D4S1",null,"AC","0","0","M","M","PEN","NF",56,68,32,-61,-37,12,1,0,0,null,25,25,null,25.04,24.24]
[null,"49","S","APOYO D4S1",null,"AB","0","0","0","0","PEN","NF",4,8,11,-31,-30,4,7,0,0,null,null,25,25,25.04,24.24]
[null,"50","S","APOYO D4S1",null,"AD","0","0","0","0","PEN","NF",-7,-5,-17,-33,-13,2,0,0,0,null,null,25,null,25.04,24.24]
[null,"51","S","APOYO D4S1",null,"AC","0","0","0","0","PEN","NF",-1,17,-2,-36,-8,18,0,0,0,null,null,25,null,25.04,24.24]
[null,"52","A","APOYO D4A3",null,"AC","0","0","0","0","PEN","NF",4,12,-31,-28,11,8,0,0,7,null,25,25,null,66.08,64.84]
[null,"53","S","APOYO D4S1",null,"AC","M","0","0","M","PEN","NF",21,-50,11,20,-44,12,0,0,18,null,null,null,null,25.04,24.24]
[null,"54","S","APOYO D4S1",null,"AD","0","0","P","0","PEN","NF",-10,-45,-28,13,-18,0,7,0,0,25,25,50,null,25.04,24.24]
[null,"55","S","APOYO D4S2",null,"AC","0","M","0","0","PEN","NF",28,-3,-48,-7,40,0,8,0,12,25,null,25,null,30.48,29.68]
[null,"56","A","APOYO D4A3",null,"AB","0","0","0","0","PEN","NF",-1,-10,3,18,-11,0,4,19,0,null,null,null,null,66.08,64.84]
[null,"57","S","APOYO D4S2",null,"AD","0","0","0","0","PEN","NF",8,-27,-19,18,4,0,0,10,0,25,25,null,null,30.48,29.68]
[null,"58","S","APOYO D4S1",null,"AB","+","M","0","M","PEN","NF",58,-110,-60,55,-12,0,0,0,14,null,25,null,null,25.04,24.24]
[null,"59","S","APOYO D4S2",null,"AA","0","0","M","0","PEN","NF",1,22,-4,-92,-29,21,0,0,0,null,null,null,25,30.48,29.68]
[null,"60","S","APOYO D4S2",null,"AD","M","0","0","0","PEN","NF",19,-41,-7,19,9,23,0,0,0,null,25,null,null,30.48,29.68]
[null,"61","S","APOYO D4S1",null,"AD","+","0","0","M","PEN","NF",16,-144,26,-19,-96,6,10,0,0,null,null,25,25,25.04,24.24]
[null,"62","A","APOYO D4A3",null,"A0","M","M","0","0","PEN","NF",31,-110,-87,38,21,0,0,7,0,50,25,null,null,66.08,64.84]
[null,"63","S","APOYO D4S1",null,"AA","+","L","0","P","PEN","NF",55,-116,-228,55,128,0,0,0,0,null,25,null,null,25.04,24.24]
[null,"64","S","APOYO D4S1",null,"AC","*","+","0","M","PEN","NF",154,-213,-10,178,64,0,2,24,0,25,null,null,null,25.04,24.24]
[null,"65","S","APOYO D4S1",null,"AB","0","M","0","0","PEN","NF",19,-12,-45,9,26,0,19,0,7,25,null,null,null,25.04,24.24]
[null,"66","A","APOYO D4A4A",null,"A0","0","0","0","0","PEN","NF",-11,-40,-17,-34,-42,0,0,2,0,25,null,25,25,105.04,103.52]
[null,"67","S","APOYO D4S1",null,"AB","0","P","M","M","PEN","NF",-2,-1,46,-74,-90,1,0,10,0,null,25,null,null,25.04,24.24]
[null,"68","S","APOYO D4S1",null,"AA","0","0","0","0","PEN","NF",1,0,3,-8,-9,0,2,0,0,null,null,null,null,25.04,24.24]
[null,"69","S","APOYO D4S1",null,"AA","0","0","0","0","PEN","NF",7,7,1,-22,-20,0,0,0,0,null,null,25,25,25.04,24.24]
[null,"70","S","APOYO D4S2",null,"AD","0","0","0","0","PEN","NF",-9,10,-39,-44,1,19,0,0,10,null,25,25,null,30.48,29.68]
[null,"71","S","APOYO D4S2",null,"AD","+","0","0","+","PEN","NF",69,-116,34,72,-100,6,0,3,0,25,25,null,null,30.48,29.68]
[null,"72","A","APOYO D4A3",null,"AA","0","0","0","0","PEN","NF",-8,-6,-43,-11,-34,2,0,0,0,null,25,null,25,66.08,64.84]
[null,"73","S","APOYO D4S2",null,"AE","0","0","M","+","PEN","NF",28,26,28,-76,-118,0,0,4,20,null,null,25,null,30.48,29.68]
[null,"74","S","APOYO D4S1",null,"AC","0","0","+","+","PEN","NF",68,69,45,-128,-108,1,2,0,0,null,25,25,null,25.04,24.24]
[null,"75","S","APOYO D4S1",null,"AB","0","0","M","M","PEN","NF",42,39,8,-71,-41,0,0,0,0,null,25,25,null,25.04,24.24]
[null,"76","S","APOYO D4S1",null,"AC","P","0","+","M","PEN","NF",12,97,18,-154,-81,2,6,0,0,null,null,null,null,25.04,24.24]
[null,"77","A","APOYO D4A3",null,"AD","M","0","P","M","PEN","NF",0,-104,8,48,-82,4,8,0,0,25,null,25,null,66.08,64.84]
[null,"78","S","APOYO D4S1",null,"AC","P","P","+","M","PEN","NF",2,100,51,-190,-90,16,0,0,0,null,25,25,null,25.04,24.24]
[null,"79","S","APOYO D4S2",null,"AE","M","0","P","0","PEN","NF",-10,-118,-20,22,-43,0,0,0,0,25,null,50,25,30.48,29.68]
[null,"80","S","APOYO D4S2",null,"AE","0","0","0","0","PEN","NF",29,-6,21,31,8,0,0,2,4,25,null,null,25,30.48,29.68]
[null,"81","S","APOYO D4S1",null,"AC","0","0","0","0","PEN","NF",-2,-7,-1,2,-12,0,1,4,0,null,null,null,null,25.04,24.24]
[null,"82","A","APOYO D4A4F",null,"AD","0","0","0","0","PEN","NF",-10,-15,-4,-12,-20,0,6,0,0,null,null,null,null,105.04,103.52]
[null,"83","A","APOYO D4A3",null,"AC","0","0","0","0","PEN","NF",0,0,0,0,0,0,0,0,0,null,null,null,null,66.08,64.84]
[null,"84","A","APOYO D4A4F",null,"A0","0","0","+","M","PEN","NF",54,51,35,-108,-59,0,6,4,0,null,25,null,25,105.04,103.52]
[null,"85","S","APOYO D4S1",null,"A0","0","M","M","0","PEN","NF",22,18,-44,-70,14,0,16,0,0,null,null,null,null,25.04,24.24]
[null,"86","S","APOYO D4S2",null,"AC","M","0","+","L","PEN","NF",64,-14,54,-130,-176,5,0,0,10,null,null,25,null,30.48,29.68]
[null,"87","S","APOYO D4S2",null,"AD","0","0","0","0","PEN","NF",-10,-20,-15,8,-6,0,0,18,4,null,null,null,null,30.48,29.68]
[null,"88","A","APOYO D4A3",null,"AD","0","M","0","0","PEN","NF",58,23,-31,-2,62,0,0,0,4,25,null,50,null,66.08,64.84]
[null,"89","S","APOYO D4S2",null,"AC","M","M","0","0","PEN","NF",0,-118,-68,8,5,0,14,8,5,25,null,null,null,30.48,29.68]
[null,"90","S","APOYO D4S2",null,"AE","0","0","+","+","PEN","NF",40,42,19,-126,-160,2,4,0,0,null,25,null,25,30.48,29.68]
[null,"91","S","APOYO D4S1",null,"AC","M","0","P","0","PEN","NF",2,-83,-7,30,-23,0,0,0,0,null,null,50,25,25.04,24.24]
[null,"92","A","APOYO D4A3",null,"AA","0","0","0","0","PEN","NF",22,13,22,-11,-9,0,0,0,0,null,null,25,25,66.08,64.84]
[null,"93","S","APOYO D4S1",null,"AA","0","0","M","0","PEN","NF",-4,-28,-33,-65,-8,1,0,22,0,25,25,null,null,25.04,24.24]
[null,"94","S","APOYO D4S1",null,"AD","M","M","0","0","PEN","NF",49,-66,-14,47,39,0,20,0,0,25,null,null,null,25.04,24.24]
[null,"95","S","APOYO D4S1",null,"AD","+","0","0","M","PEN","NF",-1,-177,4,-8,-136,0,5,0,0,null,null,null,50,25.04,24.24]
[null,"96","S","APOYO D4S2",null,"AD","M","+","0","P","PEN","NF",49,-23,-122,14,102,11,0,0,0,null,null,25,25,30.48,29.68]
[null,"97","S","APOYO D4S1",null,"AE","P","0","0","0","PEN","NF",-2,24,6,-37,-28,0,8,0,0,50,null,25,25,25.04,24.24]
[null,"98","A","APOYO D4A3",null,"AB","M","M","0","0","PEN","NF",24,-55,-52,18,24,4,8,0,0,null,null,null,null,66.08,64.84]
[null,"99","S","APOYO D4S1",null,"AC","0","0","+","+","PEN","NF",68,76,33,-128,-86,8,0,0,12,null,25,25,null,25.04,24.24]
[null,"100","S","APOYO D4S1",null,"AA","0","M","M","0","PEN","NF",23,17,-44,-58,-6,0,16,2,0,null,null,null,25,25.04,24.24]
[null,"101","S","APOYO D4S2",null,"AD","M","M","0","P","PEN","NF",20,-72,-66,20,43,0,0,0,0,null,null,null,50,30.48,29.68]
[null,"102","A","APOYO D4A3",null,"AB","0","0","0","0","PEN","NF",13,7,7,3,26,0,0,0,13,null,null,null,null,66.08,64.84]
[null,"103","A","APOYO D4A4F",null,"AC","+","M","P","M","PEN","NF",74,-100,-8,124,-44,0,0,0,0,null,null,25,25,105.04,103.52]
[null,"104","S","APOYO D4S1",null,"AB","M","0","0","0","PEN","NF",17,-68,-18,35,-9,0,0,18,0,null,25,null,25,25.04,24.24]
[null,"105","S","APOYO D4S1",null,"AB","+","M","0","+","PEN","NF",126,-75,18,119,-34,0,0,0,6,25,25,null,null,25.04,24.24]
[null,"106","A","APOYO D4A4A",null,"A0","M","0","0","0","PEN","NF",15,-60,-9,23,-20,8,1,8,0,null,25,null,25,105.04,103.52]
[null,"107","S","APOYO D4S1",null,"AC","M","M","P","P","PEN","NF",17,-100,-116,92,94,0,0,0,0,25,50,null,null,25.04,24.24]
[null,"108","S","APOYO D4S1",null,"AC","L","+","P","0","PEN","NF",82,-196,-88,176,47,0,0,11,0,25,null,null,25,25.04,24.24]
[null,"109","A","APOYO D4A3",null,"A0","0","0","0","0","PEN","NF",-7,-4,-3,-17,-12,3,4,0,0,null,null,null,null,66.08,64.84]
[null,"110","S","APOYO D4S1",null,"AC","0","M","M","P","PEN","NF",14,14,-78,-63,44,0,0,6,0,null,null,null,50,25.04,24.24]
[null,"111","S","APOYO D4S1",null,"AA","0","P","M","M","PEN","NF",-5,-5,43,-50,-96,0,0,38,0,null,25,null,null,25.04,24.24]
[null,"112","S","APOYO D4S1",null,"AA","M","0","0","0","PEN","NF",3,-82,-7,-5,9,0,0,0,6,null,null,null,null,25.04,24.24]
[null,"113","A","APOYO D4A3",null,"AB","L","+","0","M","PEN","NF",156,-94,-13,146,19,0,0,0,0,null,null,null,50,66.08,64.84]
[null,"114","A","APOYO D4A4A",null,"AB","+","*","M","P","PEN","NF",118,-50,-240,34,175,0,0,0,0,null,25,null,25,105.04,103.52]
[null,"115","A","APOYO D4A2",null,"AB","-","-","*","L","PEN","NF",24,194,190,-289,-260,4,0,19,0,null,null,null,25,41.36,40.119999999999997]
[null,"116","A","APOYO D4A2",null,"AB","0","P","M","+","PEN","NF",14,10,68,-104,-145,0,0,0,7,null,25,25,null,41.36,40.119999999999997]
[null,"117","S","APOYO D4S2",null,"AA","0","0","M","M","PEN","NF",29,29,47,-88,-86,0,18,0,0,null,null,25,25,30.48,29.68]
[null,"118","A","APOYO D4A3",null,"AA","0","0","M","M","PEN","NF",42,33,21,-26,-41,0,4,14,0,null,25,null,null,66.08,64.84]
[null,"119","S","APOYO D4S1",null,"AA","M","0","0","0","PEN","NF",-6,-64,-16,-3,-40,26,0,3,0,null,null,null,25,25.04,24.24]
[null,"120","S","APOYO D4S1",null,"AD","P","M","+","0","PEN","NF",46,129,-90,-128,17,0,0,0,0,null,50,null,25,25.04,24.24]
[null,"120-1","A","APOYO D4A4A",null,"AD","P","M","+","0","PEN","NF",46,129,-90,-128,17,0,0,0,0,null,50,null,25,105.04,103.52]
[null,"121","S","APOYO D4S1",null,"AE","+","L","0","P","PEN","NF",108,-88,-141,101,138,0,0,0,0,25,null,null,50,25.04,24.24]
[null,"122","S","APOYO D4S2",null,"AE","P","+","*","M","PEN","NF",44,75,-122,-292,-64,0,0,0,0,50,null,null,25,30.48,29.68]
[null,"123","A","APOYO D4A3",null,"AD","0","M","+","M","PEN","NF",-5,-5,-94,-202,-95,0,0,0,0,null,null,25,null,66.08,64.84]
[null,"124","S","APOYO D4S2",null,"AE","L","*","0","P","PEN","NF",86,-166,-271,83,164,0,0,0,0,null,25,null,null,30.48,29.68]
[null,"125","S","APOYO D4S1",null,"AB","M","M","0","0","PEN","NF",-7,-125,-116,-6,-12,0,0,1,0,25,25,null,null,25.04,24.24]
[null,"126","S","APOYO D4S1",null,"A0","0","0","0","0","PEN","NF",7,14,-16,-28,11,7,2,0,4,null,25,25,null,25.04,24.24]
[null,"127","S","APOYO D4S1",null,"AC","0","+","+","0","PEN","NF",90,74,-33,-76,71,9,43,0,6,25,null,null,25,25.04,24.24]
[null,"128","A","APOYO D4A3",null,"AC","M","0","0","M","PEN","NF",-3,-82,-12,-3,-121,4,0,0,0,null,null,null,25,66.08,64.84]
[null,"129","S","APOYO D4A2",null,"AC","0","P","0","M","PEN","NF",-2,-37,37,-7,-81,0,6,0,4,25,50,null,null,41.36,40.119999999999997]
[null,"130","S","APOYO D4S2",null,"AE","M","M","0","0","PEN","NF",23,-46,-41,14,13,14,19,0,0,null,null,null,null,30.48,29.68]
[null,"131","S","APOYO D4S1",null,"AB","0","0","+","+","PEN","NF",0,0,12,-201,-175,0,12,0,0,null,null,25,null,25.04,24.24]
[null,"132","S","APOYO D4S1",null,"AB","0","M","*","L","PEN","NF",140,138,48,-186,-118,0,0,6,0,null,null,null,null,25.04,24.24]
[null,"133","A","APOYO D4A3",null,"AA","*","L","P","P","PEN","NF",67,-254,-212,140,144,12,0,0,0,null,25,null,null,66.08,64.84]
[null,"134","S","APOYO D4S1",null,"AA","0","-","L","*","PEN","NF",144,137,302,-138,-213,0,0,0,0,null,null,25,25,25.04,24.24]
[null,"135","S","APOYO D4S2",null,"AD","-","P","*","L","PEN","NF",60,216,83,-278,-214,0,0,0,0,null,50,null,25,30.48,29.68]
[null,"136","S","APOYO D4S1",null,"AD","L","0","0","M","PEN","NF",91,-136,81,58,12,22,0,0,4,null,null,25,null,25.04,24.24]
[null,"137","A","APOYO D4A3",null,"AB","P","+","*","L","PEN","NF",161,214,4,-176,-123,0,8,0,0,25,null,null,25,66.08,64.84]
[null,"138","S","APOYO D4S1",null,"AE","0","+","M","P","PEN","NF",44,13,-156,-32,92,0,0,6,0,25,25,null,25,25.04,24.24]
[null,"139","A","APOYO D4A4A",null,"AE","+","M","0","0","PEN","NF",41,-104,-32,35,41,22,10,0,0,null,null,null,null,105.04,103.52]
[null,"140","S","APOYO D4S2",null,"AA","P","0","+","0","PEN","NF",8,101,-2,-150,-26,10,0,8,0,null,null,null,25,30.48,29.68]
[null,"141","S","APOYO D4S1",null,"AA","0","0","0","0","PEN","NF",4,18,6,-31,-24,14,2,0,0,null,null,25,25,25.04,24.24]
[null,"142","S","APOYO D4S2",null,"AC","0","+","*","+","PEN","NF",150,140,-14,-166,-18,0,2,16,0,null,null,null,null,30.48,29.68]
[null,"143","A","APOYO D4A2",null,"AG","*","*","0","0","PEN","NF",140,-233,-220,90,150,9,0,0,10,50,25,50,null,41.36,40.119999999999997]
[null,"144","A","APOYO D4A2",null,"AG","+","*","*","M","PEN","NF",155,-94,-142,-180,101,0,35,0,29,75,null,null,null,41.36,40.119999999999997]
[null,"145","A","APOYO D4A3",null,"AE","M","0","0","M","PEN","NF",18,-62,18,8,-56,3,0,0,9,null,null,null,null,66.08,64.84]
[null,"146","S","APOYO D4S2",null,"AB","0","0","0","0","PEN","NF",10,-25,11,-17,-48,0,1,0,0,25,null,25,50,30.48,29.68]
[null,"147","S","APOYO D4S1",null,"AC","0","M","M","0","PEN","NF",41,32,-37,-74,19,0,5,0,3,null,null,25,25,25.04,24.24]
[null,"148","S","APOYO D4S1",null,"AB","0","0","0","0","PEN","NF",-7,2,14,-12,-42,9,21,0,0,null,null,null,25,25.04,24.24]
[null,"149","S","APOYO D4S1",null,"AE","0","0","0","0","PEN","NF",-1,-26,-36,1,13,0,0,2,14,25,25,null,null,25.04,24.24]
[null,"150","S","APOYO D4S1",null,"AB","0","0","M","M","PEN","NF",42,42,35,-75,-47,0,0,0,0,null,null,25,null,25.04,24.24]
[null,"151","A","APOYO D4A3",null,"AA","0","0","0","0","PEN","NF",-5,-15,-25,-54,-37,0,5,1,0,null,25,50,25,66.08,64.84]
[null,"152","S","APOYO D4S1",null,"AD","M","0","0","0","PEN","NF",21,-50,-14,19,-13,12,0,0,0,null,25,null,25,25.04,24.24]
[null,"153","S","APOYO D4S1",null,"AC","0","0","M","M","PEN","NF",23,40,27,-70,-60,17,4,0,0,null,null,null,null,25.04,24.24]
[null,"154","S","APOYO D4S1",null,"AC","0","0","M","M","PEN","NF",52,46,55,-66,-85,0,3,0,0,null,null,25,50,25.04,24.24]
[null,"155","S","APOYO D4S1",null,"AB","0","0","0","0","PEN","NF",-7,9,-11,-42,-23,16,0,0,9,null,null,25,25,25.04,24.24]
[null,"156","A","APOYO D4A3",null,"AE","0","M","M","0","PEN","NF",47,-11,-58,-24,38,0,3,12,0,50,25,null,null,66.08,64.84]
[null,"157","S","APOYO D4S2",null,"AE","*","*","0","-","PEN","NF",115,-218,-302,126,316,0,0,11,35,null,75,null,null,30.48,29.68]
[null,"158","S","APOYO D4S1",null,"AE","0","0","0","0","PEN","NF",-4,9,-7,-32,-14,13,0,0,0,null,null,25,null,25.04,24.24]
[null,"159","A","APOYO D4A2",null,"AD","L","P","0","L","PEN","NF",164,-84,193,158,-110,0,0,0,0,null,50,null,25,41.36,40.119999999999997]
[null,"160","A","APOYO D4A3",null,"A0","0","0","M","M","PEN","NF",29,33,19,-60,-56,4,0,0,0,null,null,null,null,66.08,64.84]
[null,"161","A","APOYO D4A4F",null,"A0","0","0","M","M","PEN","NF",26,23,22,-50,-50,0,0,6,7,null,null,null,null,105.04,103.52]
[null,"162"]
[null,"163"]
[null,"164",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,50]
[null,"165",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,25]
[null,"166",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,50,25]
[null,"167",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,75]
[null,"168",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25]
[null,"169",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,50,null,25]
[null,"170"]
[null,"171"]
[null,"172"]
[null,"173",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,50]
[null,"174",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,25]
[null,"175",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,50,25]
[null,"176",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,75]
[null,"177",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25]
[null,"178",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,50,null,25]
[null,"179"]
[null,"180"]
[null,"181"]
[null,"182"]
[null,"183"]
[null,"184"]
[null,"185"]
[null,"186"]
[null,"187"]
[null,"188"]
[null,"189"]
[null,"190"]
[null,"191"]
[null,"192"]
[null,"193"]
[null,"194"]
[null,"195"]
[null,"196"]
[null,"197"]
[null,"198"]
[null,"199"]
[null,"200"]
[null,"201"]
[null,"202"]
[null,"203"]
[null,"204"]
[null,"205"]
[null,"206"]
[null,"207"]
[null,"208"]
[null,"209"]
[null,"210"]
[null,"211"]
[null,"212"]
[null,"213"]
[null,"214"]
[null,"215"]
[null,"216"]
[null,"217"]
[null,"218"]
[null,"219"]
[null,"220"]
[null,"221"]
[null,"222"]
[null,"223"]
[null,"224"]
[null,"225"]
[null,"226"]
[null,"227"]
[null,"228"]
[null,"229"]
[null,"230"]
[null,"231"]
[null,"232"]
[null,"233"]
[null,"234"]
[null,"235"]
[null,"236"]
[null,"237"]
[null,"238"]
[null,"239"]
[null,"240"]
[null,"241"]
[null,"242"]
[null,"243"]
[null,"244"]
[null,"245"]
[null,"246"]
[null,"247"]
[null,"248"]
[null,"249"]
[null,"250"]
[null,"251"]
[null,"252"]
[null,"253"]
[null,"254"]
[null,"255"]
[null,"256"]
[null,"257"]
[null,"258"]
[null,"259"]
[null,"260"]
[null,"261"]
[null,"262"]
[null,"263"]
[null,"264"]
[null,"265"]
[null,"266"]
[null,"267"]
[null,"268"]
[null,"269"]
[null,"270"]
[null,"271"]
[null,"272"]
[null,"273"]
[null,"274"]
[null,"275"]

{"sheet":"Peanas","index":3,"n_rows":9,"n_cols":8,"rows_kept":9,"cut":false,"hidden":true,"merged":[[6,0,6,1],[3,0,3,1],[0,0,0,1]]}
["Descripción de variables P800",null,"f"," 800+400"," 800x(400+R250)"," 800x(400+R500)"," 800x(400+R750)"," 800x(400+R1000)"]
["Hormigón en peana","m3",800,0.2,0.37,0.56000000000000005,0.77,1.01]
["Armado","kg",800,0,0,25,37,52]
["Descripción de variables P1000",null,"f"," 1000+400"," 1000x(400+R250)"," 1000x(400+R500)"," 1000x(400+R750)"," 1000x(400+R1000)"]
["Hormigón en peana","m3",1000,0.31,0.56000000000000005,0.83,1.1399999999999999,1.47]
["Armado","kg",1000,0,30,59,106,145]
["Descripción de variables P1200",null,"f"," 1200+400"," 1200x(400+R250)"," 1200x(400+R500)"," 1200x(400+R750)"," 1200x(400+R1000)"]
["Hormigón en peana","m3",1200,0.44,0.79,1.1599999999999999,1.57,2.02]
["Armado","kg",1200,0,30,58,120,187]

{"sheet":"Atributos CAD","index":4,"n_rows":3,"n_cols":52,"rows_kept":3,"cut":false,"hidden":false,"merged":[]}
["APOYO","TIPO","AA","AB","AC","AD","AE","AF","AG","AH","AI","AJ","AK","AL","AM","AN","GA","GB","GC","GD","GE","GF","GG","GH","GI","GJ","BA","BB","BC","BD","BE","BF","BG","BH","MA","MB","MC","MD","1F","1L","1D","2F","2L","2D","3F","3L","3D","4F","4L","4D","Frontal","Lateral"]
["T-1","D4A4F-AA","51 Ø20 c/101",4487,481,631,"27 Ø8 c/164",5416,1660,200,58,"2 Ø10 a 60",5215,7,1644,16564,1800,3542,996,836,3472,200,4738,12.2,4.33,16.520000000000003,2385.9613022672825,2385.9613022672825,2385.9613022672825,2385.9613022672825,"D4A4 - 2L 200X200X16 A-PEN","B200",19,28,66.080000000000013,67.84,2784,105.7,4436,4436,6273.4513626870494,4436,4436,6273.4513626870494,4436,4436,6273.4513626870494,4436,4436,6273.4513626870494,111.53,111.53]
["T-2","D4A4A-AB","45 Ø20 c/101",4185,481,523,"23 Ø8 c/180",4787,1460,200,44,"2 Ø8 a 50",4577,4,1444,18180,1600,3307,929,779,3158,200,4436,9.08,3.42,12.49,2385.9613022672825,2385.9613022672825,2385.9613022672825,2385.9613022672825,"D4A4 - 2L 200X200X16 A-PEN","B200",16,28,49.96,51.719999999999992,2284,89,4994,4994,7062.5825304912369,4994,4994,7062.5825304912369,5087,5087,7194.1043917919342,5087,5087,7194.1043917919342,111.53,111.53]

{"sheet":"Limites","index":5,"n_rows":28,"n_cols":31,"rows_kept":28,"cut":false,"hidden":true,"merged":[[13,0,13,1]]}
["Diámetro Pilar min",1100,1200,1300,1400,1500,1600,1700,1800,1900,2000,2100,2200,2300,2400,2500,2600,2700,2800,2900,3000,3100,3200,3300,3400,3500,3600,3700,3800,3900,4000]
["Diámetro solera max",1800,2200,2767,3333,3900,{"$f":"F2+100","v":4000},{"$f":"G2+100","v":4100},4200,4300,4400,{"$f":"K2+105","v":4505},{"$f":"L2+105","v":4610},4715,4820,4925,5030,5135,5240,5345,5450,5555,5660,5765,5870,5975,6080,6185,6290,6395,6400]
["Altura máxima Pilar",3000,3200,3400,4200,4400,4450,4500,4500,4550,4600,4600,4600,4600,4600,4600,4600,4600,4600,4600,4600,4600,4600,4600,4600,4600,4600,4600,4600,4600,4600]
["Altura max cimentación",3600,3900,4250,4500,5000,5050,5010,5100,5350,5350,5350,5350,5350,5350,5350,5350,5350,5350,5350,5350,5350,5350,5350,5350,5350,5350,5350,5350,5350,5350]
["Profundidad recueva max",350,{"$f":"(C2-C1)*0.5","v":500},{"$f":"(D2-D1)*0.5","v":733.5},{"$f":"(E2-E1)*0.5","v":966.5},1300,1400,1500,1500,1500,1600,1600,1600,1600,1600,1600,1600,1600,1600,1600,1600,1600,1600,1600,1600,1600,1600,1600,1600,1600,1600]
[]
[]
[]
[]
[]
[]
[]
[]
["PARAMETROS MaxMin (VBA)"]
["Diámetro mínimo solera (mm)",1700]
["Diámetro máximo solera (mm)",6500]
["Diámetro mínimo pilar (mm)",1100]
["Diámetro máximo pilar (mm)",5000]
["Altura mínima pilar (mm)",1100]
["Altura máxima pilar (mm)",4500]
["Altura mínima uña (mm)",400]
["Altura máxima uña (mm)",1700]
["Altura máxima cimentación (mm)",5350]
["Altura mínima cimentación (mm)",1700]
["Excavación máxima uña (mm)",1600]
["Excavación mínima uña (mm)",300]
["Ángulo uña máximo (°)",55]
["Ángulo uña mínimo (°)",50]

{"sheet":"Perfiles","index":6,"n_rows":177,"n_cols":9,"rows_kept":177,"cut":false,"hidden":true,"merged":[[8,7,9,7],[8,8,9,8],[7,7,7,8],[0,0,3,0],[0,1,1,4],[0,5,1,5]]}
["Denominación","Dimensiones",null,null,null,"Sección"]
[]
[null,"h = b","t","r1","r2","A"]
[null," mm","mm","mm","mm","mm2"]
["40x40x3",40,3,6,3,234.86279999999999]
["40x40x4",40,4,6,3,307.86279999999999]
["40x40x5",40,5,6,3,378.86279999999999]
["40x40x6",40,6,6,3,447.86279999999999,null,"Armaduras"]
["45x45x3",45,3,7,3.5,266.2577,null,"Diámetro nominal\n (mm)","Masa\n (kg/m)"]
["45x45x3,5",45,3.5,7,3.5,308.0077]
["45x45x4",45,4,7,3.5,349.2577,null,6,0.222]
["45x45x4,5",45,4.5,7,3.5,390.0077,null,8,0.39500000000000002]
["45x45x5",45,5,7,3.5,430.2577,null,10,0.61699999999999999]
["45x45x6",45,6,7,3.5,509.2577,null,12,0.88800000000000001]
["45x45x7",45,7,7,3.5,586.2577,null,14,1.21]
["50x50x3",50,3,7,3.5,296.2577,null,16,1.58]
["50x50x4",50,4,7,3.5,389.2577,null,20,2.4700000000000002]
["50x50x5",50,5,7,3.5,480.2577,null,25,3.85]
["50x50x6",50,6,7,3.5,569.2577,null,32,6.31]
["50x50x7",50,7,7,3.5,656.2577,null,40,9.86]
["50x50x8",50,8,7,3.5,741.2577]
["50x50x9",50,9,7,3.5,824.2577]
["55x55x4",55,4,8,4,430.86720000000003]
["55x55x4,5",55,4.5,8,4,481.61720000000003]
["55x55x5",55,5,8,4,531.86720000000003]
["55x55x6",55,6,8,4,630.86720000000003]
["55x55x8",55,8,8,4,822.86720000000003]
["55x55x10",55,10,8,4,1006.8672]
["60x60x4",60,4,8,4,470.86720000000003]
["60x60x5",60,5,8,4,581.86720000000003]
["60x60x6",60,6,8,4,690.86720000000003]
["60x60x8",60,8,8,4,902.86720000000003]
["60x60x10",60,10,8,4,1106.8671999999999]
["63x63x5",63,5,9,4.5,613.69129999999996]
["63x63x6",63,6,9,4.5,728.69129999999996]
["63x63x6,5",63,6.5,9,4.5,785.44129999999996]
["65x65x4",65,4,9,4.5,512.69129999999996]
["65x65x5",65,5,9,4.5,633.69129999999996]
["65x65x5,5",65,5.5,9,4.5,693.44129999999996]
["65x65x6",65,6,9,4.5,752.69129999999996]
["65x65x7",65,7,9,4.5,869.69129999999996]
["65x65x8",65,8,9,4.5,984.69129999999996]
["65x65x9",65,9,9,4.5,1097.6913]
["65x65x11",65,11,9,4.5,1317.6913]
["70x70x5",70,5,9,4.5,683.69129999999996]
["70x70x6",70,6,9,4.5,812.69129999999996]
["70x70x7",70,7,9,4.5,939.69129999999996]
["70x70x8",70,8,9,4.5,1064.6913]
["70x70x9",70,9,9,4.5,1187.6913]
["70x70x10",70,10,9,4.5,1308.6913]
["70x70x11",70,11,9,4.5,1427.6913]
["75x75x4",75,4,10,5,594.73]
["75x75x5",75,5,10,5,735.73]
["75x75x6",75,6,10,5,874.73]
["75x75x7",75,7,10,5,1011.73]
["75x75x8",75,8,10,5,1146.73]
["75x75x10",75,10,10,5,1410.73]
["75x75x12",75,12,10,5,1666.73]
["80x80x5",80,5,10,5,785.73]
["80x80x6",80,6,10,5,934.73]
["80x80x7",80,7,10,5,1081.73]
["80x80x8",80,8,10,5,1226.73]
["80x80x10",80,10,10,5,1510.73]
["80x80x12",80,12,10,5,1786.73]
["80x80x14",80,14,10,5,2054.73]
["90x90x5",90,5,11,5.5,887.98329999999999]
["90x90x6",90,6,11,5.5,1056.9833000000001]
["90x90x7",90,7,11,5.5,1223.9833000000001]
["90x90x8",90,8,11,5.5,1388.9833000000001]
["90x90x9",90,9,11,5.5,1551.9833000000001]
["90x90x10",90,10,11,5.5,1712.9833000000001]
["90x90x11",90,11,11,5.5,1871.9833000000001]
["90x90x12",90,12,11,5.5,2028.9833000000001]
["90x90x13",90,13,11,5.5,2183.9832999999999]
["90x90x15",90,15,11,5.5,2487.9832999999999]
["90x90x16",90,16,11,5.5,2636.9832999999999]
["100x100x6",100,6,12,6,1179.4512]
["100x100x6,5",100,6.5,12,6,1273.2012]
["100x100x7",100,7,12,6,1366.4512]
["100x100x8",100,8,12,6,1551.4512]
["100x100x9",100,9,12,6,1734.4512]
["100x100x10",100,10,12,6,1915.4512]
["100x100x12",100,12,12,6,2271.4512]
["100x100x14",100,14,12,6,2619.4512]
["100x100x15",100,15,12,6,2790.4512]
["100x100x16",100,16,12,6,2959.4512]
["100x100x20",100,20,12,6,3615.4512]
["110x110x6",110,6,13,6.5,1302.1337000000001]
["110x110x7",110,7,13,6.5,1509.1337000000001]
["110x110x8",110,8,13,6.5,1714.1337000000001]
["110x110x9",110,9,13,6.5,1917.1337000000001]
["110x110x10",110,10,13,6.5,2118.1336999999999]
["110x110x12",110,12,13,6.5,2514.1336999999999]
["110x110x14",110,14,13,6.5,2902.1336999999999]
["120x120x7",120,7,13,6.5,1649.1337000000001]
["120x120x8",120,8,13,6.5,1874.1337000000001]
["120x120x9",120,9,13,6.5,2097.1336999999999]
["120x120x10",120,10,13,6.5,2318.1336999999999]
["120x120x11",120,11,13,6.5,2537.1336999999999]
["120x120x12",120,12,13,6.5,2754.1336999999999]
["120x120x13",120,13,13,6.5,2969.1336999999999]
["120x120x15",120,15,13,6.5,3393.1336999999999]
["120x120x18",120,18,13,6.5,4014.1336999999999]
["130x130x8",130,8,14,7,2037.0308]
["130x130x9",130,9,14,7,2280.0308]
["130x130x10",130,10,14,7,2521.0308]
["130x130x11",130,11,14,7,2760.0308]
["130x130x12",130,12,14,7,2997.0308]
["130x130x14",130,14,14,7,3465.0308]
["130x130x16",130,16,14,7,3925.0308]
["140x140x9",140,9,15,7.5,2463.1424999999999]
["140x140x10",140,10,15,7.5,2724.1424999999999]
["140x140x11",140,11,15,7.5,2983.1424999999999]
["140x140x12",140,12,15,7.5,3240.1424999999999]
["140x140x13",140,13,15,7.5,3495.1424999999999]
["140x140x15",140,15,15,7.5,3999.1424999999999]
["140x140x17",140,17,15,7.5,4495.1424999999999]
["150x150x10",150,10,16,8,2927.4688000000001]
["150x150x12",150,12,16,8,3483.4688000000001]
["150x150x13",150,13,16,8,3758.4688000000001]
["150x150x14",150,14,16,8,4031.4688000000001]
["150x150x15",150,15,16,8,4302.4687999999996]
["150x150x16",150,16,16,8,4571.4687999999996]
["150x150x18",150,18,16,8,5103.4687999999996]
["150x150x20",150,20,16,8,5627.4687999999996]
["160x160x14",160,14,17,8.5,4315.0096999999996]
["160x160x15",160,15,17,8.5,4606.0096999999996]
["160x160x16",160,16,17,8.5,4895.0096999999996]
["160x160x17",160,17,17,8.5,5182.0096999999996]
["160x160x19",160,19,17,8.5,5750.0096999999996]
["180x180x13",180,13,18,9,4545.7651999999998]
["180x180x14",180,14,18,9,4878.7651999999998]
["180x180x15",180,15,18,9,5209.7651999999998]
["180x180x16",180,16,18,9,5538.7651999999998]
["180x180x17",180,17,18,9,5865.7651999999998]
["180x180x18",180,18,18,9,6190.7651999999998]
["180x180x19",180,19,18,9,6513.7651999999998]
["180x180x20",180,20,18,9,6834.7651999999998]
["180x180x22",180,22,18,9,7470.7651999999998]
["200x200x13",200,13,18,9,5065.7651999999998]
["200x200x15",200,15,18,9,5809.7651999999998]
["200x200x16",200,16,18,9,6178.7651999999998]
["200x200x17",200,17,18,9,6545.7651999999998]
["200x200x18",200,18,18,9,6910.7651999999998]
["200x200x19",200,19,18,9,7273.7651999999998]
["200x200x20",200,20,18,9,7634.7651999999998]
["200x200x21",200,21,18,9,7993.7651999999998]
["200x200x22",200,22,18,9,8350.7651999999998]
["200x200x23",200,23,18,9,8705.7651999999998]
["200x200x24",200,24,18,9,9058.7651999999998]
["200x200x25",200,25,18,9,9409.7651999999998]
["200x200x26",200,26,18,9,9758.7651999999998]
["200x200x28",200,28,18,9,10450.7652]
["250x250x17",250,17,18,9,8245.7651999999998]
["250x250x18",250,18,18,9,8710.7651999999998]
["250x250x19",250,19,18,9,9173.7651999999998]
["250x250x20",250,20,18,9,9634.7651999999998]
["250x250x21",250,21,18,9,10093.7652]
["250x250x22",250,22,18,9,10550.7652]
["250x250x23",250,23,18,9,11005.7652]
["250x250x24",250,24,18,9,11458.7652]
["250x250x25",250,25,18,9,11909.7652]
["250x250x26",250,26,18,9,12358.7652]
["250x250x27",250,27,18,9,12805.7652]
["250x250x28",250,28,18,9,13250.7652]
["250x250x35",250,35,18,9,16309.7652]
["300x300x25",300,25,18,12,14382.7256]
["300x300x26",300,26,18,12,14931.7256]
["300x300x27",300,27,18,12,15478.7256]
["300x300x28",300,28,18,12,16023.7256]
["300x300x29",300,29,18,12,16566.725600000002]
["300x300x30",300,30,18,12,17107.725600000002]
["300x300x31",300,31,18,12,17646.725600000002]
["300x300x32",300,32,18,12,18183.725600000002]
["300x300x33",300,33,18,12,18718.725600000002]
["300x300x34",300,34,18,12,19251.725600000002]
["300x300x35",300,35,18,12,19782.725600000002]